List of Disk2FDI-compatible hardware
------------------------------------


Known 3.5" floppy disk drives with a real index signal (good):
- Citizen
        - OSDA-20E-U
- Hewlett Packard
        - D2035-60121
- Mitsumi
        - MF355F-3250MG
- Panasonic (Matsushita)
        - JU-257A606P
- Samsung
        - SFD-321B
- Sony
        - MPF520-1
        - MPF920-E
- Toshiba
        - ND-356T-A

Known 3.5" floppy disk drives with a fake index signal (bad):
- Alps Electric co., ltd.
- Mitsumi
        - D359M3
        - D359M3D
        - D359T6
- Nec
        - FD1231H

Known 5.25" floppy disk drives with a real index signal (good):
- Nec
        - FD1157C
- Panasonic (Matsushita)
        - JU-455-5 AFS
        - JU-455-5 CGN
- Teac
        - FD-55GFR
- Toshiba
        - FDD 6473A0K

Known 5.25" floppy disk drives with a fake index signal (bad):
- Mitsumi (Newtronics)
        - D509V3

Known double-density 5.25" floppy disk drives allowing "flippy side" reading
without modification:
- Panasonic (Matsushita)
        - JU-455-5 AFS
- Toshiba
        - FDD 6473A0K
        - FUJI LR56034
