# /etc/fdprm  -  floppy disk parameter table

########################################################################
# Standard linux disk formats. Names are of the form
#  actual media capacity/maximum drive capacity
# (Note: although 5.25" HD drives can format disks at 1.44M, they're listed
#        as 1200 because that's the common maximum size.)

#		size sec/t hds trk stre gap  rate spec1 fmt_gap

"360/360":
 DS DD sect=9

"1200/1200":
 DS HD sect=15

"360/720":
 SS DD sect=9

"720/720":
 DS DD sect=9

"360/1200":
 DS DD sect=9

"720/1200":
 DS QD sect=9

"1440/1440":
 DS HD sect=18

"2880/2880":
 DS ED sect=36

"2880/2880":
 DS ED sect=36

"2880/2880":
 DS ED sect=36

"1440/1200":
 DS HD sect=18

"1680/1440":
 DS HD sect=21

"410/1200":
 DS DD sect=10 cyl=41

"820/1440":
 DS DD sect=10 cyl=82

"1476/1200":
 DS HD sect=18 cyl=82

"1722/1440":
 DS HD sect=21 cyl=82

"420/1200":
 DS DD sect=10 cyl=42

"830/1440":
 DS DD sect=10 cyl=83

"1494/1200":
 DS HD sect=18 cyl=83

"1743/1440":
 DS HD sect=21 cyl=83

"1743/1440":
 DS HD sect=21 cyl=83

"880/1200":
 DS QD tracksize=11b ssize=1KB

"1040/720":
 DS QD sect=13

"1120/720":
 DS QD tracksize=7KB mss

"1600/1200":
 DS HD tracksize=10KB mss

"1760/1440":
 DS HD sect=11 ssize=1KB

"1920/1440":
 DS HD tracksize=12KB mss

"3200/2880":
 DS ED sect=5 ssize=4KB

"3520/2880":
 DS ED tracksize=22KB ssize=4KB

"3840/2880":
 DS ED sect=3 ssize=8KB

"3840/2880":
 DS ED sect=3 ssize=8KB

"1840/1440":
 DS HD tracksize=23b ssize=2KB

"800/720":
 DS DD sect=10

"1600/1440":
 DS HD sect=20

########################################################################
# CP/M formats
#
# the name is constructed as CODsize, where COD identifies the
# brand of the computer having formatted the disk

# Generic CP/M - SSSD 8"

"GEN250":
 SS DD sect=24 dtr=0 fm=1 cyl=77 ssize=128

# ABC-80 - SSDD 48 tpi 5.25"

"ABC160":
 SS DD sect=16 ssize=256

# Actrix (Access Matrix) - SSDD 48 tpi 5.25"

"ACT180":
 SS DD sect=9

# Adler Textriter - SSDD 48 tpi 5.25"

"ADL160":
 SS DD sect=16 ssize=256

# Advanced Digital Super 6 - SSDD 48 tpi 5.25"

"ADV160":
 SS DD sect=4 ssize=1KB

# Advanced Digital Super 6 - DSDD 96 tpi 5.25"

"ADV640":
 DS QD sect=4 ssize=1KB

# Altos Series 5 - DSDD 96 tpi 5.25"

"ALT720":
 DS QD sect=9

# Amigo - SSDD 48 tpi 5.25"

"AMI200":
 SS DD sect=10

# Ampro - SSDD 48 tpi 5.25"

"AMP200":
 SS DD sect=10

# Ampro - SSDD 96 tpi 5.25"

"AMP400":
 SS QD sect=5 ssize=1KB

# Amstrad PCW8256 - DSDD 96 tpi 5.25"

"AMS720":
 DS QD sect=9

# Archive I - SSDD 96 tpi 5.25"

"ARC400":
 SS QD sect=5 ssize=1KB

# Archive II & III - DSDD 96 tpi 5.25"

"ARC800":
 DS QD sect=5 ssize=1KB

# Arisia - SSDD 48 tpi 5.25"

"ARI180":
 SS DD sect=18 ssize=256

# ATR-8000 - SSDD 48 tpi 5.25"

"ATR200":
 SS DD sect=5 ssize=1KB

# Beehive - DSDD 48 tpi 5.25"

"BEE400":
 DS DD sect=10

# Bitelex - SSDD 48 tpi 5.25"

"BIT160":
 SS DD sect=16 ssize=256

# BMC IF800 Model 20 - DSDD 48 tpi 5.25"

"BMC400":
 DS DD sect=10

# Burr-Brown - DSDD 48 tpi 5.25"

"BUR360":
 DS DD sect=18 ssize=256

# Cal-PC - DSDD 48 tpi 5.25"

"CAL400":
 DS DD sect=5 ssize=1KB

# Cashcom 100 - DSDD 96 tpi 5.25"

"CAS640":
 DS QD sect=4 ssize=1KB

# CDI-5000 - DSDD 48 tpi 5.25"

"CDI400":
 DS DD sect=5 ssize=1KB

# CMC Supersystem 2 - DSDD 96 tpi 5.25"

"CMC800":
 DS QD sect=5 ssize=1KB

# Coleco ADAM, 40 track - SSDD 48 tpi 5.25"

"COL160":
 SS DD sect=8

# Compugraphic MCS-5 - SSDD 48 tpi 5.25"

"COM160":
 SS DD sect=16 ssize=256

# Compupro (Viasyn) (1024 bytes/sector) - DSDD 96 tpi 5.25"

"COM800":
 DS QD sect=5 ssize=1KB

# Cromemco CDOS - SSSD 48 tpi 5.25"

"CRO80":
 SS SD sect=16 dtr=1 fm=1 ssize=128

# Cromemco CDOS - SSDD 48 tpi 5.25"

"CRO200":
 SS DD sect=10

# Cromemco CP/M - SSDD 48 tpi 5.25"

"CRO200":
 SS DD sect=10

# C/WP Cortex - SSDD 48 tpi 5.25"

"CWP200":
 SS DD sect=10

# Cykey - DSDD 48 tpi 5.25"

"CYK320":
 DS DD sect=16 ssize=256

# DEC DECMate II - SSDD 96 tpi 5.25"

"DEC400":
 SS QD sect=10

# DEC Rainbow - SSDD 96 tpi 5.25"

"DEC180":
 SS DD sect=9

# DEC VT-180 - SSDD 48 tpi 5.25"

"DEC180":
 SS DD sect=9

# Direct 1025 - DSDD 48 tpi 5.25"

"DIR320":
 DS DD sect=16 ssize=256

# Discovery - DSDD 96 tpi 5.25"

"DIS640":
 DS QD sect=8

# Eagle II - SSDD 96 tpi 5.25"

"EAG400":
 SS QD sect=5 ssize=1KB

# Epson QX-10 - DSDD 48 tpi 5.25"

"EPS400":
 DS DD sect=10

# Epson QX-10 (256 bytes/sector) - DSDD 48 tpi 5.25"

"EPS320":
 DS DD sect=16 ssize=256

# Epson PX-8 - DSDD 3.5"

"EPS320":
 DS DD sect=8

# Ericsson DTC - SSDD 96 tpi 5.25"

"ERI320":
 SS QD sect=16 ssize=256

# Ericsson Step One - DSDD 96 tpi 5.25"

"ERI720":
 DS QD sect=9

# Florida Graphics - DSDD 96 tpi 5.25"

"FLO640":
 DS QD sect=16 ssize=256

# Formula 1 - DSDD 48 tpi 5.25"

"FOR360":
 DS DD sect=18 ssize=256

# Fujitsu Micro 16 - DSDD 48 tpi 5.25"

"FUJ320":
 DS DD sect=16 ssize=256

# Fujitsu Micro 8 - DSDD 48 tpi 5.25"

"FUJ320":
 DS DD sect=16 ssize=256

# HCL System 2 - DSDD 96 tpi 5.25"

"HCL800":
 DS QD sect=5 ssize=1KB

# Heath H89, Magnolia CP/M - SSDD 48 tpi 5.25"

"HEA180":
 SS DD sect=9

# Heurikon MLZ-91A - DSDD 96 tpi 5.25"

"HEU640":
 DS QD sect=16 ssize=256

# IBM PC, CP/M-86 - SSDD 48 tpi 5.25"

"IBM160":
 SS DD sect=8

# IMS 5000 - SSDD 48 tpi 5.25"

"IMS160":
 SS DD sect=16 ssize=256

# IMS 5000 TurboDOS - DSDD 96 tpi 5.25"

"IMS800":
 DS QD sect=5 ssize=1KB

# Intel iPDS 100 - DSDD 96 tpi 5.25"

"INT640":
 DS QD sect=16 ssize=256

# Insight Enterprises - DSDD 48 tpi 5.25"

"INS320":
 DS DD sect=16 ssize=256

# Ithaca Intersystems - SSDD 96 tpi 5.25"

"ITH360":
 SS QD sect=18 ssize=256

# Jet-80 - DSDD 48 tpi 5.25"

"JET400":
 DS DD sect=5 ssize=1KB

# Lexoriter - SSDD 48 tpi 5.25"

"LEX160":
 SS DD sect=16 ssize=256

# LNW 2 - SSDD 48 tpi 5.25"

"LNW180":
 SS DD sect=18 ssize=256

# Macsym 150 - SSDD 96 tpi 5.25"

"MAC320":
 SS QD sect=8

# Magic - DSDD 48 tpi 5.25"

"MAG400":
 DS DD sect=10

# MAI Basic Four - DSDD 96 tpi 5.25"

"MAI640":
 DS QD sect=16 ssize=256

# Micron Quark - DSDD 48 tpi 5.25"

"MIC320":
 DS DD sect=4 ssize=1KB

# Monroe 8800 Series - SSDD 96 tpi 5.25"

"MON320":
 SS QD sect=16 ssize=256

# Morrow MD2 - SSDD 48 tpi 5.25"

"MOR200":
 SS DD sect=5 ssize=1KB

# Morrow MD3, 5, 11, 16, 34 - DSDD 48 tpi 5.25"

"MOR400":
 DS DD sect=5 ssize=1KB

# Morrow TurboDOS - DSDD 48 tpi 5.25"

"MOR320":
 DS DD sect=4 ssize=1KB

# NCR FirstStep - DSDD 96 tpi 5.25"

"NCR640":
 DS QD sect=16 ssize=256

# NEC PC-8001A - SSDD 48 tpi 5.25"

"NEC160":
 SS DD sect=16 ssize=256

# NEC PC 8801A/8831A - DSDD 48 tpi 5.25"

"NEC320":
 DS DD sect=8

# NEC PC 8500/8431A, Starlet - DSDD 3.5"

"NEC320":
 SS QD sect=16 ssize=256

# Nixdorf 8810/30 - DSDD 96 tpi 5.25"

"NIX800":
 DS QD sect=10

# OKI IF800 Model 20 - DSDD 48 tpi 5.25"

"OKI400":
 DS DD sect=10

# Olivetti ETV300 - SSDD 48 tpi 5.25"

"OLI180":
 SS DD sect=18 ssize=256

# Olivetti M20 - DSDD 48 tpi 5.25"

"OLI320":
 DS DD sect=16 ssize=256

# Olivetti 250 -  SSDD 3.5"

"OLI320":
 SS QD sect=16 ssize=256

# Olympia EX-100 - DSDD 48 tpi 5.25"

"OLY360":
 DS DD sect=9

# Olympia ETX II - SSDD 48 tpi 5.25"

"OLY180":
 SS DD sect=9

# Osborne 1 - SSSD 48 tpi 5.25"

"OSB100":
 SS SD sect=10 dtr=1 fm=1 ssize=256

# Osborne 1 - SSDD 48 tpi 5.25"

"OSB200":
 SS DD sect=5 ssize=1KB

# Osborne Executive - SSDD 48 tpi 5.25"

"OSB200":
 SS DD sect=5 ssize=1KB

# Osborne 1 + Osmosis - DSDD 96 tpi 5.25"

"OSB400":
 DS DD sect=10

# Osborne Vixen - DSDD 48 tpi 5.25"

"OSB400":
 DS DD sect=5 ssize=1KB

# Osborne Executive w/Z3 - DSDD 96 tpi 5.25"

"OSB800":
 DS QD sect=5 ssize=1KB

# OSM Zeus 4 - DSDD 96 tpi 5.25"

"OSM640":
 DS QD sect=8

# Panasonic KX-E828 - DSDD 48 tpi 5.25"

"PAN320":
 DS DD sect=16 ssize=256

# Pegasus Data Logger - DSDD 48 tpi 5.25"

"PEG360":
 DS DD sect=9

# Philips PC-2010 - SSDD 48 tpi 5.25"

"PHI160":
 SS DD sect=16 ssize=256

# Philips PC-3000 - 3004 - SSDD 96 tpi 5.25"

"PHI320":
 SS QD sect=16 ssize=256

# Pied Piper - DSDD 96 tpi 5.25"

"PIE800":
 DS QD sect=10

# PMC Micromate - DSDD 48 tpi 5.25"

"PMC400":
 DS DD sect=5 ssize=1KB

# Proglas 770KB - DSDD 96 tpi 5.25"

"PRO800":
 DS QD sect=10

# Royal Alphatronic - DSDD 48 tpi 5.25"

"ROY320":
 DS DD sect=16 ssize=256

# Sage IV - DSDD 96 tpi 5.25"

"SAG640":
 DS QD sect=8

# Sanyo MBC-1000, MBC-1150 - DSDD 48 tpi 5.25"

"SAN320":
 DS DD sect=16 ssize=256

# Sanyo  MBC-1250 - DSDD 96 tpi 5.25"

"SAN640":
 DS QD sect=16 ssize=256

# Seequa Chameleon - SSDD 48 tpi 5.25"

"SEE160":
 SS DD sect=8

# Seiko - DSDD 96 tpi 5.25"

"SEI640":
 DS QD sect=16 ssize=256

# Siemens  PG-685 - DSDD 96 tpi 5.25"

"SIE720":
 DS QD sect=9

# Siemens PG-675 DSDD 48 tpi 5.25"

"SIE360":
 DS DD sect=9

# Siemens PG-635 DSDD 3.5"

"SIE720":
 DS QD sect=9

# Sorbus TurboDOS - 5.25" DSHD (or 8" DSDD)

"SOR1232":
 DS HD sect=8 cyl=77 ssize=1KB

# Sperry UTS 30, UTS 5000 - DSDD 96 tpi 5.25"

"SPE720":
 DS QD sect=9

# Superbrain JR - SSDD 48 tpi 5.25"

"SUP175":
 SS DD sect=10 cyl=35

# Superbrain 40 track - SSDD 48 tpi 5.25"

"SUP200":
 SS DD sect=10

# Systel 2 - SSDD 48 tpi 5.25"

"SYS180":
 SS DD sect=9

# Systel 3 - DSDD 48 tpi 5.25"

"SYS360":
 DS DD sect=9

# Televideo 801, 806 - DSDD 48 tpi 5.25"

"TEL360":
 DS DD sect=18 ssize=256

# Televideo 1603 - DSDD 96 tpi 5.25"

"TEL720":
 DS QD sect=9

# TI Professional, CP/M-86 - SSDD 48 tpi 5.25"

"TI1160":
 SS DD sect=8

# Toshiba T100, T200 - DSDD 48 tpi 5.25"

"TOS320":
 DS DD sect=16 ssize=256

# TRS-80 Model 1, Omikron CP/M - SSSD 48 tpi 5.25"

"TRS0":
 SS SD sect=16 dtr=1 fm=1 cyl=0 ssize=128

# TRS-80 Model 1, Color Power II - SSDD 48 tpi 5.25"

"TRS180":
 SS DD sect=18 ssize=256

# TRS-80, MM CP/M - SSDD 48 tpi 5.25"

"TRS200":
 SS DD sect=10

# TRS-80 Model 4, MT CP/M - SSDD 48 tpi 5.25"

"TRS180":
 SS DD sect=18 ssize=256

# TRS-80 Model 4, MT CP/M - DSDD 48 tpi 5.25"

"TRS360":
 DS DD sect=18 ssize=256

# TRS-80 Model 4 - SSDD 48 tpi 5.25"

"TRS160":
 SS DD sect=8

# Visual 1050 - SSDD 96 tpi 5.25"

"VIS400":
 SS QD sect=10

# Wangwriter - DSDD 48 tpi 5.25"

"WAN320":
 DS DD sect=16 ssize=256

# Wave Mate Bullet - SSDD 48 tpi 5.25"

"WAV200":
 SS DD sect=5 ssize=1KB

# Xerox 820 - SSSD 48 tpi 5.25"

"XER80":
 SS SD sect=16 dtr=1 fm=1 ssize=128

# Xerox 820 II - SSDD 48 tpi 5.25"

"XER160":
 SS DD sect=16 ssize=256

# Zenith Z-37 Disk - SSSD 48 tpi 5.25"

"ZEN100":
 SS SD sect=10 dtr=1 fm=1 ssize=256

# Zenith Z-37 Disk - DSDD 96 tpi 5.25"

"ZEN640":
 DS QD sect=16 ssize=256

# Zenith Z89, Heath H89 - DSDD 48 tpi 5.25"

"ZEN320":
 DS DD sect=16 ssize=256

# Zenith Z89, Heath H89 - DSDD 96 tpi 5.25"

"ZEN640":
 DS QD sect=16 ssize=256

# Zenith Z90 - SSDD 48 tpi 5.25"

"ZEN160":
 SS DD sect=16 ssize=256

# Zenith Z90 - DSDD 48 tpi 5.25"

"ZEN320":
 DS DD sect=16 ssize=256

# Zenith Z-100 - SSDD 48 tpi 5.25"

"ZEN160":
 SS DD sect=8

# Zenith Z-100 - DSDD 48 tpi 5.25"

"ZEN320":
 DS DD sect=8



########################################################################
#  Other interesting formats, please contribute ;-)
#

# Commodore 1581  (the 3 1/2 drive of the Commodore 128)
"CBM1581":
 DS DD sect=10 cyl=80 ssize=512 fmt_gap=35 gap=12 swapsides

# CMD FD2000 disk drive, a third party floppy disk drive for the
# Commodore line of computers with double of the capacity:
"CMDFD2M":
  DS HD sect=10 cyl=81 ssize=1024 fmt_gap=100 gap=12 swapsides

# Color computer, sides 1 and 2
"COCO1":
 SS DD sect=18 cyl=35 ssize=256

"COCO2":
 SS DD sect=18 cyl=35 ssize=256

# TRS-8- Color Computer os9 formats (to be confirmed). Needs
# zero-based floppy patch
"COCO360":
 DS DD sect=18 cyl=40 ssize=256 tpi=48 zero-based

"COCO720":
 DS DD sect=18 cyl=80 ssize=256 tpi=96 zero-based


# TO7 (Thomson), sides 1 and 2
"TO7-1":
 SS DD sect=16 ssize=256

"TO7-2":
 SS DD sect=16 ssize=256 swapsides
