You must login to the server as administrator to setup the system.

The administrator password is webtube.

Install the server first and add your client IP's

Then install each client and put the server IP address in, this will allow you to control the clients from the server.

Win98 Servers 
*************

Please note that although webtube server does run on windows 98, we recommend NT4 server or Windows2000 for the server. The client is fine on all windows versions. 

Please also make sure your computers have the latest patches from Microsoft. These can be checked at http://windowsupdate.microsoft.com and clicking product updates 

Network settings

We recommend using internal IP addresses e.g. 10.10.10.** e.g. Set the Server IP to 10.10.10.1 and set the clients to 10.10.10.2, 10.10.10.3, 10.10.10.4 etc. 

Webtube does not support Dynamic addresses or DCHP unless you allocate a static IP to each machine. 

For more suggestions on how to set up your hardware go to http://www.webtube.co.uk/Support/Client-setup-default.htm
 

