The program of recognition  of a raster images (vectorizer) 
RasterVect
Version 6.9 Trial

Description.

Vectorizer RasterVect allows for the transformation of any raster drawings into a vector format.  There is TWAIN support for importing from scanners. Images can be acquired from any scanner. The target vector formats (DXF, WMF, EMF, EPS and AI) are supported by most CAD applications that use vector graphics, such as AutoCAD and Corel Draw. There are viewing tools like zooming, scrolling and color selection. 


Features: 

- Recognizes orthogonal lines, inclined lines, arcs and circles;
- Has four various conversion methods (outline, centerline etc);
- Has modes ORTHO and SNAP;
- Forms correct corners at crossing lines, arcs and circles;
- Keeps scale of the initial drawing;
- Has TWAIN support (scanning is in the program);
- Can correct a turn angle of an initial raster drawing; 
- Can transform a grey and colored images to black-and-white for the subsequent recognition;
- Supports various raster and vector formats;
- Has despeckle filter;
- Has batch mode possibility;
- Has raster and vector editing possibility;
- Easy in use.

Shareware.
Copyright (C) 1997-2003 RasterVect Software.
All rights reserved.
