________________________________________________________________

             IMPORTANT!

 Please, uninstall all previous versions of
 Elecard MPEG2 Player before to install the new one.

________________________________________________________________
     ELECARD MPEG 2 Player v 2.0
 Copyright (C) Moonlight Cordless ltd. 2002
   Technology Licensed from Elecard Inc.
    Copyright (C) 1996-2000 Elecard Inc.
           All Rights Reserved. 


 ELECARD MPEG 2 Player is a real time, software-only
 MPEG Player, providing high resolution, full quality decoding
 of MPEG-1, MPEG-2 and DivX, optimized for the most efficient CPU usage.
 The build-in codecs enables to play a number of multimedia formats such as:
 AVI, WAV, MP3, MOV, etc.

 Installation:
 o Unzip delivery pack and follow by Wizard.
 o During installation the program copies and registers DirectShow(R) filters 
   (Elecard MPEG2 Demultiplexer, Elecard MPEG2 Video Decoder, etc) 
 o For additional information about including DirectShow(R) filters please 
   read DecoderPackage.txt
 o After you click "Finish" the program is ready to run and doesn't require 
   rebooting your computer
 o The program runs after clicking "Start"->"Programs"->"Elecard Program Group"
   ->"MPEG2 Player."

 Uninstallation:

 o Click "Start"->"Programs"->"Elecard MPEG-2 Player"->"Setup"->"Next"->
   "Uninstall or remove the installed application"
 o During uninstallation all the above-mentioned filters and programs are 
   uninstalled

 SUPPORTED FORMATS:

 o MPEG-1 Systems
 o MPEG-1 Video only
 o MPEG-1 audio(Layer I,II,III)
 o MPEG-1 (VideoCD)
 o MPEG-2 Program Stream
 o MPEG-2 Program Stream with AC3(VOB)
 o MPEG-2 Video only
 o MPEG-2 Transport Stream
 o MPEG-2 HDTV(including ATSC)
 o PIM-2 (AVI including MPEG-2)
 o SvideoCD
 o MSMPEG 4 v1,v2,v3 (DivX 3.x); DivX 4.x; XviD; mp43; AP41; 
 o asf files
 o WMV files

 FEATURES:

 o High definition video playback/decoding
 o Real time high resolution video playback at 720x480 @ 30fps for NTSC
   or 720x576 @ 25fps for PAL playback on Pentium II 450 MHz with DirectX 
   compatible video card supporting YUV overlay
 o Displays correct aspect ratio
 o Full screen mode
 o Video frame capturing (pixel by pixel, aspect ratio or user defined)
 o DirectShow and ActiveMovie compliance
 o MPEG2 (ISO/IEC 13818) Transport, Program and Video Stream; 
   MPEG1 (ISO/IEC 11172) Systems and Video streams playback
 o Supports all 18 ATSC formats 
 o Play list function
 o Search forward and Search backward with a possibility looking through a 
   movie by step
 o Quarter resolution playback
 o Graph preview and possibilities to set filter properties
 o File list source function 
 o GOP-accurate MPEG2 Trimming 

 New in v 2.0:

 o Play list function
 o File list source function
 o Possibility to playback DivX files
 o Graph preview and possibilities to set filter properties
 o Brightness control interface(not available yet)
 o Postprocessing - deblocking
 o Double precision IDCT
 o Decoding quarter resolution for preview mode 

 SYSTEM REQUIREMENTS:

 o MMX-enhanced CPU (Intel Pentium MMX, Pentium II,
   Celeron, Pentium III, AMD K6-2, K6-3, Athlon, etc.)
 o Windows 95/98/Me/NT/2000/XP (WindowsR NT 4.0 and WindowsR 95 
   with DirectShow installed)
 o 32 MB RAM
 o Any VGA card
 o 1.5 MB of free disk space for filter file


 FEEDBACK:

 Visit ELECARD on WWW at http://moonlight.co.il
 or http://www.elecard.com
 On technical issues contact ELECARD technical support
 by e-mail at techsupp@elecard.com.
 For general information: info@elecard.com.
 For licensing information contact sales@moonlight.co.il
