Huazhong University of Science and Technology
Visual Sound Instrument (Version 3.2)
Toolbar
1.Open signal from a windows WAV sound file.
..
2.Save signal to a windows WAV sound file, or a text data file.
.
3.Control a 16bit sound card to record a signal. Use Recording Par. Item in the menu to set recording parameter.
.
4.Control a inner signal generator to produce digital signal. Use Generate Par. Item in the menu to set recording parameter.
..
5.Playing signal from sound card.Use Playing Par. Item in the menu to set recording parameter.
...
6.Stop on going Recording/Generator/Playing/Net_Data thread.
...
7.Refresh the display of VIS32.
.
8.Zoom out curve in Y direction
.
9.Zoom in curve in Y direction.
.
a.Zoom out in X direction.
.
b.Zoom in in X direction.
.
c.Move signal to left.
.
d.Move signal to right.
.
e.Reset the dispaly parameter of VSI32 to default.
.
f.Copy the analyze result to clipboard(Bitmap), then start a graph editor to view it.
.
g.Copy the analyze result to clipboard(Text), then start a text editor to view it.
.
h.Open the help document by IE.
.
i.My website.
.
j.About.
..
[Return]
.

2004.1.10