  SVGA 1024 NI Drivers (supports Windows 3.1) for 4825SX/4850EP - 1 of 2

*** Requires High Density Disk ***

These drivers enable the user to run several software applications
under the VGA 1024 video controller's Super VGA screen modes. (The
list of screen modes and the software applications are listed in the
README.DOC file on this drivers disk.) These drivers are for the
TANDY 4825 SX and 4850 EP Computers.


NOTE:

   * This drivers disk is DISK ONE of a two disk set. After drivers
     from this disk are installed, please make sure that drivers
     from DISK TWO are also installed.


This disk contains the following files--

   ACAD.LIF       CADVANCE.LIF   DISK.ID       GENERIC.LIF
   INSTALL.BAT    INSTALL.DAT    LOOK.COM      OS2.LIF
   PCAD.LIF       README.TXT     READID.EXE    VCAD.LIF
   _INSTALL.EXE   SETUP482.COM   KP.EXE        PASSWORD.COM
   CACHE482.COM   README.DOC


In order to obtain a printout of this README.TXT file, insert this
disk in Drive A, make sure your printer is switched on, is on line,
and at the C:\> prompt, type the following command--

   PRINT A:README.TXT

and press <Enter>.


The installation instructions for these drivers are included in the
README.DOC file on this diskette. In order to print the README.DOC
file, insert this drivers disk in Drive A. At the C:\> prompt,
type in the following--

   PRINT A:README.DOC

and press <Enter>. The README.DOC file is 43 pages long.


NOTE:
   * The installation instructions for drivers for Windows 3.1 are
     on Page 31 of the README.DOC file.


NOTE:
"While reasonable efforts have been taken in the preparation of this
information to assure its accuracy, Tandy Corporation/Radio Shack
assumes no liability resulting from the use of the information
contained herein."
