TEXTNO_001_

Plese set TAB to 4.

_SUBDIR,_
_DEBUG,1_
*** color
PC9801
 bit 0: secret(always 1)
 bit 1: blink
 bit 2: reverse
 bit 3: nouse(always 0)
 bit 4: nouse(always 0)
 bit 5: blue
 bit 6: red
 bit 7: green
IBMPC
 bit 0-3: forward
 bit 4-6: back
 bit   7: blink
  0:black
  1:blue
  2:green
  3:cyan
  4:red
  5:magenta
  6:brown
  7:lightgray
  8:darkgray
  9:lightblue
 10:lightgreen
 11:lightcyan
 12:lightred
 13:lightmagenta
 14:yellow
 15:white

_CHARCC,225,015_ character color(white)
_MENUFC,129,002_ menu window(green)
_MENUCC,193,003_ menu character(yellow,cyan)
_MENUSC,101,095_ menu select(reverse magenta)
_GUIDEC,229,048_ guide line character(reverse white,reverse cyan)
_BIGFRC,161,003_ big window frame(cyan)
_BIGTIC,193,003_ big title character(yellow,cyan)
_ERRFRC,065,004_ error window frame(red)
_ERRCHC,225,015_ error window character(white)

*** RS232C parameter
_RS232C,1,3,8,0,1		1st:chanel(1,2) PCAT only
						2nd:speed(0=300,1=1200,2=2400,3=4800,4=9600)
						3rd:character length(7,8)
						4th:parity(0=no,1=odd,2=even)
						5th:stop bit(1,2)
_RSRETR,05			RS232C retry counter
_TYTIME,03,03,06,10,25_	ty time 9600/4800/2400/1200/300
_MODEMI,T,120,2_			DP=P,PB=T/CD check timer(@10ms)3digit/CI time 1digit ###
_MODEMC,H0E1M1Q0V1S0=0X1_	modem init command max 40 char
_MODEAD,D_					modem ATDxxxx command max 39 char +++
_MODEOR,D_					modem ATD originate command max 39 char +++
_MODEAN,A_					modem ATA answer command max 39 char +++
_MODEDI,H0_					modem disconnect command max 39 char +++
_MODECM,+++_				modem data mode -> command mode max 3 char +++

_PASWRD,QDNITSUKODXE_ ### for QD command

*** printer
_PRIPWD,80_			curent printer wide

*** yy-mm-dd
_YMDFLG,1_			0:yy-mm-dd 1:mm-dd-yy

*** error display string
_OUTMEM,Not enough memory_
_FISIZE,File size error :_
_TXFOMA,Text format error :_
_TXDNFO,Text data not found :_
_DSFULL,Disk full :_

_ERROWI,43,5,3,33,3
00,16Error_
01_
02_
03,Press ESC to exit._

_YESNWI,50,5,0,33,3
00,01_
01Yes_
02/_
03No_
GUIDEL, ESC:No_

_{l},Line No. : 01-_
_{t},TEN No. : 01-_
_{i},ID No. : 01-_
_EDITCF,Cf._

*** initirize file
_INITFI,2470T0_

_ENDINT

***Main menu
_MAINWI,18,9,7,2,3
00,04Main menu_
01File_1_
02Edit_2_
03Communication_3_
04Print_4_
05Option_5_
06Os shell_6_
07Quit_7_
GUIDEL, ESC:Display customer _

***File menu
_FILEWI,20,7,5,0,0
00,05File menu_
01Customer_1_
02Display_2_
03Load_3_
04Save_4_
05Delete_5_
GUIDEL, ESC:To Main menu _

_FILETE,System type error_
_FILEME,mode error_
_FILEIN,Invalid file name_

***Customer
_CUSTWI,80,22,20,1,2
00,34Customer_
01Name	10,[	60,]_
02Contact	7,[	22,]_
03Phone No.	5,[	22,]_
04Address	7,[	60,]_
05_
06System type	3,[	34,]_
07Rom version	3,[	8,]_
08No. of Sta.	3,[	5,]   No. of Lines  [	5,]_
09_
10Installor	5,[	60,]_
11Contact	7,[	22,]_
12Phone No.	5,[	22,]_
13ID code	7,[	12,]_
14MODEM Phone   [	42,]_
15MODEM Speed   [	9,]_
16_
17Instal.Date	3,[	22,]   Note:_
18Issue-1	7,[	22,]_
19Issue-2	7,[	22,]_
20Issue-3	7,[	22,]_
GUIDEL, ESC:To File menu 	1, DEL:Character delete_

_SYTYPE,31,5,3,0,0
00,02System type_
01DX-E 1240 (DXE12-MCU-C)_E_ ### if DXV V
02DX-E 2470 (DXE24-MCU-C)_E$_ ### if DXV V$
03DX-E 36100(DXE36-MCU-C)_E6_ ### if DXV V6
GUIDEL, ESC:To previous item _

_SYMODE,22,4,2,0,0
00,03Mode menu_
01Mode 1(vA.00-A.99)_01_4100,4199_
02Mode 2(vB.00-B.99)_02_4200,4299_
GUIDEL, ESC:To previous item _

_MODEMS,12,6,4,0,0
00,03Speed_
014800bps_3_
022400bps_2_
031200bps_1_
04 300bps_0_

***Display
_DISPWI,80,22,1,1,2
00,34Display_
01Directory <	37,>_
_
GUIDEL, ESC:To File menu 	1, F.1:directory _

***Read
_READWI,80,22,01,1,2
00,34Load_
01Directory <	37,>_
_
GUIDEL, ESC:To File menu 	1, F.1:directory 	1, CR:Load_

_READYN,Realy over write without loading ?_

***Save
_SAVEWI,52,4,2,0,0
00,23Save_
01Directory <	37,>_
02File name <	10,>_
_
GUIDEL, ESC:To previous menu 	1, CR:Save _

_SAVEYN,Over write ?_

***Delete
_DELEWI,80,22,1,1,2
00,34Delete_
01Directory <	37,>_
_
GUIDEL, ESC:To File menu 	1, F.1:directory 	1, CR:Delete _

_DELEFN,File delete : _
_DELEYN,Aer you sure ?_

***Communication
_COMMWI,32,4,2,2,3
00,08Communication_
01PC to Main Equip.(ME)_1_
02ME to Personal computer(PC)_2_
GUIDEL, ESC:To Main menu 	1 f.6:Speed 	1 f.9:MODEM_

_COMPWI,27,9,7,2,7
00,04Pattern select_
01System data_0_
02Service No._1_
03Speed dial_2_
04One touch dial(flexible)_3_
05One touch dial(line)_4_
06One touch dial(inter)_5_
07Name_6_
GUIDEL, ESC:To Main menu 	1, CR:Start 	1 f.6:Speed 	1 f.9:MODEM _

_COMCWI,23,12,10,0,0
00,04Class menu_
01, 1 System(basic)_01_
02, 2 TEN data(basic)_02_
03, 3 Line associated_03_
04, 4 Group assigments_04_
05, 5 Loop selection_05_
06, 6 SMDR parameters_06_
07, 7 System options_07_
08, 8 Terminal options_08_
09, 9 Line options_09_
10,10 Doorphone/Paging_10_
GUIDEL, ESC:To previous menu 	1, CR:To item menu 	1, End:Help _

_COMIWI,50,15,0,30,5 *** with print menu
00,18Item menu_
GUIDEL, ESC:To Edit menu 	1, CR:*/' ' 	1, End:Help _

_COMIHL,27,6,4,0,0 *** with print help
00,11Help_
01,f.1 : Select all item__
02,f.2 : Reset all item__
03,f.3 : Reset all class__
04,f.5 : Start__

_COMTWI,45,4,2,35,3
01,ME system type : _
02,ME version     : _
GUIDEL, ESC:stop _

_COMUWI,25,15,1,27,8
00,08Status_
01,ME Type check_		**QD send
02,ME busy_			**ND received
03,Data check_			**J send
04,Skip_				**KE/IE received
05,Complete_			**K received
06,Communication Error_
07,End procedure_		**ED send
08,Initialize error_	**RS232C init error
09,Connect_				**AD received
10,Disconnect_			**ED send complete
11,ED command error_	**ED send error
12,Abort_				**ESC key press
13,Out of memory_		**Receved data size over
14,Command error_		**Receive command size error
15,Password error_    **Password unmatch
16,Protect errorr_    **Protect error
17,ID check_			**ID check
18,ID send_				**ID send
GUIDEL, ESC:Stop _

_COMRWI,25,15,0,55,7
00,08Protocol_

_COMJWI,25,7,5,0,0
00,05ME check error_
01,Error class  : _
02,      item   :_
03,      element:_
04,      object :_
05,      code   :_
GUIDEL, ESC:Exit 	1, CR:To Edit 	1, f.5:Send again 	1 f.9:Edit(selsect)_

_COMEWI,21,4,2,40,10
00,06Edit select_
01,Service No. : _
02,   Item No. : _

_COMDWI,20,10,3,0,0 ###
00,10ID_
01,ID unmatch_
02,ME(            )_
03,PC(            )_

_COMDIW,15,6,4,0,0 ###
01,Continue_1_
02,PC -> ME_2_
03,ME -> PC_3_
04,End_4_

_COMHLP,30,14,12,0,0
00,13Edit help_
01,CR  : To previous menu._
_
02,ESC : To previous menu.__
03,DEL : Code delete__
04,TAB : Tab_	_
05,VER : Space_ _
06,PgUp: Next page__
07,PgDn: Previous page__
08,f.4 : Copy__
09,f.5 : Reference__
10,f.6 : Help__
11,f.7 : Page select__
12,f.9 : To previous data__

_COMXWI,31,3,1,45,15
01,Press ESC to previous menu_

_COMSTB,Start communication ?_
_COMCL6,Service No. 6-20 send ? _
_COMTYP,Disagree System type._
_COMVER,Disagree Version._
_COMMOD,Disagree Mode._
_COMUPD,Update to system data ? _
_COMCON,Continue communication ? _

***** modem
_MODCWI,70,15,0,0,0 ###
00,06MODEM_
GUIDEL, f.1:Dialing 	1 f.2:Org.side 	1 f.3:answer side	1 f.4:Discon. 	1 f.6:Speed_

_MODNCS,CTS not ready_###
_MODNRD,MODEM not ready_###

_MODAWI,40,3,0,35,3 ###
01,Auto dial_###
02,Originate_###
03,Answer_###
04,Disconnect_###
05,Auto answer_###

_COMSWI,30,5,3,0,0 ###
01,Start communication_1_###
02,Auto answer_2_###
03,End_3_###
GUIDEL, ESC:End 	1 f.6:Speed 	1 f.9:MODEM _###

***** print
_PRIMWI,23,7,5,0,0
00,09Print_
01All of system data_1_
02Service No. select_2_
03Customer_3_
04TEN/LEN last No._4_
05Printer select_5_
GUIDEL, ESC:To Main menu 	1, CR:Start _

_PRIIWI,28,13,11,0,0
00,04Class menu_
01, 1 System(basic)_01_
02, 2 TEN data(basic)_02_
03, 3 Line associated_03_
04, 4 Group assigments_04_
05, 5 Loop selection_05_
06, 6 SMDR parameters_06_
07, 7 System options_07_
08, 8 Terminal options_08_
09, 9 Line options_09_
10,10 Doorphone/Paging_10_
11,11 Speed dial/One touch_11_
GUIDEL, ESC:To previous menu 	1, CR:Item menu _

_PRISWI,23,4,2,0,0
0180(A4) column_80_
02132 column_132_
GUIDEL, ESC:To previous menu _

_PRINWI,23,4,2,0,0
01,Last TEN No. : _
02,Last LEN No. : _
03,Last ID  No. : _
GUIDEL, ESC:To previous menu 	1, f.9:Default _

_PRIXWI,31,4,2,0,0
01,Print_
02,Press ESC to exit_

_PRICHD, DX-E Series
 Digital hyblid telephone system
 Program record form_

_PRINRD,Printer Not ready_
_PRIEXT,Print stop ?_
_PRIRST,Continue ?_
_PRIPTI,	70,Page _
_PRIDAT,	50,_

***Edit
_EDITWI,28,13,11,0,0
00,04Class menu_
01, 1 System(basic)_01_
02, 2 TEN data(basic)_02_
03, 3 Line associated_03_
04, 4 Group assigments_04_
05, 5 Loop selection_05_
06, 6 SMDR parameters_06_
07, 7 System options_07_
08, 8 Terminal options_08_
09, 9 Line options_09_
10,10 Doorphone/Paging_10_
11,11 Speed dial/One touch_11_
GUIDEL, ESC:To previous menu 	1, CR:Item menu _

_EDIIWI,50,15,0,30,5
00,18Item menu_
GUIDEL, ESC:To Class menu 	1, CR:To Edit_

_EDICWI,80,22,0,1,2
00,34Edit_
GUIDEL, ESC:To Item menu 	1, CR:To Next item 	1, End:Help _

_REFEWI,80,22,0,1,2
00,34Reference_
GUIDEL, ESC:To previous item 	1, End:Help _

_REFSWI,21,4,2,0,0
00,06Reference_
01,Service No. : _
02,   Item No. : _

_COPYWI,32,4,2,0,0
00,12Copy_
01,Destination start No. : _
02,              end No. :_

_PAGSWI,13,3,1,0,0
00,01Page select_
01,Page : _

_OPHELP,30,17,15,0,0
00,10Edit help_
01,CR  : To Next service No._
_
02,ESC : To Menu__
03,DEL : Code delete__
04,TAB : Tab_	_
05,VER : Space_ _
06,PgUp: Next page__
07,Pgdn: Previous page__
08,f.1 : Previous service No.__
09,f.2 : Next class__
10,f.3 : Preivous class__
11,f.4 : Copy__
12,f.5 : Reference__
13,f.6 : Help__
14,f.7 : Page select__
15,f.9 : To previous data__

_REFHLP,30,8,6,0,0
00,13Edit help_
01,ESC : To previous item__
02,PgUp: Next page__
03,PgDn: Previous page__
04,f.5 : Reference__
05,f.6 : Help__
06,f.7 : Page select__

_EDITUN, Undefine service number_
_PSELYN,To previous data ?_

_OPTMWI,15,3,1,0,0
00,03Option_
01Infomation_1_
GUIDEL, ESC:To Main menu 	1, CR:Start _

_OPTIWI,80,22,0,1,2
00,34Infomation_
GUIDEL, ESC:To previous menu 	1, PgUp 	1,PgDn _

_QUITYN,Realy quit without saving_

_
_QUITLN,Realy quit without disconnect line_###

*** DXE-1240
_TYPEE  ### if DXV TYPEV
00,L12,T40,I40,D400
01,04,05,06
  ,10,11,12
  ,50,51,53,54,55,56
  ,76,77_				for class 01
02,01,02,03,04,05,06,07,08,09
  ,10,11,12,13,16,17,18_		for class 02
03,01,02,03,04,05,06,07,09
  ,10
  ,20_					for class 03
04,01,02,06_				for class 04
05,01_					for class 05
06,01,02,03,04,05,06,07,08,09
  ,10,11,12,13,14,15,19_		for class 06
07,01,02,03,04,05,07
  ,11,12,13,17,18
  ,20,22,24,25,26,27,29
  ,30,31,32,33,34,35,36,37,38,39
  ,40,41,42,43,44,45,46,47,48,49
  ,50,51,54,58,59
  ,60,65,66,67,68
  ,70,71,72,74,76,77,78,79
  ,80,81,82,83,85,86,87,88,89
  ,90,91,92,93_				for class 07
08,01,02,03,04,05,06,07,08,09
  ,11,12,13,14,16,17,18
  ,20,23,24,26,27,28,29
  ,30,31,32,33,34,35,36,38
  ,40,41,42_				for class 08
09,01,02,03,04,05,08,09
  ,10
  ,20,21,22_				for class 09
10,03,04_				for class 10
11,01,02,03,04,05,06,07,08,09
  ,10,12_				for class 11

_TYPEE_M01_ ### if DXV TYPEV_M01
_TYPEE_M02_ ### if DXV TYPEV_M02

*** DXE-2470
_TYPEE$  ### if DXV TYPEV$
00,L24,T70,I70,D700
01,04,05,06
  ,10,11,12
  ,50,51,53,54,55,56
  ,76,77_				for class 01
02,01,02,03,04,05,06,07,08,09
  ,10,11,12,13,16,17,18_		for class 02
03,01,02,03,04,05,06,07,09
  ,10
  ,20_					for class 03
04,01,02,06_				for class 04
05,01_					for class 05
06,01,02,03,04,05,06,07,08,09
  ,10,11,12,13,14,15,19_		for class 06
07,01,02,03,04,05,07
  ,11,12,13,17,18
  ,20,22,24,25,26,27,29
  ,30,31,32,33,34,35,36,37,38,39
  ,40,41,42,43,44,45,46,47,48,49
  ,50,51,54,58,59
  ,60,65,66,67,68
  ,70,71,72,74,76,77,78,79
  ,80,81,82,83,85,86,87,88,89
  ,90,91,92,93_				for class 07
08,01,02,03,04,05,06,07,08,09
  ,11,12,13,14,16,17,18
  ,20,23,24,26,27,28,29
  ,30,31,32,33,34,35,36,38
  ,40,41,42_				for class 08
09,01,02,03,04,05,08,09
  ,10
  ,20,21,22_				for class 09
10,03,04_				for class 10
11,01,02,03,04,05,06,07,08,09
  ,10,12_				for class 11

_TYPEE$_M01_ ### if DXV TYPEV$_M01
_TYPEE$_M02_ ### if DXV TYPEV$_M02

*** DXE-36100
_TYPEE6  ### if DXV TYPEV6
00,L36,T100,I100,D1000
01,04,05,06
  ,10,11,12
  ,50,51,53,54,55,56
  ,76,77_				for class 01
02,01,02,03,04,05,06,07,08,09
  ,10,11,12,13,16,17,18_		for class 02
03,01,02,03,04,05,06,07,09
  ,10
  ,20_					for class 03
04,01,02,06_				for class 04
05,01_					for class 05
06,01,02,03,04,05,06,07,08,09
  ,10,11,12,13,14,15,19_		for class 06
07,01,02,03,04,05,07
  ,11,12,13,17,18
  ,20,22,24,25,26,27,29
  ,30,31,32,33,34,35,36,37,38,39
  ,40,41,42,43,44,45,46,47,48,49
  ,50,51,54,58,59
  ,60,65,66,67,68
  ,70,71,72,74,76,77,78,79
  ,80,81,82,83,85,86,87,88,89
  ,90,91,92,93_				for class 07
08,01,02,03,04,05,06,07,08,09
  ,11,12,13,14,16,17,18
  ,20,23,24,26,27,28,29
  ,30,31,32,33,34,35,36,38
  ,40,41,42_				for class 08
09,01,02,03,04,05,08,09
  ,10
  ,20,21,22_				for class 09
10,03,04_				for class 10
11,01,02,03,04,05,06,07,08,09
  ,10,12_				for class 11

_TYPEE6_M01_ ### if DXV TYPEV6_M01
_TYPEE6_M02_ ### if DXV TYPEV6_M02


_CLASS_MENU01
04 1-04 Night mode change over(Auto)_
T2NIGHT MODE_
T3 HH MM_
P0_
P1:_
t00,
	50,hh:mm =_
p0_
p1:_
dxy59,1__

05 1-05 Day mode changer over(Auto)_
T2DAY MODE_
T3 HH MM_
P0_
P1:_
*** print
t00,
	50,hh:mm =_
p0_
p1:_
dxy59,1__

06 1-06 Extension number digits_
T1 P  D_
DXY2,5
*** print
t00,
	48,Parameter  Digit_
dxy53,2
p0 ----- __

10 1-10 Make ratio_
T3 R_
P0_
t00,
	51,Data =          0:33% 1:39%_
p0_
dxy59,1__

11 1-11 PBX night mode auto change over_
T2PBX NIGHT MODE_
T3 HH MM_
P0_
P1:_
t00,
	50,hh:mm =_
p0_
p1:_
dxy59,1__

12 1-12 PBX day mode auto change over_
T2PBX DAY MODE_
T3 HH MM_
P0_
P1:_
t00,
	50,hh:mm =_
p0_
p1:_
dxy59,1__

50 1-50 Installation Date_
T2INSTAL.DATE_
T3 YY MM DD_
P0_
P1-_
P2-_
*** print
t01,
	44,INSTAL.DATE =
	49,         YY MM DD_
p0_
p1-_
p2-_
dxy59,1__

51 1-51 Record starting date_
T3 YY MM DD_
P0_
P1-_
P2-_
*** print
t01,
	42,STARTING DATE =
	49,         YY MM DD_
p0_
p1-_
p2-_
dxy59,1__

53 1-52/53 Fault Counter/Record data_
T01-52 Fault Counter_
T1 Counter :_
@012,4
T31-53 Fault Record data
COUNTER   DATE   TIME  FAULT
    No. YY MM DD hh mm N P _
DXY5,9
ML10
*** print
t00,
	48,Counter =_
%059,1
t14,

	8,1-53 Fault Record data
	10,FAULT     DATE   TIME  FAULT
	10,COUNTER YY MM DD hh mm N P _
dxy15,6
ml10__

54 1-54 Location of Option Unit_
T1SLOT UNIT_
T2 No. NAME_ 
DXY3,6
P0-_
ML8
HT20
0C,HFU_
14,HFCU+COTRU_
1C,HFCU_
24,CFU+COTRU(HL)_
2C,CFU+COTRU(L)_
34,CFU+COTRU(H)_
3C,CFU_
78,SCU_
C3,COU_
CC,PBRT_
DA,LDU_
9A,PMDMU_
E8,SMDR_
F1,VSU_
B8,ICOU_
B3,DCIU
B0,DCIU_
FF,NO USE_
*** print
t02,
	10,SLOT
	10, No. UNIT NAME_ 
dxy13,4
ml8
ht17__

55 1-55 Status of terminal_
T0TEN STATUS_
T1No. No._
P0-_
DXY1,5
ML10
HT8
*** print
t08,
	9,01:Idle or not installed
	9,08:B-ch busy
	9,11:ICM dialing  12:ICM calling  13:ICM talking
	9,14:ICM on hold  15:Programming
	9,16:Activating paging  17:Activating Camp-on
	9,18:Receiving busy tone
	9,19:Activating series call
	9,21:C/O dialring  23:C/O talking_
t12,
	10,TEN COND.
	10, No. No._
dxy12,12
ht8__

56 1-56 The state of B-channel use_
T0TEN_
T1No. SL CH_
DXY2,5
HT10
ML10
*** print
t01,
	10,TEN SL CH_
dxy12,3
ht10__

76 1-76 TEN - SLOT/TEI_
T1TEN SL TE_
DXY2,5
ML10
HT11
*** print
t01,
	10,TEN SL TE_
dxy12,3
ht11__

77 1-77 SLOT/TEI - TEN_
T1       Slot No._
T2         01   02   03   04   05   06   07   08   09   10_
T3          |    |    |    |    |    |    |    |    |    |
   01 -
   02 -
 T 03 -
 E 04 -
 I 05 -
   06 -
 N 07 -
 o 08 -
 . 09 -
   10 -
   11 -_
ML11
DXY10,7
P0_
HT5
*** print
t03,
	4,        Slot No.
	4,         01   02   03   04   05   06   07   08   09   10_
	4,          |    |    |    |    |    |    |    |    |    |
	4,   01 -
	4,   02 -
	4, T 03 -
	4, E 04 -
	4, I 05 -
	4,   06 -
	4, N 07 -
	4, o 08 -
	4, . 09 -
	4,   10 -
	4,   11 -_
dxy14,5
ml11
ht5
p0__

_CLASS_MENU02
01 2-01 Terminal type_
T0TEN TT_
DXY2,4
HT8
ML10
**** print
t04,
	7,TT means Terminal Type.
	8,00:Unused
	8,02:12 Key Tel.Dot Display
	8,03:Single Line Tel.(DP Dial)
	8,04:Single Line Tel.(DTMF Dial)
	8,05:DSS Console
	8,06:DLS Console
	8,07:PC
	8,08:DSAP
	8,11:12 Key Tel.Standard
	8,14:24 Key Tel.Standard
	8,18:24 Key Tel.Dot Display_
t12,
	09,TEN
	09,No. TT_
dxy11,16_
ht8
ml10__

02 2-02 Extension number_
T0TEN Extention_
T1No. number_
DXY2,5
HT9
ML10
**** print
dxy11,4
ht9
ml10
t02,
	9,TEN ICM
	9,No. No.__

03 2-03 Line Key Definition_
T0 TEN No.=_
T2   KEY_
T3 No. DEF  PARAMETER_
@011,3
DXY3,7
ML12
P0--_
P1 - _
HT17
t12,
	9,  KEY   PARA-
	9,No. DEF METER
_
t20,	4,TEN_
%06,4
dxy11,4
p0--_
p1 - _
ht14__

04 2-04 Class of Service_
T0TEN_
T1No. DN_
DXY2,5
HT8
ML10
**** print
dxy10,3
ml10
ht8
t01,
	8,TEN DN_
t20,	53,NOTE
	65,D:Day time
	65,N:Night time

	65,0:Class 0
	65,1:class 1
	65,2:Class 2
	65,3:Class 3
	65,4:Class 4
	65,5:Class 5
	65,6:Class 6__

05 2-05 Speed dial permit_
T0TEN_
T1No. DN_

DXY2,5
HT8
ML10
***** print
dxy11,3
ml10
ht8
t01,
	9,TEN DN_
t20,	53,NOTE
	65,D:Day time
	65,N:Nigth time

	65,0:disable
	65,1:enable__

06 2-06 CO line restriction_
T0 TEN No.=_
T2LINE_
T3 No. DN_
@011,3
DXY3,7
ML12
HT10
***** print
dxy11,9
%06,9
ht10
t05,
	10,D=Day time   N=Night time
	10,0:No restriction
	10,1:Outgoing call restriction
	10,2:Incoming call restriction
	10,3:Outgoing and Incoming call restriction_
t12,
	8,Line
	8, No. DN
_
t20,	4,TEN__

07 2-07 Outgoing line access priority_
T0TEN LINE_
T1No. No._
DXY2,5
HT8
ML10
***** print
dxy12,4
ht8
ml10
t02,
	9,TEN Line
	9, No. No.__

08 2-08 Outgoing CO auto seizure_
T0 TEN No.=_
T2LINE_
T3 No.  Au_
@011,3
DXY3,7
ML12
P0--_
HT10
***** print
dxy11,5
%06,5
ht7

t01,
	10,**0:disable  1:enable**_
t12,
	8,Line
	8, No. C_
t20,
	4,TEN__

09 2-09 Incoming CO auto seizure_
T0 TEN No.=_
T2LINE_
T3 No.  Au_
@011,3
DXY3,7
ML12
P0--_
HT10
***** print
dxy11,5
%06,5
ht7

t01,
	10,**0:disable  1:enable**_
t12,
	8,Line
	8, No. C_
t20,
	4,TEN__

10 2-10 Executive set assignment_
T0TEN_
T1No. EX_
P0-_
DXY2,5
HT8
ML10
**** print
dxy11,5
ht7
ml10
t02,
	12,0:Not assigned to EXecutive
	12,1:Assigned to EXecutive_
t11,
	9,TEN EX__

11 2-11 Secretary set assignment_
T0    SECRE-_
T1TEN TARY_
T2No. #1 #2_
P0-_
P1-_
DXY2,6
HT13
ML10
**** print
dxy7,6
ht13
ml10
t02,
	12,* mark is Assigned EXecutive extension
	12,#1:First Secretary   #2:Second Secretary_
t12,
	4,TEN Secretary
	5,No. #1 #2__

12 2-12 P.C. Associated Tel set_
T0KT  PC_
T1TEN TEN_
T2No. No._
DXY2,6
HT10
ML10
**** print
dxy10,5
ht10
ml10
t14,
	8,KT  PC
	8,TEN TEN
	8,No. No.__

13 2-13 DSS/DLS Associated Tel set_
T0DSS/DLS   KT TEN No._
T1No.(TEN)- F -- S -- T_
P0(   )-_
P1--_
P2--_
DXY2,5
ML12
**** print
dxy8,4
p0(   )-_
p1--_
p2--_
ht25
ml6
t02,
	6, DSS/DLS   KT TEN No.
	6, No.(TEN)- F -- S -- T__

16 2-16 Held line answer restriction_
T0 LINE No.=_
T1TEN DN_
@012,3
DXY2,5
ML10
P0-_
HT8
***** print
dxy11,6
%05,6
ht8
t02,
	10,D:Day time   N:Night time
	10,**0:disable    1:enable**_
t12,
	9,TEN
	9,No. DN
_
t20,   LINE__

17 2-17 DSS console key assignment_
T0DSS No.=     (DSS TEN No.=    )_
T2KEY TEN_
T3No. No._
@010,3
@128,3
DXY3,7
HT8
ML10
***** print
dxy23,4
%014,3
%118,4
ml10
ht8
t12,
	21,KEY TEN
	21,No. No._
t20,
	4,DSS No.=
	4,(DSS TEN No.=    )__

18 2-18 DLS Console key assignment_
T0DLS No.=     (DLS TEN No.=    )_
T2KEY_
T3No. D PAR_
@010,3
@128,3
DXY2,7
HT9
ML10
***** print
dxy23,4
%014,3
%118,4
ht9
t12,
	21,KEY
	21,No. D PAR_
t20,
	4,DLS No.=
	4,(DLS TEN No.=    )__

_CLASS_MENU03
01 3-01 Line definition_
T0  LINE_
T1 No. DEF_
DXY3,5
P0--_
HT12
ML12
***** print
dxy11,6
ht7
tpf
p0--_
t02,
	12,00:Unused   01:DP(20pps)   02:DP(10pps)
	12,03:DTMF     04:Tandem trunk_
t12,
	9, LINE
	9,No. DEF.__

02 3-02 Circuit type_
T0  LINE_
T1 No. TYPE_
DXY3,5
P0--_
HT12
ML12
***** print
dxy11,5
ht7
p0--_
t01,
	12,1:CO line   2:PBX line_
t12,
	9, LINE
	9,No. TYPE__

03 3-03 Ringing station (day)_
T0 LINE No.=_
T2TEN D_
DXY2,6
@012,3
HT8
ML10
***** print
dxy11,5
%05,5
ht7
t01,
	12,0:No ringing   1:Ringing_
t12,
	9,TEN
	9,No. D
_
t20,   LINE__

04 3-04 Ringing station (night)_
T0 LINE No.=_
T2TEN N_
DXY2,6
@012,3
HT7
ML10
***** print
dxy10,5
%05,5
ht7
t01,
	12,0:No ringing   1:Ringing_
t12,
	9,TEN
	9,No. N
_
t20,   LINE__

05 3-05 Line select D/N change over_
T0  LINE_
T1 No. Ma_
DXY3,5
P0-_
HT12
ML12
***** print
dxy11,5
ht12
p0-_
t01,
	12,0:Manual   1:Auto_
t12,
	8,LINE
	8, No. Au__

06 3-06 D/N mode setup telset_
T0 LINE  KT_
T1  No. F   S_
DXY4,5
HT12
ML12
***** print
dxy11,5
ht12
p0-_
p1-_
t01,
	12,F:First Extension  S:Second Extension_
t12,
	8,LINE  KT
	8, No. F  S__

07 3-07 PBX night mode transfer_
T0 LINE_
T1  No. T_
DXY4,5
HT12
ML12
***** print
dxy11,5
ht7
p0-_
t01,
	10,**0:disable   1:enable**_
t12,
	8,LINE
	8, No. Au__

08 3-08 Power Failure Tel._
T0 LINE PF_
T1  No. TEN_
DXY4,5
HT12
ML12
***** print
dxy11,4
ht7
p0--_
t12,
	8,LINE PF
	8, No. TEN__

09 3-09 Condition of Answering_
T0 LINE _
T1  No. C_
DXY4,5
HT12
ML12
***** print
dxy11,5
ht7
p0-_
t01,
	12,0:Reversing   1:Time out_
t12,
	8,LINE
	8, No. C__

10 3-10 Trunk access groups_
T0 LINE_
T1  No. G_
DXY4,5
HT12
ML12
***** print
dxy11,5
ht7
p0-_
t01,
	12,0:Unassigned   1 to 9:Group 1 to 9_
t12,
	8,LINE
	8, No. G__

11 3-11 椏嬥僇僂儞僩掆巭忦審_
T0 LINE _
T1  No. C_
DXY4,5
HT15
ML12__

20 3-20 Flashing/Grounding_
T0 LINE_
T1  No. L_
DXY4,5
HT12
ML12
***** print
dxy11,5
ht12
p0-_
t01,
	12,0:Flashing   1:Grounding_
t12,
	8,LINE
	8, No. L__

_CLASS_MENU04
01 4-01 Station Grouping_
T0 Group No.=_
T1TEN G_
@013,3
DXY2,5
HT7
ML10
***** print
dxy12,5
%05,6
ht7

t01,
	12,0:Not assigned    1:Assigned_
t12,
	10,TEN
	10,No. G
_
t20,   GROUP
    No.__

02 4-02 Pilot Number Setup_
T0 GROUP PILOT_
T1  No.   No._
P0 - _
DXY4,5
HT15
ML10
***** print
dxy11,4
ht15
ml10
p0 - _
t12,
	8,GROUP PILOT
	8, No.   No.__

03 4-03 擂脖俨輵銜\屇傃弌偟斣崋_
T0 GROUP PILOT_
T1  No.   No._
P0 - _
DXY4,5
HT15
ML10__

06 4-06 Alternate answering_
T0 Group No.=_
T2  GN P_
@013,3
DXY3,6
HT15
ML10
***** print
dxy12,4
%05,5
ht7
ml4
t01,
	12,0:Not assigned    1:Assigned_
t11,
	9, No. G
_
t20,   GROUP
    No.__

_CLASS_MENU05
01 5-01 Line assignment_
T0 Group No.=_
T2 LINE_
T3  No. A_
@013,3
DXY4,7
HT12
ML12
***** print
dxy12,5
%05,6
ht7
t01,
	12,0:Unassigned    1:Assigned_
t12,
	9,LINE
	9, No. A
_
t20,   GROUP
    No.__

_CLASS_MENU06
01 6-01 Call duration timer_
T1 Duration Timer=_
T2     Sec._
P0_
DXY2,5
*** print
t00,
	40,Timer =     Sec._
p0_
dxy49,1__

02 6-02 Account code entry_
T1 Account code=_
P0_
DXY2,5
*** print
t00,
	39,A.code =_
p0_
dxy49,1__

03 6-03 Incoming print out_
T1 Incoming print out=_
P0_
DXY2,5
*** print
t00,
	40,Print =_
t11,
	60,0:print out
	60,1:not p.out_
p0_
dxy49,1__

04 6-04 Restriction data_
T1 Restriction data=_
P0_
DXY2,5
*** print
t00,
	40,Print =_
t11,
	60,0:print out
	60,1:not p.out_
p0_
dxy49,1__

05 6-05 Outgoing number print out_
T1 Outgoing number print out=_
P0_
DXY2,5
*** print
t00,
	40,Print =_
t11,
	60,0:p.out
	60,1:p.out w/o last 2_
p0_
dxy49,1__

06 6-06 PBX connection_
T1 PBX connection=_
P0_
DXY2,5
*** print
t00,
	40,Print =_
t11,
	60,0:print out
	60,1:not p.out_
p0_
dxy49,1__

07 6-07 Date print out format_
T1 Date print out format=_
P0_
DXY2,5
*** print
t00,
	40,Print =_
t11,
	60,0:M/D/Y  1:Y/M/D
	60,2:D/M/Y  3:Y/D/M_
p0_
dxy49,1__

08 6-08 #Digit print out_
T1 #Digit print out=_
P0_
DXY2,5
*** print
t00,
	40,Print =_
p0_
dxy49,1__

09 6-09 Duration time printout_
T1 Duration time out=_
T2     Sec._
P0_
DXY2,5
*** print
t00,
	40,Timer =     Sec._
t10,
	60,0 Sec=print out all_
p0_
dxy49,1__

10 6-10 TEN print out_
T0TEN_
T1No. P_
DXY2,5
HT7
ML10
**** print
dxy11,5
ht7
ml10
t01,
	12,0:Not print out  1:Print out_
t12,
	9,TEN
	9,No. P__

11 6-11 Line number print out_
T0LINE_
T1 No. P_
DXY3,5
HT10
ML12
**** print
dxy11,5
ht12
t01,
	12,0:Not print out  1:Print out_
t12,
	8,LINE
	8, No. P__

12 6-12 Account code_
T1 Account code=_
P0_
DXY2,5
*** print
t00,
	39,A.code =_
t11,
	64,0:disable
	64,1:enable_
p0_
dxy49,1__

13 6-13 Account code redial_
T1 Account code redial=_
P0_
DXY2,5
*** print
t00,
	39,A.code =_
t11,
	64,0:disable
	64,1:enable_
p0_
dxy49,1__

14 6-14 SLT Account code_
T1 SLT Account code=_
P0_
DXY2,5
*** print
t00,
	39,A.code =_
t11,
	64,0:disable
	64,1:enable_
p0_
dxy49,1__

15 6-15 Forced account code_
T0TABLE ACCOUNT  PAGE=_
T1 No.   CODE_
@021,3
DXY3,5
HT15
ML10
**** print
dxy11,4
ht17
ml10
p0 -_
t12,
	9,TABLE ACCOUNT
	9, No.   CODE__

19 6-19 Printer bit rate_
T1 Printer bit rate=_
P0_
DXY2,5
*** print
t00,
	38,Printer =_
t14,
	30,**1: 300bps non parity  2: 300bps parity
	30,**3:1200bps non parity  4:1200bps parity
	30,**5:2400bps non parity  6:2400bps parity
	30,**7:4800bps non parity  8:4800bps parity_
p0_
dxy49,1__

20 6-20 Initialisation_
T1 Initialisation=_
P0_
DXY2,5__

_CLASS_MENU07
01 7-01 Trunk # Indication_
T1 Trunk # Indication=_
P0_
DXY2,5
*** print
t00,
	50,DATA =_
t11,
	10,**0:not indication  1:indication**_
p0_
dxy58,1__

02 7-02 I.C. Handsfree answer_
T1 I.C.Handsfree answer=_
P0_
DXY2,5
*** print
t00,
	50,DATA =_
t11,
	10,**0:disable  1:enable**_
p0_
dxy58,1__

03 7-03 Conference call_
T1 Conference call=_
P0_
DXY2,5
*** print
t00,
	50,DATA =_
t11,
	10,**0:disable  1:enable**_
p0_
dxy58,1__

04 7-04 Series call(Return Transfer)_
T1 Series call=_
P0_
DXY2,5
*** print
t00,
	50,DATA =_
t11,
	10,**0:disable  1:enable**_
p0_
dxy58,1__

05 7-05 Message waiting_
T1 Message waiting=_
P0_
DXY2,5
*** print
t00,
	50,DATA =_
t11,
	10,**0:disable  1:enable**_
p0_
dxy58,1__

07 7-07 Exclusive hold_
T1 Exclusive hold=_
P0_
DXY2,5
*** print
t00,
	50,DATA =_
t11,
	10,**0:disable  1:enable**_
p0_
dxy58,1__

08 7-08 DTMF transmission(Class-1)_
T1 DTMF transmission(Class-1)=_
P0_
DXY2,5
*** print
t00,
	50,DATA =_
t11,
	10,**0:disable  1:enable**_
p0_
dxy58,1__

09 7-09 DTMF transmission(Class-2)_
T1 DTMF transmission(Class-2)=_
P0_
DXY2,5
*** print
t00,
	50,DATA =_
t11,
	10,**0:disable  1:enable**_
p0_
dxy58,1__

10 7-10 DTMF transmission(Class-3 to 6)_
T1 DTMF transmission(Class-3 to 6)=_
P0_
DXY2,5
*** print
t00,
	50,DATA =_
t11,
	10,**0:disable  1:enable**_
p0_
dxy58,1__

11 7-11 All call paging_
T1 All call paging=_
P0_
DXY2,5
*** print
t00,
	50,DATA =_
t11,
	10,**0:disable  1:enable**_
p0_
dxy58,1__

12 7-12 Line camp-on/hold free transfer_
T1 Line camp-on=_
P0_
DXY2,5
*** print
t00,
	50,DATA =_
t11,
	10,**0:null  1:camp-on  2:hold**_
p0_
dxy58,1__

13 7-13 Composite communication_
T1 Composite communication=_
P0_
DXY2,5
*** print
t00,
	50,DATA =_
t11,
	10,**0:disable  1:enable**_
p0_
dxy58,1__

17 7-17 Station camp-on_
T1 Station camp-on=_
P0_
DXY2,5
*** print
t00,
	50,DATA =_
t11,
	10,**0:disable  1:enable**_
p0_
dxy58,1__

18 7-18 Step call_
T1 Step call=_
P0_
DXY2,5
*** print
t00,
	50,DATA =_
t11,
	10,**0:disable  1:enable**_
p0_
dxy58,1__

20 7-20 Preset call_
T1 Preset call=_
P0_
DXY2,5
*** print
t00,
	50,DATA =_
t11,
	10,**0:disable  1:enable**_
p0_
dxy58,1__

22 7-22 Extension page chime_
T1 Extension page chime=_
P0_
DXY2,5
*** print
t00,
	50,DATA =_
t11,
	10,**0:disable  1:enable**_
p0_
dxy58,1__

24 7-24 All call page answer back_
T1 All call page answer back=_
P0_
DXY2,5
*** print
t00,
	50,DATA =_
t11,
	10,**0:disable  1:enable**_
p0_
dxy58,1__

25 7-25 Room monitor_
T1 Room monitor=_
P0_
DXY2,5
*** print
t00,
	50,DATA =_
t11,
	10,**0:disable  1:enable**_
p0_
dxy58,1__

26 7-26 Doorphone box_
T1 Doorphone No._
T2 Doorphone No._
P0 = _
DXY15,4
ML2
*** print
t01,
	50,Doorphone No.
	50,Doorphone No._
t11,
	10,**0:not provided  1:provided**_
p0 =_
ml2
dxy64,1__

27 7-27 Lock control_
T1 Lock control No._
T2 Lock control No._
P0 = _
DXY18,4
ML2
*** print
t01,
	47,Lock control No.
	47,Lock control No._
t11,
	10,**0:not provided  1:provided**_
p0 =_
ml2
dxy64,1__

29 7-29 Trunk reselection_
T1 Trunk reselection=_
P0_
DXY2,5
*** print
t00,
	50,DATA =_
t11,
	10,**0:disable  1:enable**_
p0_
dxy58,1__

30 7-30 Hold alarm timer_
T1 Hold alarm timer=_
T2    x10 Sec._
P0_
DXY2,5
*** print
t00,
	49,Timer =     x10 Sec._
t11,
	10,**0:no feature**_
p0_
dxy58,1__

31 7-31 Hold line termination timer_
T1 Timer=_
T2    x10 Sec._
P0_
DXY2,5
*** print
t00,
	49,Timer =     x10 Sec._
t11,
	10,**0:no feature**_
p0_
dxy58,1__

32 7-32 Unanswered incoming alarm timer_
T1 Timer=_
T2    x10 Sec._
P0_
DXY2,5
*** print
t00,
	49,Timer =     x10 Sec._
t11,
	10,**0:no feature**_
p0_
dxy58,1__

33 7-33 Long-cycle ringing period_
T1 Timer=_
T2     Sec._
P0_
DXY2,5
*** print
t00,
	49,Timer =     Sec._
p0_
dxy58,1__

34 7-34 Clock alarm tone duration_
T1 Timer=_
T2     Sec._
P0_
DXY2,5
*** print
t00,
	49,Timer =     Sec._
p0_
dxy58,1__

35 7-35 Long conversation warning tone start_
T1 Timer=_
T2     min._
P0_
DXY2,5
*** print
t00,
	49,Timer =     Min._
p0_
dxy58,1__

36 7-36 Long conversation warning initial start_
T1 Timer=_
T2     Sec._
P0_
DXY2,5
*** print
t00,
	49,Timer =     Sec._
p0_
dxy58,1__

37 7-37 Doorphone chime tone duration_
T1 Timer=_
T2     Sec._
P0_
DXY2,5
*** print
t00,
	49,Timer =     Sec._
p0_
dxy58,1__

38 7-38 Doorphone chime termination duration_
T1 Timer=_
T2     Sec._
P0_
DXY2,5
*** print
t00,
	49,Timer =     Sec._
p0_
dxy58,1__

39 7-39 Flashing time specification_
T1 Timer=_
T2    x0.0165 Sec._
P0_
DXY2,5
*** print
t00,
	49,Timer =     x0.1 Sec._
p0_
dxy58,1__

40 7-40 Line disconnect/lock up timer_
T1 Timer=_
T2    x0.1 Sec._
P0_
DXY2,5
*** print
t00,
	49,Timer =     x0.1 Sec._
p0_
dxy58,1__

41 7-41 Display change over timer_
T1 Timer=_
T2     Sec._
P0_
DXY2,5
*** print
t00,
	49,Timer =     Sec._
p0_
dxy58,1__

42 7-42 Monitor to timer change over_
T1 Timer=_
T2     Sec._
P0_
DXY2,5
*** print
t00,
	49,Timer =     Sec._
p0_
dxy58,1__

43 7-43 Voice message timer_
T1 Timer=_
T2    x10 Sec._
P0_
DXY2,5
*** print
t00,
	49,Timer =     x10 Sec._
t11,
	10,**0:unlimited**_
p0_
dxy58,1__

44 7-44 Trunk to Trunk transfer/forward_
T1 Timer=_
T2    x10 Sec._
P0_
DXY2,5
*** print
t00,
	49,Timer =     x10 Sec._
t11,
	10,**0:unlimited**_
p0_
dxy58,1__

45 7-45 Hooking pulse for tandem connect_
T1 Timer=_
T2    x0.1 Sec._
P0_
DXY2,5
*** print
t00,
	49,Timer =     x0.1 Sec._
p0_
dxy58,1__

46 7-46 Hooking pulse time range_
T1 Timer=_
T2    x0.1 Sec._
P0_
DXY2,5
*** print
t00,
	49,Timer =     x0.1 Sec._
p0_
dxy58,1__

47 7-47 Exclusive hold to common hold_
T1 Timer=_
T2    x10 Sec._
P0_
DXY2,5
*** print
t00,
	49,Timer =     x10 Sec._
t11,
	10,**0:unlimited**_
p0_
dxy58,1__

48 7-48 Non-sound detection forced cut off_
T1 Timer=_
T2     Sec._
P0_
DXY2,5
*** print
t00,
	49,Timer =     Sec._
t11,
	10,**0:unlimited**_
p0_
dxy58,1__

49 7-49 Message waiting clear time_
T1 Timer=_
T2     Hour_
P0_
DXY2,5
*** print
t00,
	49,Timer =     Hour_
t11,
	10,**0:unlimited**_
p0_
dxy58,1__

50 7-50 Incoming call tone definition_
T0REGISTRATION_
T1 No. P FREQ._
DXY3,5
ML8
*** print
t00,
	9,Registration
	9, No. P FREQ._
t10,
	30,**P=Frequancy pttern**
	30, 0:Single(1freq.)     1:Dual-slow(2freq.)
	30, 2:Dual-fast(2freq.)  3:Tripple(3freq.)
	30, 4:Quad(4freq.)

	30,  Registration Freq.
	30, 1:0.4KHz  2:0.5KHz  3:0.6KHz  4:0.8KHz
	30, 5:1.0KHz  6:1.3KHz  7:2.0KHz_
p0-_
p1-_
ml8
dxy12,4__

51 7-51 DTMF signal spec._
T1 DTMF signal spec.=_
P0_
DXY2,5
*** print
t00,
	50,Data =_
t11,
	10,**0:75mS on/off  1:100mS on/off  2:150mS on/off**_
p0_
dxy58,1__

53 7-53 Restricted class dial digit_
T0CLASS_
T1  No. D_
P0-_
DXY4,5
ML6
*** print
t02,
	9,Class
	9,  No. D_
t10,
	30,**D=00:unlimited**_
p0-_
ml6
dxy13,4__

54 7-54 PBX access codes_
T1 PBX access code_
T2 TABLE_ 
T3   No. CODE_
P0-_
DXY5,7
ML4
*** print
t02,
	9,Table  Access
	9,  No.   CODE_
p0---_
ml4
dxy13,4__

58 7-58 MOH source_
T1 MOH souce=_
P0_
DXY2,5
*** print
t00,
	50,Data =_
t11,
	10,**0:not installed  1:installed**_
p0_
dxy58,1__

59 7-59 BGM source_
T1 BGM souce=_
P0_
DXY2,5
*** print
t00,
	50,Data =_
t11,
	10,**0:not installed  1:installed**_
p0_
dxy58,1__

60 7-60 Voice message connection_
T1 Voice message =_
P0_
DXY2,5
*** print
t00,
	50,Data =_
t11,
	10,**0:not installed  1:installed**_
p0_
dxy58,1__

65 7-65 FAX. Connection_
T0            LINE No._
T1 FAX. No._
T2 FAX. No._
P0 = _
DXY10,4
ML2
*** print
t03,
	9,           Line No.
	9,FAX. No.
	9,FAX. No._
p0 = _
ml2
dxy18,3__

66 7-66 Simplified voice recording_
T0PACKAGE_
T1  No. N_
P0--_
DXY4,5
ML8
*** print
t02,
	9,Package
	9,  No.   N_
t10,
	30,**0:no feature
	30,**1:trunk voice recording
	30,**2:extension voice recording
	30,**3:in-communication/private recording
	30,**4:station voice message_
p0---_
ml8
dxy13,4__

67 7-67 Voice recording extensions_
T1ASSIGN. TEN_
T2   No.  No._
P0--_
DXY5,6
ML2
*** print
t02,
	9,Assign. TEN
	9,   No.  No._
p0--_
ml2
dxy14,4__

68 7-68 Private voice recording_
T0ASSIGN. TEN_
T1   No.  No._
P0--_
DXY5,5
HT10
ML8
*** print
t02,
	9,Assign. TEN
	9,   No.  No._
p0--_
ml4
ht10
dxy14,4__

70 7-70 Max. digits of Local call(class 2/3)_
T1 Class #_
T2 Class #_
P0 = _
DXY9,4
ML2
*** print
t02,
	9, Class-      digits
	9, Class-      digits_
p0 = _
ml2
dxy17,2__

71 7-71 Max. digits of outgoing call(class 2-4)_
T1  Class-       digits_
T2  Class-       digits
  Class-       digits_
P0 = _
DXY9,4
ML3
*** print
t00,
	9, Class-       digits
	9, Class-       digits
	9, Class-       digits_
p0 = _
ml3
dxy17,2__

72 7-72 Flash/Function key_
T1Flash/Function key=_
P0_
DXY2,5
*** print
t00,
	50,Data =_
t12,
	10,**(FLASH)key pushing**
	10,  0:hooking  1:flashing_
p0_
dxy58,1__

74 7-74 COS Restriction on speed dial_
T0            R_
T1  Class-_ 
T2  Class- 
  Class-
  Class-_
P0 = _
DXY9,4
ML4
*** print
t00,
	50,0=Not restricted
	50,1=Restricted_
t14,
	9, Class-
	9, Class-
	9, Class-
	9, Class-_
p0 = _
ml4
dxy17,3__

76 7-76 Repeatdial pattern_ ###
T1pattern =_
P0_
DXY2,5
*** print
t00,
	50,Pattern =_
p0_
dxy58,1__

77 7-77 Permit code table for Class-2_
T1 No. PERMIT CODE_
DXY3,5
HT17
ML10
**** print
dxy11,3
ml20
ht20
p0 -_
t11,
	9, No. ACCESS CODE__

78 7-78 Permit code table for Class-3_
T1 No. PERMIT CODE_
DXY3,5
HT17
ML10
**** print
dxy11,3
ml20
ht20
p0 -_
t11,
	9, No. PERMIT CODE__

79 7-79 Permit code table for Class-4_
T1 No. PERMIT CODE_
DXY3,5
HT17
ML10
**** print
dxy11,3
ml20
ht20
p0 -_
t11,
	9, No. PERMIT CODE__

80 7-80 International call permit code_
T0    PERMIT_
T1 No.  CODE_
DXY3,5
HT17
ML10
**** print
dxy11,3
ht20
ml5
p0 -_
t11,
	9, No. PERMIT CODE__

81 7-81 Deny code table_
T0     DENY_
T1 No.  CODE_
DXY3,5
HT17
ML10
**** print
dxy11,3
ml5
ht20
p0 -_
t11,
	9, No. Restricted code__

82 7-82 Absence message_
T1Absence message =_
P0_
DXY2,5
*** print
t00,
	50,Data =_
t11,
	10,**0:disable  1:enable**_
p0_
dxy58,1__

83 7-83 BGM on external speakers_
T1 SPEAKER No._
T2 SPEAKER No._
P0 = _
DXY13,4
ML2
*** print
t01,
	50,Speaker No.
	50,Speaker No._
t11,
	10,**0:disable  1:enable**_
p0 = _
ml2
dxy62,1__

84 7-84 Restriction table_
T0TABLE No.=_
T1 RESTRICTED CODE_
T2No.CODE_
@012,3
DXY1,6
HT8
ML10
*** print
t12,
	11,Restricted
	11, No. Code_
t20,
	4,Table
	4, No._
p0-_
ml20
ht10
%06,5
dxy14,4__

85 7-85 Emergency code overrides_
T0EMERGENCY CODE_
T1 No.  CODE_
P0--_
DXY3,5
ML10
*** print
t02,
	9,Emergency
	9,No.  Code_
p0--_
ml5
ht12
dxy11,4__

86 7-86 International call access number_
T1International call access No.=_
P0_
DXY2,5
*** print
t00,
	48,Number =_
p0_
dxy58,1__

87 7-87 Release time/Abandoned hold_
T1Release time =_
P0_
DXY2,5
*** print
t00,
	50,Time =_
t11,
	10,**0:not released  1:400-600mS loop on  2:20-90mS loop on**_
p0_
dxy58,1__

88 7-88 Intrusion tone for break-in_
T1Intrusion tone =_
P0_
DXY2,5
*** print
t00,
	50,Data =_
t11,
	10,**0:disable  1:enable**_
p0_
dxy58,1__

89 7-89 DTMF transmission_
T1  Class-_
T2  Class-
  Class-
  Class-
  Class-
  Class-_
P0 = _
DXY9,4
ML6
*** print
t01,
	10,**0:disable  1:enable**_
t10,
	9,Class #
	9,Class #
	9,Class #
	9,Class #
	9,Class #
	9,Class #_
p0 = _
ml6
dxy17,3__

90 7-90 Call abandonment time_
T1Call abandonment time =_
T2   Sec._
P0_
DXY2,5
*** print
t00,
	49,Timer =   Sec._
p0_
dxy58,1__

91 7-91 Hold alarm duration timer_
T1Hold alarm duration timer =_
T2     Sec._
P0_
DXY2,5
*** print
t00,
	49,Timer =     Sec._
p0_
dxy58,1__

92 7-92 Follow Me Xfer duration timer_
T1Duration timer =_
T2     Sec._
P0_
DXY2,5
*** print
t00,
	49,Timer =     Sec._
p0_
dxy58,1__

93 7-93 Grounding time specification_
T1 Timer =_
T2    x0.0165 Sec._
P0_
DXY2,5
*** print
t00,
	49,Timer =     x0.0165 Sec._
p0_
dxy58,1__

94 7-94 Ring inword alarm timer_
T1 Timer=_
T2     x10 Sec._
P0_
DXY2,5
*** print
t00,
	49,Timer =     x10 Sec._
p0_
dxy58,1__

_CLASS_MENU08
01 8-01 Line key access_
T0TEN_
T1No. L_
DXY2,5
HT7
ML10
*** print
t01,
	10,0:preselection   1:singleaccess on-hook dialing_
t12,
	9,TEN
	9,No. L_
p0-_
ht7
ml10
dxy11,5__

02 8-02 Idle trunk off-hook access_
T0TEN_
T1No. I_
DXY2,5
HT7
ML10
*** print
t01,
	10,**0:disable   1:enable**_
t12,
	9,TEN
	9,No. I_
p0-_
ht7
ml10
dxy11,5__

03 8-03 Incoming call off-hook access_
T0TEN_
T1No. I_
DXY2,5
HT7
ML10
*** print
t01,
	10,**0:disable   1:enable**_
t12,
	9,TEN
	9,No. I_
p0-_
ht7
ml10
dxy11,5__

04 8-04 Speed dial program telephone_
T0TEN_
T1No. S_
DXY2,5
HT7
ML10
*** print
t01,
	10,0:impossible   1:possible_
t12,
	9,TEN
	9,No. S_
p0-_
ht7
ml10
dxy11,5__

05 8-05 Dial touch tone_
T0TEN_
T1No. D_
DXY2,5
HT7
ML10
*** print
t01,
	10,**0:disable   1:enable**_
t12,
	9,TEN
	9,No. D_
p0-_
ht7
ml10
dxy11,5__

06 8-06 Busy (off-hook)signaling permission_
T0TEN_
T1No. B_
DXY2,5
HT7
ML10
*** print
t01,
	10,**0:disable   1:enable**_
t12,
	9,TEN
	9,No. B_
p0-_
ht7
ml10
dxy11,5__

07 8-07 Incoming unanswered alarm_
T0TEN_
T1No. I_
DXY2,5
HT7
ML10
*** print
t01,
	10,**0:disable   1:enable**_
t12,
	9,TEN
	9,No. I_
p0-_
ht7
ml10
dxy11,5__

08 8-08 HFAB verification tone_
T0TEN_
T1No. H_
DXY2,5
HT7
ML10
*** print
t01,
	10,**0:disable   1:enable**_
t12,
	9,TEN
	9,No. H_
p0-_
ht7
ml10
dxy11,5__

09 8-09 Long conversation warning_
T0TEN L_
DXY2,4
HT7
ML10
*** print
t01,
	10,**0:disable   1:enable**_
t12,
	9,TEN
	9,No. L_
p0-_
ht7
ml10
dxy11,5__

11 8-11 Trk to Trk Xfer permission_
T0TEN_
T1No. T_
DXY2,5
HT7
ML10
*** print
t01,
	10,**0:disable   1:enable**_
t12,
	9,TEN
	9,No. T_
p0-_
ht7
ml10
dxy11,5__

12 8-12 Zone page verification tone_
T0TEN_
T1No. T_
DXY2,5
HT7
ML10
*** print
t01,
	10,**0:disable   1:enable**_
t12,
	9,TEN
	9,No. T_
p0-_
ht7
ml10
dxy11,5__

13 8-13 Break-in permitted station_
T0TEN_
T1No. B_
DXY2,5
HT7
ML10
*** print
t01,
	10,**0:disable   1:enable**_
t12,
	9,TEN
	9,No. B_
p0-_
ht7
ml10
dxy11,5__

14 8-14 Break-in interrupted station assign_
T0TEN_
T1No. B_
DXY2,5
HT7
ML10
*** print
t01,
	10,0:not interrupted   1:interrupted_
t12,
	9,TEN
	9,No. B_
p0-_
ht7
ml10
dxy11,5__

16 8-16 DND on intercom_
T0TEN_
T1No. D_
DXY2,5
HT7
ML10
*** print
t01,
	10,**0:disable   1:enable**_
t12,
	9,TEN
	9,No. D_
p0-_
ht7
ml10
dxy11,5__

17 8-17 DND on trunk_
T0TEN_
T1No. D_
DXY2,5
HT7
ML10
*** print
t01,
	10,**0:disable   1:enable**_
t12,
	9,TEN
	9,No. D_
p0-_
ht7
ml10
dxy11,5__

18 8-18 Intercom signal(ring/voice)_
T0TEN_
T1No. S_
DXY2,5
HT7
ML10
*** print
t01,
	10,0:ringing call   1:voice announced call_
t12,
	9,TEN
	9,No. S_
p0-_
ht7
ml10
dxy11,5__

20 8-20 Voice over_
T0TEN_
T1No. S_
DXY2,5
HT7
ML10
*** print
t01,
	10,**0:disable  1:enable**_
t12,
	9,TEN
	9,No. V_
p0-_
ht7
ml10
dxy11,5__

21 8-21 Station voice message permission_
T0TEN_
T1No. P_
DXY2,5
HT7
ML10
*** print
t01,
	10,**0:disable  1:enable**_
t12,
	9,TEN
	9,No. P_
p0-_
ht7
ml10
dxy11,5__

22 8-22 Speaker phone assign_
T0TEN_
T1No. S_
DXY2,5
HT7
ML10
*** print
t12,
	9,TEN
	9,No. S_
p0-_
ht7
ml10
dxy11,4__

23 8-23 Paging permitted telephones_
T0TEN_
T1No. P_
DXY2,5
HT7
ML10
*** print
t01,
	10,**0:disable  1:enable**_
t12,
	9,TEN
	9,No. P_
p0-_
ht7
ml10
dxy11,5__

24 8-24 Follow Me Xfer permitted_
T0TEN_
T1No. F_
DXY2,5
HT7
ML10
*** print
t01,
	10,**0:disable   1:enable**_
t12,
	9,TEN
	9,No. F_
p0-_
ht7
ml10
dxy11,5__

26 8-26 Voice announce call permisson_
T0TEN_
T1No. V_
DXY2,5
HT7
ML10
*** print
t01,
	10,**0:disable   1:enable**_
t12,
	9,TEN
	9,No. V_
p0-_
ht7
ml10
dxy11,5__

27 8-27 DND override_
T0TEN_
T1No. D_
DXY2,5
HT7
ML10
*** print
t01,
	10,0:not permited   1:permited_
t12,
	9,TEN
	9,No. D_
p0-_
ht7
ml10
dxy11,5__

28 8-28 Absence setting permit_
T0TEN_
T1No. A_
DXY2,5
HT7
ML10
*** print
t01,
	10,0:not permited   1:permited_
t12,
	9,TEN
	9,No. A_
p0-_
ht7
ml10
dxy11,5__

29 8-29 Trunk handsfree call permit_
T0TEN_
T1No. T_
DXY2,5
HT7
ML10
*** print
t01,
	10,0:not permited   1:permited_
t12,
	9,TEN
	9,No. T_
p0-_
ht7
ml10
dxy11,5__

30 8-30 Instantaneous incoming permit_
T0TEN_
T1No. I_
DXY2,5
HT7
ML10
*** print
t02,
	10,0:not instantaneous   1:instantaneous CR mode
	10,2:instantaneous /CR mode_
t12,
	9,TEN
	9,No. I_
p0-_
ht7
ml10
dxy11,6__

31 8-31 Call origination access priority_
T0TEN_
T1No. C_
DXY2,5
HT7
ML10
*** print
t03,
	10,0:extension line
	10,1:loop access trk/individual trk/extension line
	10,2:individual trk/loop access_
t12,
	9,TEN
	9,No. C_
p0-_
ht7
ml10
dxy11,7__

32 8-32 Incoming call access priority_
T0TEN_
T1No. I_
DXY2,5
HT7
ML10
*** print
t02,
	10,0:trunk call access priority
	10,1:intercom call access priority_
t12,
	9,TEN
	9,No. I_
p0-_
ht7
ml10
dxy11,6__

33 8-33 Trunk incoming call tone(D/N)_
T0TEN_
T1No. DN_
DXY2,5
HT7
ML10
*** print
t01,
	10,D=Day time   N=Night time_
t12,
	9,TEN
	9,No. DN_
p0-_
ht7
ml10
dxy11,5__

34 8-34 Intercom incoming call tone(D/N)_
T0TEN_
T1No. DN_
DXY2,5
HT7
ML10
*** print
t01,
	10,D=Day time   N=Night time_
t12,
	9,TEN
	9,No. DN_
p0-_
ht7
ml10
dxy11,5__

35 8-35 Long cycle ringing_
T0TEN_
T1No. L_
DXY2,5
HT7
ML10
*** print
t05,
	9,0:Standard cycle ringing
	9,1:Long cycle ringing on CO calls
	9,2:Long cycle ringing on ICM calls
	9,3:Long cycle ringing on CO/ICM calls
	9,4:1sec.on/2sec.off ringing on CO/ICM calls for single line tel._
t12,
	9,TEN
	9,No. L_
p0-_
ht6
ml10
dxy11,9_

36 8-36 Preset off-hook access(hot line)_
T0TEN  HL_
T1 No. No._
DXY3,5
HT9
ML10
*** print
t01,
	10,HL(Hot Line)=00:unassigned_
t12,
	8,TEN  HL
	8, No. No._
p0-_
ht7
ml10
dxy11,5__

38 8-38 Headset connection_
T0TEN_
T1No. H_
DXY2,5
HT7
ML10
*** print
t01,
	10,0:not connected  1:connected_
t12,
	9,TEN
	9,No. H_
p0-_
ht7
ml10
dxy11,5__

40 8-40 Service Observation_
T0TEN_
T1No. S_
DXY2,5
HT7
ML10
*** print
t01,
	10,**0:disable   1:enable**_
t12,
	9,TEN
	9,No. S_
p0-_
ht7
ml10
dxy11,5__

41 8-41 Mode selection of Receiver level_
T0TEN M_
DXY2,4
HT7
ML10
*** print
t03,
	10,0:return to the initial level
	10,1:adjust volume controller without releasing
	10,2:only adjust volume controller_
t12,
	9,TEN
	9,No. M_
p0-_
ht7
ml10
dxy11,7__

42 8-42 Dial blocking permitted station_
T0TEN_
T1No. D_
DXY2,5
HT7
ML10
*** print
t01,
	10,0:disable   1:enable_
t12,
	9,TEN
	9,No. D_
p0-_
ht7
ml10
dxy11,5__

_CLASS_MENU09
01 9-01 Line number indication_
T0LINE TELEPHONE_
T1 No.   No._
DXY3,5
HT17
ML10
*** print
t02,
	9,Line Telephone
	9, No.   No._
p0-_
ht20
dxy12,4__

02 9-02 Private line assignment_
T0LINE_
T1 No. P_
DXY3,5
HT12
ML12
*** print
t01,
	10,0:common  1:executive private_
t12,
	8,Line
	8, No. P_
p0-_
ht7
dxy11,5__

03 9-03 Trk to Trk forward(night)_
T0LINE_
T1 No. T_
DXY3,5
HT12
ML12
*** print
t01,
	10,0:non  1:voice message device  2:trunk forward_
t12,
	8,Line
	8, No. T_
p0-_
ht7
dxy11,5__

04 9-04 Trk to Trk transfer permission_
T0 LINE No.=_
T2LINE_
T3 No. T_
@012,3
DXY3,7
HT7
ML12
*** print
t01,
	10,**0:disable  1:enable**_
t12,
	8,Line
	8, No. T_
t20,
	4,LINE_
p0-_
ht7
%06,5
dxy11,5__

05 9-05 Speech level for Trk to Trk_
T0LINE_
T1 No. S_
DXY3,5
HT10
ML12
*** print
t01,
	10,0:2dB up  1:4dB up  2:6dB up_
t12,
	8,Line
	8, No. S_
p0-_
ht10
dxy11,5__

08 9-08 Camp-on permission_
T0LINE_
T1 No. C_
DXY3,5
HT10
ML12
*** print
t01,
	10,**0:disable  1:enable**_
t12,
	8,Line
	8, No. C_
p0-_
ht10
dxy11,5__

09 9-09 External speaker incoming audible_
T0      EXTERNAL_
T1      SPEAKER_
T2 LINE  #1 #2_
T3  No.  DN DN_
P0--_
DXY4,7
HT12
ML12
*** print
t01,
	10,D=Day time   N=Night time  #1=First SP  #2=Second SP
	10,0:not audible   1:audible_
t12,
	13,External
	13,Speaker
	8,Line  #1 #2
	8, No.  DN DN_
p0--_
p1-_
ht12
dxy11,8__

10 9-10 Hook pulse for tandem_
T0LINE_
T1 No. H_
DXY3,5
HT10
ML12
*** print
t01,
	10,**0:disable  1:enable**_
t12,
	8,Line
	8, No. H_
p0-_
ht10
dxy11,5__

20 9-20 Trk to Trk setup phone_
T0LINE TEN_
T1 No. No._
DXY3,5
HT10
ML12
*** print
t12,
	8,Line TEN
	8, No. No._
p0-_
ht10
dxy11,4__

21 9-21 Voice mail connection_
T0LINE TEN_
T1 No. No._
DXY3,5
HT10
ML12
*** print
t12,
	8,Line TEN
	8, No. No._
p0-_
ht10
dxy11,4__

22 9-22 Non-Private CO line_
T0LINE_
T1 No. P_
DXY3,5
HT10
ML12
*** print
t01,
	10,0:ordinary CO line  1:non-private CO line_
t12,
	8,Line
	8, No. P_
p0-_
ht10
dxy11,5__

_CLASS_MENU10
0310-03 Paging group assignments_
T0GROUP No.=_
T1TEN P_
@012,3
DXY2,5
HT7
ML10
*** print
t01,
	10,0:out of the group  1:in the group_
t12,
	11,TEN
	11,No. G_
t20,
	4,GROUP
	4, No._
%06,6
p0-_
ht7
dxy13,5__

0410-04 Doorphone ringing station assignment_
T0DOORPHONE No.=_
T1TEN_
T2No. D_
@016,3
DXY2,6
HT7
ML10
*** print
t01,
	10,0:not audible  1:audible_
t12,
	11,TEN
	11,No. D_
t20,
	4,DOOR-
	4,PHONE
	4, No._
%06,7
p0-_
ht7
dxy13,5__

_CLASS_MENU11
01 11-01 Common speed dial_
T0 Page : _
T2 SPEED DIAL_
T3No. TELEPHONE No.        NAME_
@09,3
DXY2,7
ML10
*** print
dxy8,3
ml45
t01,
	6,No. telephone No.	9,Name_
ht37__

02 11-02 Personal speed dialing_
T0 TEN No : _
T2 SPEED DIAL_
T3No. TELEPHONE No._
DXY2,7
ML10
@011,3
***** print
dxy11,4
%06,4
ht30
ml15
t12,

	8, No. telephone No.
_
t20,	4,TEN__

03 11-03 One touch(flexible)_
T0 TEN No : _
T2 ONE TOUCH DIAL_
T3 F. TELEPHONE No._
ML12
@011,3
***** print
dxy11,4
ht30
ml16
%06,4
t12,

	8, No. telephone No.
_
t20,	4,TEN__

04 11-04 DSS/DLS One touch(flexible)_
T0 DSS/DLS No : _
T1 ONE TOUCH DIAL_
T2 F. TELEPHONE No._
ML14
DXY2,6
@015,3
***** print
dxy15,4
%06,4
ht30
ml17
t12,

	13,telephone No.
_
t20,	3,DSS/DLS No.__

05 11-05 One touch(C/O Line)_
T0 TEN No : _
T2 ONE TOUCH DIAL(C/O)_
T3 F. TELEPHONE No._
DXY2,7
ML12
@011,3
***** print
dxy11,4
ht30
ml16
%06,4
t12,

	8, No. telephone No.
_
t20,	4,TEN__

06 11-06 DSS/DLS One touch(C/O Line)_
T0 DSS/DLS No : _
T1 ONE TOUCH DIAL(C/O)_
T2 F. TELEPHONE No._
ML14
DXY2,6
@015,3
***** print
dxy15,4
ht30
ml17
%06,4
t12,

	13,telephone No.
_
t20,	3,DSS/DLS No.__

07 11-07 One touch(Intercom)_
T0 TEN No : _
T2 ONE TOUCH DIAL(ICM)_
T3 F. TELEPHONE No._
DXY2,7
ML12
@011,3
***** print
dxy11,4
ht30
ml16
%06,4
t12,

	13,telephone No.
_
t20,	4,TEN__

08 11-08 DSS/DLS One touch(Intercom)_
T0 DSS/DLS No : _
T1 ONE TOUCH DIAL(C/O)_
T2 F. TELEPHONE No._
ML14
DXY2,6
@015,3
***** print
dxy15,4
ht30
ml17
%06,4
t12,

	13,telephone No.
_
t20,	3,DSS/DLS No.__

09 11-09 Name(Intercom)_
T0 Page : _
T1TEN  ICM_
T2 No. No.  Name_
ML10
HT20
P0-   -_
DXY3,6
@09,3
***** print
dxy11,3
p0-   -_
ht21
t11,
	9,TEN ICM Name__

10 11-10 Name(Intercom group)_
T0INTERCOM_
T1 G   No.  Name_
HT20
P0--   -_
ML10
DXY2,5
***** print
dxy11,3
p0--   -_
ht21
ml10
t11,
	10,No. ICM Name__

12 11-12 Name(Line)_
T0LINE TELEPHON_
T1 No.    No.       Name_
P0-            -_
HT30
ML12
DXY2,5
***** print
dxy11,3
p0-            -_
ht28
ml12
t11,
	8,LEN  TELEPHONE     Name__
_
