			Fahrenheit Windows Installer
			      "Standard" Drivers

1. Insert a blank floppy into your floppy drive.

2. Copy these files to that floppy.

		(i.e. copy *.* a:)

3. Type FINSTALL from the floppy drive.

	A:		<ENTER>
	FINSTALL 	<ENTER>

4. Installation complete.