	     PIPELINE 64 WINDOWS95 UTILITY 1.01 INSTALLATION
	     -----------------------------------------------

    The Pipeline 64 Windows95 Utility 1.01 consists of 2 diskettes:
    
    The first diskette is contained in the file P64101D1.EXE.
    This first diskette contains the Windows95 driver with Direct 
    Draw support and OASIS 95 Utility.

    The second diskette is contained in the file P64101D2.EXE.
    This second diskette contains the MediaMatics MPEG Arcade for
    Windows 95.


    To make install diskettes:
    - Extract the archive file 9710_w95.EXE to the TEMP directory
      on your C: drive. This will produce the following files:  
      P64101D1.EXE, P64101D2.EXE and README.TXT (this file).
    - Label two blank formatted 1.44MB diskettes DISK1 and DISK 2.
    - Place the diskette labelled DISK 1 in your floppy drive.
    - Log (change) to the drive containing the blank floppy disk.
      (A: or B:)
    - On the command line type C:\TEMP\P64101D1 and press enter.
    - When the A: or B: prompt returns, place the diskette labelled 
      DISK 2 in your floppy drive.
    - On the command line type C:\TEMP\P64101D2 and press enter.
    - When the A: or B: prompt returns, creation of the install
      diskettes is complete.


    To install the Windows95 driver:

    - Make sure the system is using Standard VGA driver (to be sure,
      boot up Win95 in Safe Mode - see Windows 95 documentation)
    - From Start, select Settings - Control Panel
    - Select Display.  From the Display Properties, select Settings -
      Change Display Type - Change from Adapter Type - Have Disk
    - Select the correct path where the first diskette of the Pipeline
      64 Win95 Utility is
    - After the drivers have been copied over to the hard disk,
      follows the instruction on the screen to reboot the system.


    To install the OASIS 95 utility:

    - Run SETUP.EXE from the diskette labeled DISK 1 (first diskette)
    - Follow the instructions on the screen


    To install the MediaMatics Arcade:

    - Run SETUP.EXE from the diskette labeled DISK 2 (second diskette)
    - Follow the instructions on the screen

-- end of readme.txt --
