

                        ATTENTION

In order for the telesound system to work properly, the Sound Card mixer (volume) levels
must be high enough.

Make sure that your rear volume wheel (if exists) is high, and that all of the volumes in
your windows mixer program (or in the audio station program) are high (as high as you
can get without getting noises).

REMEMBER: In order for any volume change to apply, you must save the mixer after
the change.

To save the mixer, right after changing the values, go to the PHONE PAD, select the
mixer menu, and choose the "save mixer" option.

The mixer changes WILL NOT affect your normal work because after saving the mixer
you can reduce volumes again (not the rear wheel), and telesound will restore the
settings you defined only for phone operation.


MIXER CONTROL:
                To set mixer levels for the TeleSound System operation set the
levels in your Sound Card's mixer program and then press the save mixer button.

SERIAL PORT:
                If the wrong serial port is choosen , you might get a
ringing sound when you start the CONFIG program.

           *** END OF FILE ***

