The Amateur Radio Project - F.M., A.M. and S.S.B. transmitters

# F.M., A.M. and S.S.B. transmitters

### Question 24 of 24

Conventionally, in SSB transmission,

- i upper sideband would be used on the 20m band
- ii upper sideband would be used on the 40m band

1. i and ii are both true
2. i is true but ii is false
3. i is false but ii is true
4. i and ii are both false

1 | 2 | 3 | 4

Back |

page (tq1824)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd | Contact details