# C.W. transmitters and keying

### Explanation of question 2

The buffer amplifier of a transmitter will normally be operating in class

1. A
2. AB
3. B
4. C

The answer is :- 1 The buffer amplifier must present an even, light load oi~ the oscillator. For this reason, class A is used.

BACK

page (tq1702ex)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
Contact details