-----------------------------------------------------
Router IP Console version 3.3 (build 403) Readme File
(c) 2000-2001, Innerdive Solutions, LLC.
-----------------------------------------------------

This document provides late-breaking or other information that supplements the Router IP Console version 3.3 documentation.

--------
CONTENTS
--------

1. PRODUCT DESCRIPTION

2. NEW FEATURES

3. INSTALLATION NOTES
   3.1 Before You Run Setup
       3.1.1 Hardware Requirements
       3.1.2 Software Requirements

4. TECHNICAL SUPPORT
   4.1 Visiting the Innerdive's Web Site


----------------------
1. PRODUCT DESCRIPTION
----------------------

Router IP Console is a SNMP based tool for the management and control of SNMP devises (such as routers, repeaters etc). It can understand Cisco specific routers, and can also raise an alarm on critical situations such as a router's CPU overload, router's memory exhausted, or an interface going to a down state. You can have alerts sent by e-mail. Also you can examine a history of values of any displayed SNMP parameter and view it graph.


------------------------------------------
2. NEW FEATURES IN ROUTER IP CONSOLE 3.3
------------------------------------------

This release of Router IP Console adds several exciting features to give the user more power and control on their routers. New features include:
* Now you can use SNMP Trap Service on the Windows NT 4.0 and Windows 2000.
* New parameter added to the alarm templates - interface description.
* The alarm sound now can play continously until operator press the "Confirm" button. 
* You can setup a timeout value for the internal e-mail sender.
* Internal SNMP library was upgraded - now RIC is more (and more) stable.
* For the Cisco routers a chassis ID was displayed.

---------------------
3. INSTALLATION NOTES
---------------------

3.1 Before You Run Setup

Before you install Router IP Console, make sure that your computer meet the minimum hardware and software requirements.

3.1.1 Hardware Requirements

To install Router IP Console, you must meet certain hardware requirements, which include:

· Pentium(r) x86-compatible computer.
· Minimum 10 MB free space on hard disk.
· Minimum 32 MB RAM.
 
3.1.2 Software Requirements

Before you install Router IP Console, your computer must meet the following software requirements:

· Windows(r) 95/98/ME or NT4(SP3+)/2000 
· Microsoft Internet Explorer(r) 4.01 or higher 
· WinSock2 update installed (required for Windows(r) 95 only).

--------------------
4. TECHNICAL SUPPORT
--------------------

4.1 Visiting the Innerdive Solutions, LLC. Web Site

You can visit the Innerdive's Router IP Console Home Page on the World Wide Web for documentation updates and information about other related products. The address is http://www.innerdive.com/
