;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU
;UU                                                                        UU
;UU  Miles Design Audio Interface Library                                  UU
;UU                                                                        UU
;UU  Sound driver installation message file                                UU
;UU                                                                        UU
;UU  Default selection criteria/examples:                                  UU
;UU                                                                        UU
;UU    .E BLASTER ........ Environment var 'BLASTER' must be present       UU
;UU    .C MVSOUND ........ CONFIG.SYS must contain 'MVSOUND' string        UU
;UU    .A AWEUTIL ........ AUTOEXEC.BAT must contain 'AWEUTIL' string      UU
;UU                                                                        UU
;UU    .NE BLASTER ....... Environment var 'BLASTER' must NOT be present   UU
;UU    .NC MVSOUND ....... CONFIG.SYS must NOT contain 'MVSOUND' string    UU
;UU    .NA AWEUTIL ....... AUTOEXEC.BAT must NOT contain 'AWEUTIL' string  UU
;UU    .ND  .............. Entry cannot be selected as default             UU
;UU                                                                        UU
;UU    .T1  .............. Optional BLASTER Tn, if present, must be 1|3    UU
;UU    .T2  .............. Mandatory BLASTER Tn must be 2|4|5              UU
;UU    .T3  .............. Mandatory BLASTER Tn must be >=6                UU
;UU                                                                        UU
;UU  I/O default derivation:                                               UU
;UU                                                                        UU
;UU    .IOB .............. Derive I/O defaults from BLASTER variable       UU
;UU    .IOD .............. I/O defaults = first driver default entry       UU
;UU    .ION .............. Do not allow manual I/O configuration at all    UU
;UU                                                                        UU
;UU    .IOA .............. Use I/O address only (must appear at end)       UU
;UU    .IOL .............. Suppress high-DMA prompt (must appear at end)   UU
;UU                                                                        UU
;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[sblaster.dig]

;
;Selected by default if BLASTER variable is of type T1 or T3 (or no T 
;specifier), and no other "clone" variable exists (ULTRASND, MVSOUND, etc.)
;
;Default I/O parms from BLASTER
;

.E BLASTER
.T1
.NE ULTRASND
.NE SNDSCAPE
.NC MVSOUND.SYS
.IOB
.IOL

.SPECIAL_TEXT
Si vous utilisez un adaptateur Sound Blaster, Sound Galaxy, Thunderboard 
ou Pro Audio Spectrum, choisissez ce pilote. D'autres cartes son qui ne 
sont pas directement support‚es peuvent fonctionner avec ce pilote, si 
elles assurent une compatibilit‚ mat‚rielle avec Sound Blaster sans 
pilote d'‚mulation ni programme r‚sident (TSR).
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[sbpro.dig]

;
;Selected by default if BLASTER variable is of type T2, T4, or T5
;and no other "clone" variable exists
;
;Default I/O parms from BLASTER
;

.E BLASTER
.T2
.NE ULTRASND
.NE SNDSCAPE
.NC MVSOUND.SYS
.IOB
.IOL

.SPECIAL_TEXT
Ce pilote supporte toutes les versions de Sound Blaster Pro et les 
adaptateurs compatibles. L'utilisation avec Sound Blaster 16 ou AWE32 
est d‚conseill‚e. 
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[sb16.dig]

;
;Selected by default if BLASTER variable is of type T6
;
;Default I/O parms from BLASTER (I/O address only)
;

.E BLASTER
.T3
.NE ULTRASND
.NE SNDSCAPE
.NC MVSOUND.SYS
.IOB
.IOA

.SPECIAL_TEXT
Pour obtenir un son num‚rique de haute qualit‚ avec un adaptateur Sound 
Blaster 16 ou AWE32, choisissez ce pilote.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[rap10.dig]

;
;Never selected by default
;
;Default I/O parms from driver
;

.ND
.IOD

.HIGH_DMA_PAIRS

.SPECIAL_TEXT
AVERTISSEMENT : Pendant l'auto-d‚tection de la carte Roland RAP-10, le 
pilote v‚rifie que la RAP-10 est pr‚sente … l'adresse E/S 320H ou 330H. 
Le pilote NE VERIFIE ni le canal DMA ni les paramŠtres IRQ de la carte. 
Si votre carte RAP-10 n'est pas configur‚e en IRQ 9, ou si les canaux DMA 
5 et 6 sont d‚j… utilis‚s par une autre carte, choisissez l'option 
"Passer l'auto-d‚tection et configurer le pilote manuellement" du men 
suivant, et entrez les paramŠtres E/S correspondant … votre carte. Sinon, 
votre systŠme peut ne pas fonctionner ou des gr‚sillements se produire 
lors de la diffusion des sons.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[proaudio.dig]

;
;Selected by default if CONFIG.SYS contains MVSOUND string
;
;No configuration allowed
;

.C MVSOUND.SYS
.ION

.SPECIAL_TEXT
Ce pilote assure un son num‚rique st‚r‚o avec toutes les versions de 
Media Vision Pro Audio Spectrum. Si vous rencontrez des difficult‚s, 
choisissez plut“t le pilote compatible Sound Blaster. L'utilitaire 
MVSOUND.SYS de Media Vision doit ˆtre charg‚ en m‚moire, faute de quoi 
votre carte ne sera pas d‚tect‚e.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[ultra.dig]

;
;Selected by default if environment contains ULTRASND variable
;
;Default I/O parms from driver
;

.E ULTRASND
.IOD

.SPECIAL_TEXT
Lors de l'utilisation de ce pilote, assurez-vous qu'aucun utilitaire 
GRAVIS n'est activ‚ (par exemple, SBOS, UltraMIDI, Mega-Em...). Vous 
devez poss‚der au moins la version 2.0 du logiciel systŠme UltraSound.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[jammer.dig]

;
;Never selected by default
;
;Default I/O parms from driver
;

.ND
.IOD

.NAME
New Media Corporation WaveJammer(TM) Digital Audio

.SPECIAL_TEXT
La carte WaveJammer de New Media Corporation assure un son de haute 
qualit‚ pour portables ‚quip‚s de cartes PCMCIA. Choisissez le pilote Ad 
Lib (R) Music Synthesizer Card pour restituer les s‚quences musicales FM 
avec la carte WaveJammer.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[sndscape.dig]

;
;Selected by default if environment contains SNDSCAPE variable
;
;Default I/O parms from driver
;

.E SNDSCAPE
.IOD

.NAME
Ensoniq SoundScape(TM) Digital Audio

.SPECIAL_TEXT
Choisissez ce pilote si vous avez une carte son Ensoniq SoundScape (TM) 
ou compatible
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[sndsys.dig]

;
;Never selected by default
;
;Default I/O parms from driver
;

.ND
.IOD

.NAME
Microsoft(R) Windows(TM) Sound System or 100% compatible

.SPECIAL_TEXT
Choisissez ce pilote si votre carte est compatible Microsoft Windows 
Sound System.
Si le canal DMA 1 est d‚j… utilis‚ par une autre carte, choisissez un 
autre canal DMA en s‚lectionnant l'option "Passer l'auto-d‚tection et 
configurer le pilote manuellement". Si vous fonctionnez sous Windows 95 
ou utilisez un autre systŠme Plug & Play, consultez le gestionnaire de 
p‚riph‚riques pour connaŒtre l'adresse E/S utilis‚e.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[adrv688.dig]

;
;Never selected by default
;
;Default I/O parms from driver
;

.ND
.IOD

.NAME
ESS Technology ES688 Digital Audio

.SPECIAL_TEXT
Ce pilote supporte les systŠmes ‚quip‚s d'un jeu de puce ES688 de ESS 
Technology.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[mpu401.mdi]

;
;Never selected by default
;
;Default I/O parms from driver
;

.ND
.IOD

.SPECIAL_TEXT
La plupart des synth‚tiseurs General MIDI supportent la norme d'interface 
mat‚rielle Roland MPU-401 MIDI parmi lesquels Roland Sound Canvas Rap-10 
et compatibles ainsi que les cartes-fille additionnelles des Sound 
Blaster 16.Les p‚riph‚riques MPU-401 offrent en g‚n‚ral les meilleurs 
performances et rendus sonores  les utilisateurs de contr“leurs Adaptec 
SCSI peuvent choisir l'option "Passer l'auto-d‚tection et configurer le 
pilote manuellement" du menu suivant pour r‚duire les probabilit‚s de 
problŠmes de d‚tection de la MPU-401.Si vous avez une Creative Labs 
AWE-32 choisissez plut“t "Creative Labs AWE-32 (TM) General MIDI".
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[sndscape.mdi]

;
;Selected by default if environment contains SNDSCAPE variable
;
;Default I/O parms from driver
;

.E SNDSCAPE
.IOD

.NAME
Ensoniq SoundScape(TM) General MIDI

.SPECIAL_TEXT
Choisissez ce pilote si vous avez une carte son Ensoniq SoundScape (TM) 
ou compatible.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[ultra.mdi]

;
;Selected by default if environment contains ULTRASND variable
;
;Default I/O parms from driver
;

.E ULTRASND
.IOD

.SPECIAL_TEXT
Lors de l'utilisation de ce pilote, assurez-vous qu'aucun utilitaire 
GRAVIS n'est activ‚ (par exemple, SBOS, UltraMIDI, Mega-Em...). Vous 
devez poss‚der au moins la version 2.0 du logiciel systŠme UltraSound.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[sbawe32.mdi]

;
;Selected by default if AUTOEXEC contains AWEUTIL string
;
;Default I/O parms from driver
;
.A AWEUTIL
.IOD

.NAME
Creative Labs AWE-32(TM) General MIDI

.SPECIAL_TEXT
Utilis‚ avec la carte Creative Labs AWE-32, ce pilote offre une synthŠse 
musicale General MIDI … plusieurs ondes. Pour obtenir un son num‚rique, 
choisissez le pilote "Creative Labs Sound Blaster 16 ou AWE32".
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[sblaster.mdi]

;
;Selected by default if BLASTER variable is of type T1 or T3 (or no T 
;specifier), and no other "clone" variable exists (ULTRASND, MVSOUND, etc.)
;
;Default I/O parms from BLASTER (A only)
;

.E BLASTER
.T1
.NE ULTRASND
.NE SNDSCAPE
.NC MVSOUND.SYS
.IOB
.IOA

.SPECIAL_TEXT
Ce pilote peut ˆtre utilis‚ avec n'importe quelle carte de synth‚tiseur 
musical dont la compatibilit‚ FM Sound Blaster ne d‚pend pas de 
programmes r‚sidents. Les utilisateurs de cartes General MIDI plus 
perfectionn‚es ne doivent choisir le pilote Sound Blaster que si des 
difficult‚s se produisent lors de l'utilisation du pilote de la carte 
General MIDI, l'ancien jeu de puce Sound Blaster OPL-2 n'assurant pas la 
qualit‚ sonore offerte par de plus r‚cents p‚riph‚riques
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[sbpro2.mdi]

;
;Selected by default if BLASTER variable is of type T6 or >, and AUTOEXEC does
;not contain AWEUTIL string
;
;Default I/O parms from BLASTER (A only)
;

.E BLASTER
.T3
.NE ULTRASND
.NE SNDSCAPE
.NC MVSOUND.SYS
.NA AWEUTIL
.IOB
.IOA

.NAME
Creative Labs Sound Blaster(TM) 16

.SPECIAL_TEXT
Ce pilote est con‡u pour fonctionner avec les adaptateurs Sound Blaster 
16 qui ne sont pas ‚quip‚s de cartes-fille General MIDI comme la Wave 
Blaster.
Bien que l'AWE-32 puisse ‚galement ˆtre support‚e par le pilote Sound 
Blaster 16, ses utilisateurs doivent choisir le pilote "Creative Labs 
AWE-32 (TM) General MIDI" pour un rendu sonore optimal.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[sbpro2.mdi]

;
;Selected by default if BLASTER variable is of type T2, T4, or T5,
;no other "clone" variable exists, and inp(388) == 0x00
;
;Default I/O parms from BLASTER (A only)
;

.E BLASTER
.T2
.NE ULTRASND
.NE SNDSCAPE
.NC MVSOUND.SYS
.IOB
.IOA

.SPECIAL_TEXT
Si votre Sound Blaster Pro est un modŠle "courant" ‚quip‚ du synth‚tiseur 
Yamaha OPL-3, ou si la qualit‚ de la musique diffus‚e n'est pas 
satisfaisante lors de l'utilisation d'un autre pilote Sound Blaster Pro, 
choisissez cette option.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[sbpro1.mdi]

;
;Selected by default if BLASTER variable is of type T2, T4, or T5,
;no other "clone" variable exists, and inp(388) == 0x06
;
;Default I/O parms from BLASTER (A only)
;

.E BLASTER
.T2
.NE ULTRASND
.NE SNDSCAPE
.NC MVSOUND.SYS
.IOB
.IOA

.SPECIAL_TEXT
Ce pilote permet aux utilisateurs des versions pr‚c‚dentes de Sound 
Blaster Pro de b‚n‚ficier d'une musique st‚r‚o FM avec 18 formes d'onde 
et deux op‚rateurs. Cependant, la plupart des cartes son Sound Blaster 
et compatibles, y compris la Sound Blaster 16, ont recours … un jeu de 
puce plus puissant : le OPL-3. Avec ces derniŠres cartes, choisissez 
plut“t le pilote "Creative Labs Sound Blaster Pro (TM) (nouvelle 
version).
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[pas.mdi]

;
;Selected by default if MVSOUND exists in CONFIG.SYS, and inp(388) == 0x06
;
;No configuration allowed
;

.C MVSOUND.SYS
.ION

.SPECIAL_TEXT
Seuls les utilisateurs des premiŠres cartes Pro Audio Spectrum de Media 
Vision doivent choisir ce pilote. L'utilitaire MVSOUND.SYS de Media 
Vision doit ˆtre charg‚ en m‚moire, faute de quoi la carte ne sera pas 
d‚tect‚e.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[pasplus.mdi]

;
;Selected by default if MVSOUND exists in CONFIG.SYS, and inp(388) == 0x00
;
;No configuration allowed
;

.C MVSOUND.SYS
.ION

.SPECIAL_TEXT
Les utilisateurs des cartes Pro Audio Spectrum Plus et Pro Audio Spectrum 
16 de Media Vision doivent choisir ce pilote. L'utilitaire MVSOUND.SYS de 
Media Vision doit ˆtre charg‚ en m‚moire, faute de quoi la carte ne sera 
pas d‚tect‚e.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[adlibg.mdi]

;
;Selected by default if GOLD variable exists in AUTOEXEC.BAT
;
;Default I/O parms from driver  
;

.E GOLD
.IOD

.SPECIAL_TEXT
Ce pilote supporte la carte Ad Lib Gold Music Synthesizer en mode FM 
quatre op‚rateurs
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[adlib.mdi]

.ND
.ION

.SPECIAL_TEXT
Ce pilote peut ˆtre utilis‚ avec n'importe quelle carte de synth‚tiseur 
musical FM compatible Ad Lib qui ne d‚pende pas de programmes r‚sidents 
pour la compatibilit‚ FM Ad Lib. Les utilisateurs de cartes General MIDI 
plus perfectionn‚es ne doivent choisir le pilote Ad Lib que si des 
difficult‚s se produisent lors de l'utilisation du pilote de la carte 
General MIDI, l'ancien jeu de puce Ad Lib OPL-2 n'assurant pas la qualit‚ 
sonore offerte par de plus r‚cents p‚riph‚riques.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU


[opl3.mdi]

;
;Never selected by default
;
;No configuration -- always at $388
;

.ND
.ION

.NAME
ESS Technology ES688 FM Audio

.SPECIAL_TEXT
Ce pilote supporte les systŠmes ‚quip‚s d'un jeu de puce ES688 de ESS 
Technology.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[esfm.mdi]

;
;Never selected by default
;
;Configuration from driver
;

.ND
.IOD

.NAME
ESS Technology ES1688, ES1788, ES1888 Enhanced FM Audio

.SPECIAL_TEXT
Ce pilote supporte les systŠmes ‚quip‚s d'un jeu de puce ES1688, ES1788 
ou ES1888 de ESS Technology. Ce pilote permet d'obtenir des performances 
FM musicales accrues. Si vous rencontrez des problŠmes, choisissez plut“t 
le pilote "ESS Technology ES688 FM Audio".
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[opl3.mdi]

;
;Never selected by default
;
;No configuration -- always at $388
;

.ND
.ION

.SPECIAL_TEXT
Ce pilote est destin‚ … tous les synth‚tiseurs musicaux FM Yamaha OPL-3, 
y compris ceux qui ne sont support‚s par aucun pilote de cette liste.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[mt32mpu.mdi]

;
;Never selected by default
;
;Default I/O parms from driver
;

.ND
.IOD

.SPECIAL_TEXT
Bien que la Roland MT-32 ne soit pas compatible General MIDI, elle 
utilise la norme d'interface mat‚rielle MPU-401 pour communiquer avec les 
applications. Les d‚tenteurs d'une carte MT-32 utilisant les contr“leurs 
Adaptec SCSI peuvent choisir l'option "Passer l'auto-d‚tection et 
configurer le pilote manuellement" du menu suivant pour r‚duire les 
probabilit‚s de problŠmes de d‚tection de la MPU-401.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[tandy.mdi]

;
;Never selected by default
;
;No configuration allowed
;

.ND
.ION

.SPECIAL_TEXT
Ce pilote fournit un support musical … trois formes d'ondes compatible 
Tandy 1000.
.END_SPECIAL_TEXT

;UUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUUU

[pcspkr.mdi]

;
;Never selected by default
;
;No configuration allowed
;

.ND
.ION

.SPECIAL_TEXT
Ce pilote, qui offre une synthŠse musicale de trŠs basse qualit‚, fournit 
un support musical (1 forme d'onde) pour haut parleur interne de PC IBM. 
.END_SPECIAL_TEXT

 
