;
;***********************************************************************\
;*                                                                      *
;*      Adapter Description File (ADF) for Allied Telesis               *
;*      Copyright (c) 1994 by Allied Telesis,  All rights reserved.     *
;*                                                                      *
;*      Version:        1.0             Original                        *
;*                                                                      *
;*                                                                      *
;*   for  AT1720T    POS ID = 6410                                      *
;*   for  AT1720BT   POS ID = 6413                                      *
;*   for  AT1720AT   POS ID = 6416                                      *
;*   for  AT1720FT   POS ID = 6419                                      *
;***********************************************************************/
;
AdapterId 06413h

AdapterName "Allied Telesis AT1720BT"

NumBytes 3


NamedItem
Prompt "Interrupt Request Number"
    choice "IRQ  3 "    pos[1]=00xxxxxxb pos[2]=x0xxxxxxb int 3
    choice "IRQ  4 "    pos[1]=01xxxxxxb pos[2]=x0xxxxxxb int 4
    choice "IRQ  5 "    pos[1]=10xxxxxxb pos[2]=x0xxxxxxb int 5
    choice "IRQ  9 "    pos[1]=11xxxxxxb pos[2]=x0xxxxxxb int 9
    choice "IRQ 10 "    pos[1]=00xxxxxxb pos[2]=x1xxxxxxb int 10
    choice "IRQ 11 "    pos[1]=01xxxxxxb pos[2]=x1xxxxxxb int 11
    choice "IRQ 12 "    pos[1]=10xxxxxxb pos[2]=x1xxxxxxb int 12
    choice "IRQ 15 "    pos[1]=11xxxxxxb pos[2]=x1xxxxxxb int 15
Help
    "Select the interrupt (IRQ) number to be used by the AT-1720 Adapter.
    If a conflict with another device exists, use the F5=Previous and
    F6=Next keys to change IRQ assignments (conflicts are indicated
    with an asterisk)."


NamedItem 
Prompt "Boot ROM Memory Address"
    choice "Disabled" pos[1]=xx111xxxb 
    choice "C4000"   pos[1]=xx000xxxb  mem 0c4000h-0c7ffffh
    choice "C8000"   pos[1]=xx001xxxb  mem 0c8000h-0cbffffh
    choice "CC000"   pos[1]=xx010xxxb  mem 0cc000h-0cfffffh
    choice "D0000"   pos[1]=xx011xxxb  mem 0d0000h-0d3ffffh
    choice "D4000"   pos[1]=xx100xxxb  mem 0d4000h-0d7ffffh
    choice "D8000"   pos[1]=xx101xxxb  mem 0d8000h-0dbffffh
    choice "DC000"   pos[1]=xx110xxxb  mem 0dc000h-0dfffffh
Help
    "If your AT-1720 contains a boot ROM, select the desired starting
    memory address for the ROM.
    If no boot ROM is installed, select the 'Disabled' choice.
    Use the F5=Previous and F6=Next keys to alter the selection."


NamedItem 
Prompt "I/O Port Addresses"
    choice "0x0400-0x04FF"   pos[1]=xxxxx000b  io 0400h-04FFh
    choice "0x1400-0x14FF"   pos[1]=xxxxx100b  io 1400h-14FFh 
    choice "0x2400-0x24FF"   pos[1]=xxxxx001b  io 2400h-24FFh 
    choice "0x3400-0x34FF"   pos[1]=xxxxx101b  io 3400h-34FFh 
    choice "0x4400-0x44FF"   pos[1]=xxxxx010b  io 4400h-44FFh
    choice "0x5400-0x54FF"   pos[1]=xxxxx110b  io 5400h-54FFh 
    choice "0x6400-0x64FF"   pos[1]=xxxxx011b  io 6400h-64FFh 
    choice "0x7400-0x74FF"   pos[1]=xxxxx111b  io 7400h-74FFh 
Help
    "Select the desired address range for the AT-1720's I/O ports.
    Use the F5=Previous and F6=Next keys to alter the selection."


NamedItem 
Prompt "Port Selection"
	choice "Auto Select"    pos[2]=xx00xx1xb  
	choice "Twisted Pair"   pos[2]=xx01xx0xb  
	choice "BNC"            pos[2]=xx11xx1xb  
Help
	"Select the desired port to be used by the AT-1720 adapter.
	'Twisted Pair' selects the 10BaseT (UTP/RJ45) port.
	'BNC' selects the 10Base2 (Thin Ethernet) port.
	'Auto Select' causes the AT-1720BT to automatically use the UTP port
	when a Twisted Pair cable is connected, or to use the BNC port if no
	cable if connected to the UTP port."


NamedItem 
Prompt "Twisted Pair Type"
	choice "100ohm UTP/STP"             pos[2]=xxxx01xxb  
	choice "150ohm STP"                 pos[2]=xxxx10xxb  
Help
	"Select the type of cabling to be used whenever the Twisted Pair port
	is active.  This option has no effect when the BNC port is active."
