             +++++++++++++++++++++++++++++++++              ++++
           ++++++++++++++++++++++++++++++++++++           +++++++
          +++++++++++++++++++++++++++++++++++++         ++++++++
          ++++++++++++++++++++++++++++++++++++        ++++++++
                                                   ++++++++
                                                  ++++++++
          +++++++++++++++++++++++++++           ++++++++
          +++++++++++++++++++++++++++++       ++++++++
           +++++++++++++++++++++++++++++     ++++++++
             +++++++++++++++++++++++++++     ++++++++
                                              ++++++++
                                               ++++++++
    ++++++++++++++++++++++++++++++++++++        ++++++++
   +++++++++++++++++++++++++++++++++++++         ++++++++
   ++++++++++++++++++++++++++++++++++++           ++++++++
    +++++++++++++++++++++++++++++++++               +++++

(C)Copyright 1993-1996 SysKonnect,
a business unit of Schneider & Koch & Co. Datensysteme GmbH.
All rights reserved
==========================================================================

SKFINT.TXT

Readme File for Windows NT NDIS3 Driver for SK-NET FDDI ISA Adapters
Subject: SKFINT.SYS NDIS3 Driver corresponding to the NDIS 3.0
	 Specification as delivered with Windows NT.



Version / Date / Author of this file: v2.10 / 28-Mar-1996 / SW
Version / Date / Author of the referred subject: v2.32 / 28-Mar-1996 / SW

This file contains
(1) Overview
(2) Required files
(3) Installation instructions
(4) Troubleshooting
(5) History

===============================================================================


(1) OVERVIEW
============

This README explains how to install the SKFINT.SYS driver on a
Windows NT workstation or server.
***


(2) REQUIRED FILES
==================

In a single directory

- OEMNADSK.HLP	Help file for SK-NET drivers

- OEMNADSK.DLL	Dialogs for SK-NET drivers

- OEMSETUP.INF	Setup script for the driver

- SKFINT.SYS	The driver
***


(3) INSTALLATION INSTRUCTIONS
=============================

NOTE:	On an EISA machine, the SK-NET FDDI ISA Adapter should be
	configured using the appropriate EISA configuration file.

Step 1: Start Windows NT.

Step 2: Open the CONTROL PANEL.

Step 3: Start NETWORK.

Step 4: Select ADD ADAPTER.

Step 5: Select <OTHER>.

Step 6: Type in the path to OEMSETUP.INF.

Step 7: Select the driver presented and select the appropriate configuration.
	Then choose OK and restart your system.
***


(4) TROUBLESHOOTING
===================

If you encounter problems using the SK-NET FDDI ISA Adapter, please
re-read carefully the instructions above and the documentation supplied
with the system.

If this does not help, please send us a description of the problems you have.

Also refer to your system log file (using the event viewer) and check
it for entries from SKFINT.

The last 5 DWORDs of the logging data are:

- Slot number (-1 if the adapter is not EISA-configured),

- Interrupt number,

- Dma channel,

- Base I/O port, and

- Vendor code (3 bytes) / adapter id (1 byte)

of the adapter that caused the error.

Follows a list of some events, possible reasons (may be incomplete)
and suggestions to fix your problem.

Event ID:	5001 -	Could not allocate the resources necessary
			for operation.
Reason(s):	Not enough RAM or pagefile too small.
Help:		...

---------------

Event ID:	5003 -	Could not find an adapter.
Reason(s):	Wrong slot or IO Port.
		Adapter physically not installed.
		System configuration information invalid.
Help:		Check slot/port settings.
		Check if adapter is physically present.
		Check system configuration.

---------------

Event ID:	5004 -	Could not connect to the interrupt number supplied.
Reason(s):	The selected interrupt is already in use.
Help:		Select free interrupt.

---------------

Event ID:	5007 -	Timed out during an operation.
Reason(s):	Wrong interrupt, DMA channel or base address.
		Cable not connected.
Help:		Start a driver under e.g. DOS (with the same resource usage)
		  and see if it works.
		Check cabling.

---------------

Event ID:	5009 -	Does not support the configuration supplied.
Reason(s):	Invalid IRQ or DMA given.
Help:		Check configuration.

---------------

Event ID:	5012 -	The I/O base address supplied does not match
			the jumpers on the adapter.
Reason(s):	Jumper settings and software configuration conflict.
Help:		Check jumper settings against software configuration.


If your special problem is not listed or the error persists, please
send us your system log file or at least the event id number and the
logging data (as dwords) of the entries made by SKFINT.
***


(5) HISTORY
===========

v2.00 Rev. A
  - OID_GEN_DRIVER_VERSION now returns NDIS version (3.00) instead of driver
    version.
  - On EISA and MCA machines the installation script inserts the keyword
    <BusNumber> into the registry.
  - More memory is used as receive buffer to reduce overflows.
v2.00 Rev. C
  - Fixed test for successful memory allocation.
v2.00 Rev. D
  - Runs on multiprocessor systems.
  - LINK_SPEED reporting corrected.
v2.01
  - Rejecting unsupported filters.
v2.10
  - Included EnhancedNonLlc mode.
  - Implemented limited promiscuous mode (receive all non-LLC frames).
    This may be disabled by setting <LimitPromiscuous> to 1 in the registry.
  - SBA/ESS added
  - Runs stable on multiprocessor systems.
v2.10 Rev. C
  - Fixes a problem with string parameter parsing (may prevent SBA/ESS from
    starting)
v2.20
  - Fixes OID problems seen with the new NDIS tester.
v2.30
  - Fixed system crashing due to TCPIP reentrancy problems (stack
    overflow).
  - No longer writing a "Timeout" error log entry under heavy load.
  - Double receive buffers allow parallel execution of DMA and receive
    indication.
  - Reset mechanism; both "soft" (caused by protocol) and "hard" (caused by
    timeout watchdog).
v2.31
  - Software or hardware failure detected by driver caused the driver to
    stop (endless software loop).
  - Sender could deadlock when network load was heavy.
v2.32
  - Fixed lookahead length problems (OID_GEN_CURRENT_LOOKAHEAD) experienced
    with new NDIS Tester (NCT).
***

*** End of information file ***
