AdapterID 063CAh
AdapterName  "Hewlett Packard StarLAN-10 Adapter Rev 1.1"
NumBytes 1

NamedItem
Prompt "Enable/Disable Adapter"

Choice " Adapter Enabled " pos[0]=XXXXXXX1b
Choice " Adapter Disabled " pos[0]=XXXXXXX0b

Help

"Lets you enable or disable the StarLAN-10 card.
Use the Enabled setting for normal use.
Use the Disabled setting if you are not using
the StarLAN-10 card and enabling it causes a conflict
with another card."

NamedItem
Prompt "I/O Address Range"

choice " 400 to  41F"  pos[0]=000XXXXXb io 0400h-041Fh
choice "1400 to 141F"  pos[0]=001XXXXXb io 1400h-141Fh
choice "2400 to 241F"  pos[0]=010XXXXXb io 2400h-241Fh
choice "3400 to 341F"  pos[0]=011XXXXXb io 3400h-341Fh
choice "4400 to 441F"  pos[0]=100XXXXXb io 4400h-441Fh
choice "5400 to 541F"  pos[0]=101XXXXXb io 5400h-541Fh
choice "6400 to 641F"  pos[0]=110XXXXXb io 6400h-641Fh
choice "7400 to 741F"  pos[0]=111XXXXXb io 7400h-741Fh

Help

"Selects the range of the I/O addresses used by the
StarLAN-10 card.  The addresses in the selected range
cannot be used by another adapter."


NamedItem
Prompt "Interrupt Level"

choice " Channel 3 "  pos[0]=XXXX000Xb  int 3
choice " Channel 4 "  pos[0]=XXXX001Xb  int 4
choice " Channel 5 "  pos[0]=XXXX010Xb  int 5
choice " Channel 7 "  pos[0]=XXXX011Xb  int 7
choice " Channel 9 "  pos[0]=XXXX100Xb  int 9
choice " Channel 10"  pos[0]=XXXX101Xb  int 10
choice " Channel 11"  pos[0]=XXXX110Xb  int 11
choice " Channel 12"  pos[0]=XXXX111Xb  int 12

Help

"Selects the interrupt level used by the StarLAN-10
card.  The interrupt level may be shared with
another adapter.  However, an unshared interrupt
level will improve adapter performance.
Furthermore, the HP OfficeShare network does
not allow for sharing the interrupt level."


