
[Filter]
Comment=No BROADCASTS or MULTICASTS
Lines=9
Line1=0,5,0
Line2=1,11,1
Line3=2,97,1,1,FDDI,:Destination Address bits,0,31,2,1,FDDI:Destination Address bits includes Bit 0x0 ON ( Group address ) 
Line4=1,11,1
Line5=2,97,1,1,TOKENRING,:Destination Address I/G Bit       ,0,13,2,1,TOKENRING:Destination Address I/G Bit        == 0x1 ( Group address ) 
Line6=1,11,1
Line7=2,97,1,1,ETHERNET,:Destination Address bits,0,31,2,1,ETHERNET:Destination Address bits includes Bit 0x0 ON ( Group address ) 
Line8=1,97,1,3,-1,Protocol == Any
Line9=1,97,0,2,27,30,27,ANY <--> ANY
