;----------------------------------------
; Modem responses are normally located in the global [Responses]
; section.  Most modems will return one of the responses listed in the
; global [Responses] section.  If you encounter a modem with a different
; response sequence than any of the responses already listed, add that
; new sequence to the global [Respones] section. You may also put new
; modem response sequences immediately following the command section of
; a specific modem.  Such responses are checked before the global
; responses.
;
; Individual modems will have separate command sections.  Modems with
; identical command sequences can be aliased.  E.g., if modem 2 has the
; same command sequences as modem 1, then modem 2's section might be
; as follows:
;
;      [modem 2]
;      alias=modem 1
;
; Aliases to aliased sections are not allowed. In other words, in the
; example given above, if you have "modem 3" which also has an identical
; command sequence to modem 1 and modem 2, you can alias modem 3 to
; modem 1, but you cannot alias modem 3 to modem 2.
;----------------------------------------

[Responses]

;----------------------------------------
;OK, ERROR, NO DIALTONE, NO CARRIER, etc
;----------------------------------------

OK=<lf>OK<cr><lf>
OK=<cr><lf>OK<cr><lf>
OK=<cr><cr><lf>OK<cr><lf>
OK=<hFF><cr><lf>OK<cr><lf>
LOOP=<lf>RING<cr><lf>
LOOP=<cr><lf>RING<cr><lf>
LOOP=<cr><lf>RRING<cr><lf>
LOOP=<cr><lf>RINGING<cr><lf>
LOOP=<cr><lf>DIALING<cr><lf>
ERROR=<cr><lf>ERROR<cr><lf>
ERROR=<cr><lf>ABORTED<cr><lf>
ERROR_NO_CARRIER=<cr><lf>NO CARRIER<cr><lf>
ERROR_VOICE=<cr><lf>VOICE<cr><lf>
ERROR_NO_DIALTONE=<cr><lf>NO DIALTONE<cr><lf>
ERROR_NO_DIALTONE=<cr><lf>NO DIAL TONE<cr><lf>
ERROR_BUSY=<cr><lf>BUSY<cr><lf>
ERROR_NO_ANSWER=<cr><lf>NO ANSWER<cr><lf>
ERROR_NO_PROMPTTONE=<cr><lf>NO PROMPTTONE<cr><lf>

;PDI modem
ERROR=<cr><lf>ERROR DATA Button not defined<cr><lf>

;----------------------------------------
;CONNECT responses with APPEND macro come first to force proper match
;----------------------------------------


;Zoom V32bis modem
CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: LAPM<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

;ATI modems, Hayes V Series; Practical

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: LAP-M/HDX<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42bis<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps> V.34<cr><lf><append>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42bis<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: LAP-M/HDX<cr><lf>\
<cr><lf>COMPRESSION: MNP5<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: MNP5<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: LAP-M/HDX<cr><lf>\
<cr><lf>COMPRESSION: MNP4<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: MNP4<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps>/ARQ<cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: LAP-M/HDX<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

;Stray char (0xFF) appears from time to time.
CONNECT=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf><hFF>

CONNECT=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: MNP<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: MNP<cr><lf>\
<cr><lf>COMPRESSION: CLASS 5<cr><lf><cr>\
<lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: MNP<cr><lf>\
<cr><lf>COMPRESSION: MNP5<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: MNP<cr><lf>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

;Next connect response occasionally occurs on Practical Peripherals 9600SA
CONNECT=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROT<hFF>OCOL: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: V.42/LAPM<cr><lf>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: LAPM<cr><lf>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: V.42/LAPM<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf><cr>\
<lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: V.42/LAPM<cr><lf>\
<cr><lf>COMPRESSION: CLASS 5<cr><lf><cr>\
<lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: V.42/LAPM<cr><lf>\
<cr><lf>COMPRESSION: NONE<cr><lf><cr>\
<lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: ALT<cr><lf>\
<cr><lf>COMPRESSION: CLASS 5<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: ALT<cr><lf>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: ALT<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: NONE<cr><lf>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

;megahertz pcmcia responses
CONNECT_EC=\
<cr><lf>CARRIER <carrierbps> V.34<cr><lf><append>\
<cr><lf>PROTOCOL: NONE<cr><lf>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps> V.34<cr><lf><append>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps> V.34<cr><lf><append>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps> V.34<cr><lf><append>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42bis<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

;----------------------------------------
;CONNECT responses that do not use the APPEND macro
;----------------------------------------

CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>

;AT&T ARK DM 424
CONNECT_EC=<cr><lf>CONNECT <connectbps> EC<cr><lf>

;AT&T Dataports like an extra space
CONNECT=<cr><lf>CONNECT <connectbps> <cr><lf>
CONNECT=<cr><lf>CONNECT <connectbps> <cr><lf><cr><lf>

;Telebits

CONNECT=<cr><lf>CONNECT <connectbps>/<carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/LAPM/<carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/LAPM/COMP/<carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/REL/COMP/<carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/REL/<carrierbps><cr><lf>

;;Digicom Scout

CONNECT=<cr><lf>CONNECT <connectbps><hFF>

CONNECT=\
<cr><lf>CONNECT<cr><lf>

CONNECT=<cr><lf>PLEASE SET TO <connectbps><cr><lf>

CONNECT=\
<cr><lf>PROTOCOL: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT=<cr><lf>CONNECT FAST<cr><lf>

;Racal RMD

CONNECT_EC=<cr><lf>CONNECT <carrierbps> MNP <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> V.42 <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> V.42 bis <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> V.42bis <connectbps><cr><lf>

;UDS Motorola
CONNECT_EC=\
<cr><lf>CONNECT <connectbps>/REL<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <connectbps>/LAPM<cr><lf>

;USRobotics modems

CONNECT=<cr><lf>CONNECT <ignore>/NONE<ignore>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/ARQ<cr><lf>

;Codex 3261Fast returns this if *XC1
;Codex 2264 also returns this

CONNECT_EC=<cr><lf>CONNECT <connectbps> RELIABLE<cr><lf>
CONNECT=<cr><lf>CONNECT <connectbps>/V32/NONE<cr><lf>

;;ATIs use this string

CONNECT_EC=<cr><lf>CONNECT <connectbps>/LAP-M <cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/LAP-M <cr><lf><cr><lf>OK<cr><lf>

CONNECT_EC=<cr><lf>CONNECT <connectbps>/LAPM/COMP<cr><lf>

;ZyXel U-1496

CONNECT_EC=<cr><lf>CONNECT <connectbps>/V32b <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V32b <carrierbps>/MNP4<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V32b <carrierbps>/MNP3<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V32b <carrierbps>/V42b<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V32b <carrierbps>/V42 <cr><lf>
CONNECT=<cr><lf>CONNECT <connectbps>/V32b <carrierbps>/NONE<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.32 <carrierbps>T/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.32 <carrierbps>T/MNP4<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.32 <carrierbps>T/MNP3<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.32 <carrierbps>T/V42b<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.32 <carrierbps>T/V42 <cr><lf>
CONNECT=<cr><lf>CONNECT <connectbps>/V.32 <carrierbps>T/NONE<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.22b <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.22b <carrierbps>/MNP4<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.22b <carrierbps>/MNP3<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.22b <carrierbps>/V42b<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.22b <carrierbps>/V42 <cr><lf>
CONNECT=<cr><lf>CONNECT <connectbps>/V.22b <carrierbps>/NONE<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/ZyX  <carrierbps>/MNP5/SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/ZyX  <carrierbps>/MNP4/SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/ZyX  <carrierbps>/MNP3/SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/ZyX  <carrierbps>/V42b/SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/ZyX  <carrierbps>/V42/SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V32b <carrierbps>/MNP5/SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V32b <carrierbps>/MNP4/SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V32b <carrierbps>/MNP3/SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V32b <carrierbps>/V42b/SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V32b <carrierbps>/V42/SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/ZyX  <carrierbps>/V42B/SREJ<cr><lf>
CONNECT=<cr><lf>CONNECT <connectbps>/V32b <carrierbps>/NONE<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.32 <carrierbps>T/MNP5/SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.32 <carrierbps>T/MNP4/SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.32 <carrierbps>T/MNP3/SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.32 <carrierbps>T/V42b/SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.32 <carrierbps>T/V42/SREJ<cr><lf>
CONNECT=<cr><lf>CONNECT <connectbps>/V.32 <carrierbps>T/NONE<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.22b <carrierbps>/MNP5/SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.22b <carrierbps>/MNP4/SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.22b <carrierbps>/MNP3/SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.22b <carrierbps>/V42b/SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.22b <carrierbps>/V42/SREJ<cr><lf>
CONNECT=<cr><lf>CONNECT <connectbps>/V.22b <carrierbps>/NONE<cr><lf>

;NEC modems

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>CONNECT <connectbps>/V.42bis<cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>CONNECT <connectbps>/V.42<cr><lf>

CONNECT=\
<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>CONNECT <connectbps>/REC<cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>CONNECT <connectbps>/REL<cr><lf>

;Supra

CONNECT=\
<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>OK<cr><lf>\
<cr><lf>OK<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

;Texas Instruments Internal
CONNECT_EC=<cr><lf>CONNECT <connectbps>/REL
CONNECT_EC=<cr><lf>CONNECT <connectbps>/REL MNP
CONNECT_EC=<cr><lf>CONNECT <connectbps>/REL V.42
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.42

;Rockwell
CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL: ALT<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

;----------------------------------------
; Additional Responses for German Modems
;----------------------------------------

;Creatix LCxxx

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps>/REL<cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: CLASS5<cr><lf>\
<cr><lf>CONNECT <connectbps>/REL<cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps>/REL<cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL: ALT<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps>/REL<cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL: ALT<cr><lf>\
<cr><lf>COMPRESSION: CLASS5<cr><lf>\
<cr><lf>CONNECT <connectbps>/REL<cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL: ALT<cr><lf>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps>/REL<cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL: ALT-CELLULAR<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps>/REL<cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL: ALT-CELLULAR<cr><lf>\
<cr><lf>COMPRESSION: CLASS5<cr><lf>\
<cr><lf>CONNECT <connectbps>/REL<cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL: ALT-CELLULAR<cr><lf>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps>/REL<cr><lf>

; ZyXEL (german and austrian versions)
; ZyXEL CELLULAR MODES
;
; ATTENTION: 1 OR 2 spaces before <carrierbps> required

CONNECT_EC=<cr><lf>CONNECT <connectbps>/CELL  <carrierbps>/V42b/SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/CELL  <carrierbps>/V42 /SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/CELL  <carrierbps>/V42b<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/CELL  <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/CELL  <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/CELL  <carrierbps>/MNP4<cr><lf>
CONNECT=<cr><lf>CONNECT <connectbps>/CELL  <carrierbps>/NONE<cr><lf>

CONNECT_EC=<cr><lf>CONNECT <connectbps>/CELL <carrierbps>/V42b/SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/CELL <carrierbps>/V42 /SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/CELL <carrierbps>/V42b<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/CELL <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/CELL <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/CELL <carrierbps>/MNP4<cr><lf>
CONNECT=<cr><lf>CONNECT <connectbps>/CELL <carrierbps>/NONE<cr><lf>

CONNECT_EC=<cr><lf>CONNECT <connectbps>/CELL <carrierbps>T/V42b/SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/CELL <carrierbps>T/V42 /SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/CELL <carrierbps>T/V42b<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/CELL <carrierbps>T/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/CELL <carrierbps>T/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/CELL <carrierbps>T/MNP4<cr><lf>
CONNECT=<cr><lf>CONNECT <connectbps>/CELL <carrierbps>T/NONE<cr><lf>

CONNECT_EC=<cr><lf>CONNECT <connectbps>/CELL <carrierbps>C/V42b/SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/CELL <carrierbps>C/V42 /SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/CELL <carrierbps>C/V42b<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/CELL <carrierbps>C/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/CELL <carrierbps>C/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/CELL <carrierbps>C/MNP4<cr><lf>
CONNECT=<cr><lf>CONNECT <connectbps>/CELL <carrierbps>C/NONE<cr><lf>

; Centraleurope ZyXEL PROPRIETARY MODES

CONNECT_EC=<cr><lf>CONNECT <connectbps>/ZyX  <carrierbps>/V42b/SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/ZyX  <carrierbps>/V42 /SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/ZyX  <carrierbps>/V42b<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/ZyX  <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/ZyX  <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/ZyX  <carrierbps>/MNP4<cr><lf>
CONNECT=<cr><lf>CONNECT <connectbps>/ZyX  <carrierbps>/NONE<cr><lf>

CONNECT_EC=<cr><lf>CONNECT <connectbps>/ZyX <carrierbps>/V42b/SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/ZyX <carrierbps>/V42 /SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/ZyX <carrierbps>/V42b<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/ZyX <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/ZyX <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/ZyX <carrierbps>/MNP4<cr><lf>
CONNECT=<cr><lf>CONNECT <connectbps>/ZyX <carrierbps>/NONE<cr><lf>

; ZYXEL - STANDARD MODES (additional responses to US versions)

CONNECT_EC=<cr><lf>CONNECT <connectbps>/V32b <carrierbps>/V42b/SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V32b <carrierbps>/V42 /SREJ<cr><lf>

CONNECT_EC=<cr><lf>CONNECT <connectbps>/V32b  <carrierbps>/V42b/SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V32b  <carrierbps>/V42 /SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V32b  <carrierbps>/V42b<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V32b  <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V32b  <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V32b  <carrierbps>/MNP4<cr><lf>
CONNECT=<cr><lf>CONNECT <connectbps>/V32b  <carrierbps>/NONE<cr><lf>

CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.32 <carrierbps>T/V42b/SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.32 <carrierbps>T/V42 /SREJ<cr><lf>

CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.32  <carrierbps>/V42b/SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.32  <carrierbps>/V42 /SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.32  <carrierbps>/V42b<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.32  <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.32  <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.32  <carrierbps>/MNP4<cr><lf>
CONNECT=<cr><lf>CONNECT <connectbps>/V.32  <carrierbps>/NONE<cr><lf>

CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.22b <carrierbps>/V42b/SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.22b <carrierbps>/V42 /SREJ<cr><lf>

CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.22  <carrierbps>/V42b/SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.22  <carrierbps>/V42 /SREJ<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.22  <carrierbps>/V42b<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.22  <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.22  <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V.22  <carrierbps>/MNP4<cr><lf>
CONNECT=<cr><lf>CONNECT <connectbps>/V.22  <carrierbps>/NONE<cr><lf>

;the next section attempts to catch all other responses not
;explicitly listed above.  The port speed is not changed
;from what it was originally set to by RAS.

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><ignore>

;----------------------------------------
[Angia DataStart for CompaqLTE]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=&U1
<compression_off>=&U0
<protocol_on>=\\N7
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATX3D

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=ANGIA Corporation

COMMAND_INIT=AT&F&C1&D2 L3 V1 W2 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL4<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL4<cr><lf>

;----------------------------------------
[Apex Data PCMCIA 144]
ALIAS=Megahertz XJack PCMCIA 144
DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=APEX DATA INC. V.32bis

;----------------------------------------
[ATI 2400 etc/e]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=&U1
<compression_off>=&U0
<protocol_on>=&Q6
<protocol_off>=&Q0
<autodial_on>=ATDT
<autodial_off>=AT X3 D

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=2400
MAXCONNECTBPS=9600

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=2400etc/e

COMMAND_INIT=AT&F&C1&D2 X4 W1 V1 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><compression><protocol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[ATI 9600 etc/e]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
;<compression_on>=&U1
;compression forced off for stability
<compression_on>=&U0
<compression_off>=&U0
<protocol_on>=&Q6
<protocol_off>=&Q0
<autodial_on>=ATDT
<autodial_off>=AT X3 D

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=38400

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=960

COMMAND_INIT=AT&F&C1&D2 W1 X4 V1 S0=0 S2=128 S7=55 <cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[AT&T 2224 CEO]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=AT X3 D

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=2400
MAXCONNECTBPS=2400

COMMAND_INIT=AT&F&C1&D2 V1 X4 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><speaker><cr>
COMMAND_LISTEN=ATS0=1<cr>
COMMAND_DIAL=<autodial><phonenumber><cr>

;----------------------------------------
[AT&T Comsphere 3810]
ALIAS=AT&T Comsphere 3820
DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=3810

;----------------------------------------
[AT&T Comsphere 3811]
ALIAS=AT&T Comsphere 3820
DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=3811

;----------------------------------------
[AT&T Comsphere 3820]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1"H3
<compression_off>=%C0"H0
<protocol_on>=\\N5
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=38400

DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=3820

COMMAND_INIT=AT&F&C1&D2 V1 X7 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><compression><protocol><speaker><cr>
COMMAND_LISTEN=ATS0=1<cr>
COMMAND_DIAL=<autodial><phonenumber><cr>

;----------------------------------------
[AT&T Comsphere 3810 Plus 288]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1"H3
<compression_off>=%C0"H0
<protocol_on>=\\N5
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=28800
MAXCONNECTBPS=57600

DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=3980-A1-401

COMMAND_INIT=AT&F&C1&D2 V1 X7 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><compression><protocol><speaker><cr>
COMMAND_LISTEN=ATS0=1<cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
;----------------------------------------
[AT&T Comsphere 3830]
ALIAS=AT&T Comsphere 3820
DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=3830

;----------------------------------------
[AT&T Dataport]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N5
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=38400

DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=3710
DETECT_RESPONSE=3721

COMMAND_INIT=AT&F&C1&D2 V1 X7 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><compression><protocol><speaker><cr>
COMMAND_LISTEN=ATS0=1<cr>
COMMAND_DIAL=<autodial><phonenumber><cr>

;----------------------------------------
[AT&T Dataport Express]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N7
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=38400

DETECT_STRING=ATI1<cr>
DETECT_RESPONSE=FW Level 091394

COMMAND_INIT=AT&F&C1&D2 V1 X7 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><compression><protocol><speaker><cr>
COMMAND_LISTEN=ATS0=1<cr>
COMMAND_DIAL=<autodial><phonenumber><cr>

;----------------------------------------
[AT&T Dataport 288]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N7
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=28800
MAXCONNECTBPS=57600

DETECT_STRING=ATI1<cr>
DETECT_RESPONSE=FW Level 030695

COMMAND_INIT=AT&F&C1&D2 V1 X7 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><compression><protocol><speaker><cr>
COMMAND_LISTEN=ATS0=1<cr>
COMMAND_DIAL=<autodial><phonenumber><cr>

;----------------------------------------
[AT&T Paradyne PCMCIA]
ALIAS=AT&T Dataport
DETECT_STRING=ATI7<cr>
DETECT_RESPONSE=Credit Card
DETECT_RESPONSE=CREDIT CARD

;----------------------------------------
[AT&T KeepInTouch Express PCMCIA]
ALIAS=AT&T Dataport
DETECT_STRING=ATI7<cr>
DETECT_RESPONSE=Credit Card
DETECT_RESPONSE=CREDIT CARD

;----------------------------------------
[AT&T 4024]

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=2400
MAXCONNECTBPS=2400

<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=24

COMMAND_INIT=ATE1Q0V1X4Y0S0=0 S7=15 &D2&C1&M0 <speaker><cr>
COMMAND_LISTEN=ATS0=2<cr>
COMMAND_DIAL=<autodial><phonenumber><cr>

;----------------------------------------
[Bocamodem M1440 Alt]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=38400

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
;use both %C and appropriate S46 settings to work correctly
<compression_on>=%C1S46=138
<compression_off>=%C0S46=136
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=TR14

COMMAND_INIT=AT&F&C1&D2&R1Q0V1E1X4 S0=0 S7=55 S2=128<cr>

;to get short responses
;COMMAND_INIT=ATW0S95=0<cr>
;to get long responses
COMMAND_INIT=ATW1S95=44<cr>

COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

[Boca Modem V.Fast Class]
ALIAS=Hayes Optima 28800

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=VFC
DETECT_STRING=ATI<cr>
DETECT_RESPONSE=28800

;----------------------------------------
[Cardinal 2400e]
ALIAS=Hayes Compatible 2400

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=249
DETECT_RESPONSE=248
DETECT_RESPONSE=242

;----------------------------------------
[Cardinal 9600]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&H1&I1
<hwflowcontrol_off>=&H0&I0
<compression_on>=&M6
<compression_off>=&M4
<protocol_on>=&M4
<protocol_off>=&M0&B0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=19200

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=9600
DETECT_RESPONSE=AT&T V.32bis

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55<speaker><cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Cardinal 14400]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=38400

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55<speaker><cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Cardinal 14400 Internal]
;Compression turned off for stability.
;Maximum DTE speed set to 19200
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C0
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=V1.<?><?> TR14
DETECT_RESPONSE=U8
DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=144
DETECT_RESPONSE=AT&T V.32

CALLBACKTIME=10
DEFAULTOFF=compression protocol hwflowcontrol
CLIENTDEFAULTOFF=compression protocol hwflowcontrol
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55<speaker><cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Codex 2264]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=9600

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=*FL3
<hwflowcontrol_off>=*FL0
<compression_on>=*SM3
<compression_off>=*SM0
<protocol_on>=*SM2
<protocol_off>=*SM0
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT&F&C1&D2S0=0 V1 *XC1 E1 S7=55 S2=128<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Codex 3220]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=19200
MAXCONNECTBPS=38400

<hwflowcontrol_off>=*FL0
<hwflowcontrol_on>=*FL3
<protocol_off>=*SM0
<protocol_on>=*SM3
<compression_off>=*DC0
<compression_on>=*DC1
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=AT&I0<cr>
DETECT_RESPONSE=7040

COMMAND_INIT=AT&F&C1&D2 V1 X4 *XC1 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Codex 3260]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=19200
MAXCONNECTBPS=38400
<hwflowcontrol_off>=*FL0
<hwflowcontrol_on>=*FL3
<protocol_off>=*SM0
<protocol_on>=*SM3
<compression_off>=*DC0
<compression_on>=*DC1
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT&F&C1&D2 V1 *XC1 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>
;----------------------------------------
[Codex 3261]
ALIAS=Codex 3260

DETECT_STRING=AT&I0<cr>
DETECT_RESPONSE=6510

;----------------------------------------
[Codex 3262]
ALIAS=Codex 3260

;----------------------------------------
[Codex 3263]
ALIAS=Codex 3260

;----------------------------------------
[Codex 3265]
ALIAS=Codex 3260

;----------------------------------------
[Codex 3260 Fast]

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=19200
MAXCONNECTBPS=38400
<hwflowcontrol_off>=*FL0
<hwflowcontrol_on>=*FL3
<protocol_off>=*SM0
<protocol_on>=*SM3
<compression_off>=*DC0
<compression_on>=*DC1
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT&F S0=0 &C1 &D2 V1 X4 S2=128 *XC1 S7=55<cr>
COMMAND_INIT=AT<speaker><protocol><hwflowcontrol><compression><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Codex 3261 Fast]
ALIAS=Codex 3260 Fast

DETECT_STRING=AT&I0<cr>
DETECT_RESPONSE=7061

;----------------------------------------
[Codex 3262 Fast]
ALIAS=Codex 3260 Fast

;----------------------------------------
[Codex 3263 Fast]
ALIAS=Codex 3260 Fast

;----------------------------------------
[Codex 3265 Fast]
ALIAS=Codex 3260 Fast

;----------------------------------------
[Codex V.34R]
ALIAS=Codex 3260 Fast

;----------------------------------------
[Codex 3220 Plus]
;ALIAS=Codex 3220
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=19200
MAXCONNECTBPS=38400

<hwflowcontrol_off>=*FL0
<hwflowcontrol_on>=*FL3
<protocol_off>=*SM0
<protocol_on>=*SM3
<compression_off>=*DC0
<compression_on>=*DC1
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=AT X3 D

COMMAND_INIT=AT&F&C1&D2 V1 X4 *XC1 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Compaq 2400 PCMCIA]
ALIAS=Hayes Compatible 2400

DETECT_STRING=ATI9<cr>
DETECT_RESPONSE=iNC215US

;----------------------------------------
[Compaq SpeedPAQ 144]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<protocol_on>=\\N3
<protocol_off>=\\N0
<compression_on>=%C1
<compression_off>=%C0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=19200
MAXCONNECTBPS=38400

DETECT_STRING=ATI9<cr>
DETECT_RESPONSE=COMPAQ

COMMAND_INIT=AT&F&C1&D2 V1 W2S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>

;----------------------------------------
[Compaq SpeedPAQ 144 PCMCIA]
ALIAS=Compaq SpeedPAQ 144
DETECT_STRING=ATI9<cr>
DETECT_RESPONSE=COMPAQ

;--------------------------------------------------------------------------------
; WARNING: The following modem had problems with CALLBACK feature in RAS.
;--------------------------------------------------------------------------------
[CXR Telcom 1445]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=*LR2*LG2
<hwflowcontrol_off>=*LR0*LG0
<protocol_on>=*M2
<protocol_off>=*M1
<compression_on>=*E1
<compression_off>=*E0
<autodial_on>=ATDT
<autodial_off>=ATD


CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=38400

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=1445

COMMAND_INIT=AT&F1<cr>
COMMAND_INIT=AT&C1&D2 *V1 *N1 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><speaker><compression><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP5<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP5<cr><lf>

;----------------------------------------
[DataRace RediModem V.32bis]
;Error control and flow control forced on for stability.
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q3
<protocol_on>=\\N3
<protocol_off>=\\N3
<compression_on>=%C1
<compression_off>=%C0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=38400

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=PC Half-Card V.32bis/V.42bis/Fax

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55 W1<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Datatrek 2424AMH]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=2400
MAXCONNECTBPS=2400

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><ignore>
CONNECT=<cr><lf><h07>CONNECT <connectbps><ignore>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <connectbps><ignore>
CONNECT=<cr><lf><h07>CONNECT <connectbps><ignore>

;----------------------------------------
[Datatrek Elite 624D]
;Advanced features disabled
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=2400
MAXCONNECTBPS=2400

DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=DataTrek <?><?> <?>.<?><?><?> D32

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55<cr>
;COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker>-M0\\V0<cr>
COMMAND_INIT=AT<speaker>-M0\\V0<cr>
COMMAND_INIT=AT%C0<cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
		
;----------------------------------------
[Datatrek V.32]
;Supported as a client modem only
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=9600

DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=DataTrek <?><?> <?>.<?><?><?> PR

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><speaker>-M0 \\V0<cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>

;----------------------------------------
[DP Defender 1000D Hayes Ultra]

;This entry uses the Digital Pathways Defender 1000D with the
;Hayes Ultra 9600 modem.
;The macro definitions, <xxx_xx>=, and COMMAND_INIT= lines must be
;changed in order to use other modems with the Defender.
;Set Defender ports to fixed 19200 bps (not autobaud).
;Set Originate Fallback to OFF on Configure DAD Options screen.
;(If used with Telebit WorldBlazer set S51=5 to fix port speed at 19200.)

DEFAULTOFF=compression
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200
CALLBACK_TIME=10

<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=&Q0
<protocol_on>=&Q5
<compression_off>=S46=136
<compression_on>=S46=2
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT&F&C1&D2 V1 X4 S0=0 S2=128 S7=55 W1 S95=44<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>

COMMAND_LISTEN=ATE0Q1S0=2<cr>
LOOP=<h0d>
LOOP=<h0d><ignore>
CONNECT=<match>"DIALIN_GATEWAY"
CONNECT=<?><?><?><?><hC0><h21><ignore>
CONNECT=<?><?><?><hC0><h21><ignore>
CONNECT=<?><?><hC0><h21><ignore>


;----------------------------------------
[Digicom Scout]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=*F3
<hwflowcontrol_off>=*F0
<compression_on>=*E9
<compression_off>=
<protocol_on>=*E5
<protocol_off>=*E0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=38400

DETECT_STRING=AT*O<cr>
DETECT_RESPONSE=SCOUT

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT*M0<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Digicom Scout Plus]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=*F3
<hwflowcontrol_off>=*F0
<compression_on>=*E9
<compression_off>=
<protocol_on>=*E5
<protocol_off>=*E0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=38400

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=961

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT&C1&D2 V1 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT*M0<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[DSI 9624LE Plus]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=*F3
<hwflowcontrol_off>=*F0
<compression_on>=*E9
<compression_off>=
<protocol_on>=*E5
<protocol_off>=*E0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=38400

DETECT_STRING=AT*O<cr>
DETECT_RESPONSE=9624LEP

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55*M0<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[DSI 9624E]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=*F3
<hwflowcontrol_off>=*F0
<compression_on>=*E9
<compression_off>=
<protocol_on>=*E5
<protocol_off>=*E0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=19200

DETECT_STRING=AT*O<cr>
DETECT_RESPONSE=MODEL: 9624E

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT*M0<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Eiger 144 PCMCIA]
ALIAS=Megahertz XJack PCMCIA 144
DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=RC144DPL

;----------------------------------------
[ETech UFOMATE P1496MX]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=$F4
<hwflowcontrol_off>=$F5
<compression_on>=$C1
<compression_off>=$C0
<protocol_on>=$E3
<protocol_off>=$E0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=19200
MAXCONNECTBPS=38400

DETECT_STRING=ATI1<cr>
DETECT_RESPONSE=P1496MX

COMMAND_INIT=AT&F&C1&D2 $X1 V1 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Evercom 24]
ALIAS=Hayes Compatible 2400

DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=EV943

;----------------------------------------
[Evercom 24E]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATX3D

DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=EV947


CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=2400
MAXCONNECTBPS=2400

COMMAND_INIT=ATZ&C1&D2 V1 S0=0 S2=128 S7=55<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Evercom 24E+]

<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=2400
MAXCONNECTBPS=2400

COMMAND_INIT=AT&F &C1 &D2 Q0 V1 \N1 S0=0 S2=128 S7=55<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;-----------------------------------------------
; Fastcomm Communications MonoFRAD
; (Frame Relay Access Device)
;
; The MonoFRAD has no modem command language.
; Thus, RAS can't query the device to recognize
; it automatically.
;
; To use this device, configure the RAS port,
; cancel the automatic configuration, and then
; select this entry from the listbox.
;
;-----------------------------------------------

[Fastcomm MonoFRAD]

CALLBACK_TIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=57600
MAXCONNECTBPS=115200

COMMAND_INIT=
NoResponse

COMMAND_LISTEN=
NoResponse

COMMAND_DIAL=
NoResponse

;----------------------------------------
[Gateway 2000 Internal Alt]
ALIAS=US Robotics Sportster 14400
;-----------------------------------------
[Gateway 2000 Internal]
<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=\\N0
<protocol_on>=\\N3
<compression_off>=%C0
<compression_on>=%C1
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=38400

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=Gateway TelePath 1.5

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55 W1 S95=44<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Gateway 2000 Nomad 14400]
<hwflowcontrol_off>=\\Q0
<hwflowcontrol_on>=\\Q3
<protocol_off>=\\N0
<protocol_on>=\\N7
<compression_off>=%C0
<compression_on>=%C1
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATX1D

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=Texas Instrument V.32

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=19200
MAXCONNECTBPS=38400

COMMAND_INIT=AT&F&C1&D2 V1 X4 S0=0 S2=128 S7=55 W0<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Gateway 2000 PCMCIA]
ALIAS=Megahertz XJack PCMCIA 144
DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=GATEWAY2000
DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=RC144DPL

;----------------------------------------
[Generic 144 PCMCIA modem]
ALIAS=Megahertz XJack PCMCIA 144
DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=RC144DPL

;----------------------------------------
[GVC SM2400]
ALIAS=Hayes Compatible 2400

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=249
DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=AT-C2401-0E
;----------------------------------------
[GVC SM96]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=38400

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N6
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=SM-96

COMMAND_INIT=AT&F&C1&D2Q0V1E1S0=0S2=128S7=55<speaker><cr>
COMMAND_INIT=AT<compression><hwflowcontrol><protocol><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP/COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>
CONNECT=<cr><lf><cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf><cr><lf>CONNECT <carrierbps>/MNP<cr><lf>
CONNECT_EC=<cr><lf><cr><lf>CONNECT <carrierbps>/MNP/COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf><cr><lf>CONNECT <carrierbps>/MNP COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf><cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf><cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP/COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>
CONNECT=<cr><lf><cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf><cr><lf>CONNECT <carrierbps>/MNP<cr><lf>
CONNECT_EC=<cr><lf><cr><lf>CONNECT <carrierbps>/MNP/COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf><cr><lf>CONNECT <carrierbps>/MNP COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf><cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf><cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>

;----------------------------------------
[GVC FM14400]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=38400

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N6
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=FM-144VBIS
DETECT_RESPONSE=FM-1114V

COMMAND_INIT=AT&F&C1&D2Q0V1E1S0=0S2=128 S7=55 S95=44<cr>
COMMAND_INIT=AT<speaker><compression><hwflowcontrol><protocol><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP/COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP/COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>

;----------------------------------------
[Hayes Accura 14400]
ALIAS=Hayes Optima 14400

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=14400

;----------------------------------------
[Hayes Accura 28800]
ALIAS=Hayes Optima 28800

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=28800

;----------------------------------------
[Hayes Compatible 1200]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=1200
MAXCONNECTBPS=1200
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATX3D

COMMAND_INIT=ATQ0V1E1S0=0S2=128 S7=55<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Hayes Compatible 2400]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATX3D

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=2400
MAXCONNECTBPS=2400

;DETECT_STRING=ATI<cr>
;DETECT_RESPONSE=249

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Hayes Compatible 9600]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATX3D
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=9600

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Hayes Compatible 14400]
ALIAS=Hayes Optima 14400
DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=14400

;----------------------------------------
[Hayes Pocket Modem 2400]
ALIAS=Hayes Compatible 2400

;DETECT_STRING=ATI0<cr>
;DETECT_RESPONSE=249

;----------------------------------------
[Hayes Smartmodem 2400]
ALIAS=Hayes Compatible 2400

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=249
DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=04-000

;----------------------------------------
[Hayes Smartmodem 9600]
ALIAS=Hayes Compatible 9600
DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=960

;----------------------------------------
[Hayes Optima 9600]
<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=&Q0
<protocol_on>=&Q5
<compression_off>=S46=136
<compression_on>=S46=2
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATX3D

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=38400

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=960

COMMAND_INIT=AT&F&C1&D2 V1 X4 S0=0 S2=128 S7=55 W1 S95=44<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Hayes Optima 14400]
<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=&Q0
<protocol_on>=&Q5
<compression_off>=S46=136
<compression_on>=S46=2
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=38400

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=14400

COMMAND_INIT=AT&F&C1&D2 V1 X4 S0=0 S2=128 S7=55 W1 S95=44<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Hayes Optima PCMCIA 14400]
ALIAS=Hayes Optima 14400
DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=PCMCIA
DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=RC144DPL

;----------------------------------------
[Hayes Optima 28800]
<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=&Q0
<protocol_on>=&Q5
<compression_off>=S46=136
<compression_on>=S46=2
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=15
DEFAULTOFF=compression
MAXCARRIERBPS=28800
MAXCONNECTBPS=57600

DETECT_STRING=ATI<cr>
DETECT_RESPONSE=28800

COMMAND_INIT=AT&F&C1&D2 V1 X4 S0=0 S2=128 S7=55 W0 S95=44<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Hayes Ultra 9600]
ALIAS=Hayes Optima 9600

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=960

;----------------------------------------
[Hayes Ultra 14400]
ALIAS=Hayes Optima 14400

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=14400

;----------------------------------------
[Hayes V Series Smartmodem 9600]
<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=&Q0
<protocol_on>=&Q5
<compression_off>=S46=0
<compression_on>=S46=2
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=AT X3 D

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=19200

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=960

;Reset modem
COMMAND_INIT=AT&/3<cr>
OK=<ignore>
COMMAND_INIT=AT&\\3<cr>
OK=<ignore>
COMMAND_INIT=AT&F&W<cr>

COMMAND_INIT=AT&F&C1&D2 X4 V1 W1 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[IBM 14400 PCMCIA]
ALIAS=Megahertz XJack PCMCIA 144
DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=PCMCIA
DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=RCV144DPL
DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=RC144DPL

;----------------------------------------
[Infotel 1414VQE External]
ALIAS=Hayes Optima 14400
DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=14400

;----------------------------------------
[Intel SatisFaxtion 100]
ALIAS=Hayes Compatible 2400

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=AF-C

;----------------------------------------
[Intel SatisFaxtion 400e]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1"H3
<compression_off>=%C0"H0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=AT X3 D

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=38400

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=U20
DETECT_RESPONSE=U21

COMMAND_INIT=AT&F&C1&D2 V1 \\V3 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<speaker><hwflowcontrol><compression><protocol><cr>
COMMAND_LISTEN=ATS0=1<cr>
COMMAND_DIAL=<autodial><phonenumber><cr>

;----------------------------------------
[Intel 9600EX]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=38400

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1"H3
<compression_off=%C0"H0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATX3D

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=969
DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=U21

COMMAND_INIT=AT&F&C1&D2V1S0=0 X4 \\V2 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><compression><protocol><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL-LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL-MNP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL-LAPM-COMP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL-MNP-COMP<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL-LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL-MNP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL-LAPM-COMP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL-MNP-COMP<cr><lf>

;----------------------------------------
[Intel 14400EX]
ALIAS=Intel SatisFaxtion 400e

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=U20
DETECT_RESPONSE=U21

DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=INTEL 14400E

;----------------------------------------
[Intel 14400 PCMCIA]
ALIAS=Megahertz XJack PCMCIA 144
DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=144
DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=RC144DPL

;----------------------------------------
[Kingston DataRex PCMCIA 144]
ALIAS=Megahertz XJack PCMCIA 144
DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=PCMCIA
DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=RC144DPL

;----------------------------------------
[Macronix Maxlite Fax 9696]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=38400

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C1%M3
<compression_off>=%C0
<protocol_on>=&Q5
<protocol_off>=&Q0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=MAXFAX MAXLITE

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Macronix VOMAX 2000]
ALIAS=Hayes Compatible 2400
DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=VOMAX 2.1

;----------------------------------------
[Megahertz P2144 AA Batteries]
ALIAS=Megahertz T3144 for Toshiba

;----------------------------------------
[Megahertz P296FMV AA Batteries]
ALIAS=Megahertz T396FM for Toshiba

;----------------------------------------
[Megahertz P2144 Pkt Faxmodem]
;strings for rockwell chip modem
DEVICETYPE=modem
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=19200

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&Q5
<hwflowcontrol_off>=&Q0
<protocol_on>=\\N5
<protocol_off>=\\N0
<compression_on>=%C1
<compression_off>=%C0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=144DPL+FAX

COMMAND_INIT=AT&F&C1&D2 W2\\G0\\J0 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL<cr><lf>

;----------------------------------------
[Megahertz T3144 for Toshiba]
DEVICETYPE=modem
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=19200

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<protocol_on>=\\N7
<protocol_off>=\\N0
<compression_on>=%C1
<compression_off>=%C0
<autodial_on>=ATDT
<autodial_off>=ATX3D

COMMAND_INIT=AT&F&C1&D2 W2\\G0\\J0\\V1 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL<cr><lf>

;----------------------------------------
[Megahertz T396FM for Toshiba]
DEVICETYPE=modem
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=19200

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<protocol_on>=\\N7
<protocol_off>=\\N0
<compression_on>=%C1
<compression_off>=%C0
<autodial_on>=ATDT
<autodial_off>=ATX3D

COMMAND_INIT=AT&F&C1&D2 W2\\G0\\J0\\V1 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL<cr><lf>

;----------------------------------------
[Megahertz C596FM for CompaqLTE]
ALIAS=Megahertz T396FM for Toshiba

;----------------------------------------
[Megahertz Z396FM for Zenith]
ALIAS=Megahertz T396FM for Toshiba

;----------------------------------------
[Megahertz Z3144 for Zenith]
ALIAS=Megahertz T3144 for Toshiba

DETECT_STRING=AT%V<cr>
DETECT_RESPONSE=AT&T V.32bis/V.42bis/FAX 14400

;----------------------------------------
[Megahertz C5144 for Compaq LTE]
ALIAS=Megahertz T3144 for Toshiba

DETECT_STRING=AT%V<cr>
DETECT_RESPONSE=AT&T V.32bis/V.42bis/FAX 14400

;----------------------------------------
[Megahertz Alternative]
; use this section if you get Error 651 when
; using [Megahertz P2144] section above.
ALIAS=Hayes Optima 14400

;----------------------------------------
[Megahertz XJack PCMCIA 144]
DEVICETYPE=modem
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=19200
MAXCONNECTBPS=38400

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<protocol_on>=\\N3
<protocol_off>=\\N0
<compression_on>=%C3
<compression_off>=%C0
<autodial_on>=ATDT
<autodial_off>=ATX3D

DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=MEGAHERTZ
DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=RC144DPL

COMMAND_INIT=AT&F&C1&D2 L2 X4 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Megahertz XJack PCMCIA 288]
DEVICETYPE=modem
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=28800
MAXCONNECTBPS=57600

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<protocol_on>=\\N3
<protocol_off>=\\N0
<compression_on>=%C1
<compression_off>=%C0
<autodial_on>=ATDT
<autodial_off>=ATX3D

DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=MEGAHERTZ
DETECT_STRING=ATI<cr>
DETECT_RESPONSE=MHZ AT&T V.34

COMMAND_INIT=AT&F&C1&D2 L2 W0 X4 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Metricom Wireless 9600]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=9600

COMMAND_INIT=AT&F&C1&D2 S0=0 S2=127 S7=55<cr>
COMMAND_DIAL=ATDT<phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[MicroCom DeskPorte FAST]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=28800
MAXCONNECTBPS=57600

<speaker_on>=M1
<speaker_off>=M0
<protocol_on>=\\N3
<protocol_off>=\\N0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C3
<compression_off>=%C0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=DeskPorte V.FC

COMMAND_INIT=AT&F&C1&D2 V1 -M0 W1 S2=128 S7=55<cr>
COMMAND_INIT=AT<speaker><compression><hwflowcontrol><protocol><cr>

COMMAND_LISTEN=ATS0=1<cr>
COMMAND_DIAL=<autodial><phonenumber><cr>

;----------------------------------------
[MicroCom DeskPorte FAST ES28.8]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=28800
MAXCONNECTBPS=57600

<speaker_on>=M1
<speaker_off>=M0
<protocol_on>=\\N3
<protocol_off>=\\N0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C3
<compression_off>=%C0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=VFC
DETECT_STRING=ATI<cr>
DETECT_RESPONSE=28800

COMMAND_INIT=AT&F&C1&D2 V1 M0 W1 S2=128 S7=55<cr>
COMMAND_INIT=AT<speaker><compression><hwflowcontrol><protocol><cr>

COMMAND_LISTEN=ATS0=1<cr>
COMMAND_DIAL=<autodial><phonenumber><cr>

;----------------------------------------
[MicroCom DeskPorte V.34]
ALIAS=MicroCom DeskPorte FAST

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=DeskPorte 28.8

;----------------------------------------
[MicroCom TravelCard 288 PCMCIA]
ALIAS=MicroCom DeskPorte FAST

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=TravelCard V.FC

;----------------------------------------
[MicroCom QX 4232bis]
;Advanced features disabled, MAXCONNECT set to 19200
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

<speaker_on>=M1
<speaker_off>=M0
<protocol_on>=\\N3
<protocol_off>=\\N0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C3
<compression_off>=%C0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=1441
DETECT_RESPONSE=1442

COMMAND_INIT=AT&F&C1&D2 W1 V1 \\V1 \\N0 \\Q0 \\J1 %C0 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<speaker><cr>

COMMAND_LISTEN=ATS0=1<cr>
;CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
;CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL<cr><lf>

COMMAND_DIAL=<autodial><phonenumber><cr>
;CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
;CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL<cr><lf>

;----------------------------------------
[MicroComQX 4232HS]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=9600

<speaker_on>=M1
<speaker_off>=M0
<protocol_on>=\\N3
<protocol_off>=\\N0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C3
<compression_off>=%C0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=962

COMMAND_INIT=AT&F&C1&D2 V1 \\V1 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<speaker><compression><hwflowcontrol><protocol><cr>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL<cr><lf>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL<cr><lf>

;----------------------------------------
[MicroGate MG96]
;Error control and flow control forced on for stability.
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=38400

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K3
<protocol_on>=&Q5
<protocol_off>=&Q5
<compression_on>=%C1
<compression_off>=%C0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=TR14

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55 w1<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>

;----------------------------------------
[MicroGate MG144]
;Error control and flow control forced on for stability.
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=38400

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K3
<protocol_on>=&Q5
<protocol_off>=&Q5
<compression_on>=%C1
<compression_off>=%C0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=14400

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55 w1<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>

;----------------------------------------
[MicroPorte 1042]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=2400
MAXCONNECTBPS=9600

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C3
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=AT%V<cr>
DETECT_RESPONSE=MicroPorte

COMMAND_INIT=AT&F&C1&D2 V1 \\V1 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL<cr><lf>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL<cr><lf>

;---------------------------
[Modem Blaster 144 PCMCIA]
ALIAS=New Media 144 PCMCIA
DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=CL-MD1414AT

;----------------------------------------
[Motorola Power 288]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=28800
MAXCONNECTBPS=57600
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N7
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=Motorola Power 28.8

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT&C1&D2 \\V1 S0=0 S2=128 S7=30<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;-------------------------------------------
[MultiTech MultiModem 224]
;Hardware flow control hardcoded ON for stability.
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&E4
<hwflowcontrol_off>=&E4
<compression_on>=&E15
<compression_off>=&E14
<protocol_on>=&E1
<protocol_off>=&E0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=2400
MAXCONNECTBPS=19200

DETECT_STRING=ATI2<cr>
DETECT_RESPONSE=MT224

COMMAND_INIT=AT&F E1 &C1<cr>
COMMAND_INIT=AT V1 &D2 &Q1 X4 S0=0 S2=128 S7=55 $BA0<cr>
COMMAND_INIT=AT<compression><protocol><hwflowcontrol><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM COMPRESSED<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM COMPRESSED<cr><lf>

;-------------------------------------------
[MultiTech MultiModem MT932]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&E4
<hwflowcontrol_off>=&E3
<compression_on>=&E15
<compression_off>=&E14
<protocol_on>=&E1
<protocol_off>=&E0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=38400

DETECT_STRING=ATI2<cr>
DETECT_RESPONSE=MT932BA

COMMAND_INIT=AT&SF1&S0&W<cr>
COMMAND_INIT=AT E1<cr>
COMMAND_INIT=AT &F &C1 V1 &D2 &Q0 X4 &S0 S0=0 S2=128 S7=55 $BA0<cr>
COMMAND_INIT=AT<compression><hwflowcontrol><protocol><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM COMPRESSED<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM COMPRESSED<cr><lf>

;-------------------------------------------
[MultiTech MultiModem MT1432]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&E4
<hwflowcontrol_off>=&E3
<compression_on>=&E15
<compression_off>=&E14
<protocol_on>=&E1
<protocol_off>=&E0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=19200
MAXCONNECTBPS=38400

DETECT_STRING=ATI2<cr>
DETECT_RESPONSE=MT1432ZDX

COMMAND_INIT=AT&SF1&S0&W<cr>
COMMAND_INIT=AT E1<cr>
COMMAND_INIT=AT &F &C1 V1 &D2 &Q0 X4 &S0 S0=0 S2=128 S7=55 $BA0<cr>
COMMAND_INIT=AT<compression><hwflowcontrol><protocol><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM COMPRESSED<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM COMPRESSED<cr><lf>

;-------------------------------------------
[MultiTech MultiModem MT2834]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&E4
<hwflowcontrol_off>=&E3
<compression_on>=&E15
<compression_off>=&E14
<protocol_on>=&E1
<protocol_off>=&E0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=15
DEFAULTOFF=compression
MAXCARRIERBPS=28800
MAXCONNECTBPS=57600


DETECT_STRING=ATI<cr>
DETECT_RESPONSE=247
DETECT_STRING=ATI2<cr>
DETECT_RESPONSE=MT2834BA

COMMAND_INIT=AT&SF1&S0&W<cr>
COMMAND_INIT=AT E1<cr>
COMMAND_INIT=AT &F &C1 V1 &D2 &Q0 X4 &S0 S0=0 S2=128 S7=55 $BA0<cr>
COMMAND_INIT=AT<compression><hwflowcontrol><protocol><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM COMPRESSED<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM COMPRESSED<cr><lf>

;----------------------------------------
[NEC 9635E Plus]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N6
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=19200
MAXCONNECTBPS=38400

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=N9635E/PLUS

COMMAND_INIT=AT&F&C1&D2 \\V3 V1 S0=0 S2=128 S7=55 <cr>
COMMAND_INIT=AT<compression><hwflowcontrol><protocol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;---------------------------
[NEC 14.4 Data/Fax PCMCIA]
ALIAS=AT&T Dataport

;----------------------------------------
[New Media 144 PCMCIA]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATX3D
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=19200
MAXCONNECTBPS=38400

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=CL-MD1414AT

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[NoteWorthy 14400 PCMCIA]
ALIAS=Megahertz XJack PCMCIA 144
DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=144
DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=RC144DPL

;----------------------------------------
[Null Modem 4800]

CALLBACK_TIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=4800
MAXCONNECTBPS=4800

COMMAND_INIT=
NoResponse

COMMAND_LISTEN=
CONNECT=CLIENT
CONNECT=<h00>CLIENT
COMMAND_LISTEN=CLIENTSERVER
NoResponse

COMMAND_DIAL=CLIENT
CONNECT=SERVER

;----------------------------------------
[Null Modem 9600]

CALLBACK_TIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=9600

COMMAND_INIT=
NoResponse

COMMAND_LISTEN=
CONNECT=CLIENT
CONNECT=<h00>CLIENT
COMMAND_LISTEN=CLIENTSERVER
NoResponse

COMMAND_DIAL=CLIENT
CONNECT=SERVER

;----------------------------------------
[Null Modem 19200]

CALLBACK_TIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=
NoResponse

COMMAND_LISTEN=
CONNECT=CLIENT
CONNECT=<h00>CLIENT
COMMAND_LISTEN=CLIENTSERVER
NoResponse

COMMAND_DIAL=CLIENT
CONNECT=SERVER

;----------------------------------------
[Null Modem 38400]

CALLBACK_TIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=38400
MAXCONNECTBPS=38400

COMMAND_INIT=
NoResponse

COMMAND_LISTEN=
CONNECT=CLIENT
CONNECT=<h00>CLIENT
COMMAND_LISTEN=CLIENTSERVER
NoResponse

COMMAND_DIAL=CLIENT
CONNECT=SERVER

;----------------------------------------
[Octocom 8324]
;Hardware flow control and error correction are set ON for stability.
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<protocol_off>=&E0
<protocol_on>=&E1
<compression_off>=*E0
<compression_on>=*E1
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=2400
MAXCONNECTBPS=9600

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=317

COMMAND_INIT=AT&F &C3 &D2 &I2 V1 E1 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/LAP-M ACTIVE<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/LAP-M ACTIVE<cr><lf>


;----------------------------------------
[Octocom 8396]
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<protocol_off>=&E0
<protocol_on>=&E1
<compression_off>=*E0
<compression_on>=*E1
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATD


CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=19200
MAXCONNECTBPS=38400

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=321

COMMAND_INIT=AT&F &C3 &D2 &I2 V1 E1 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/LAP-M ACTIVE<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/LAP-M ACTIVE<cr><lf>

;----------------------------------------
[PDI-1000]
;Supported on client side only.
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=9600

COMMAND_INIT=AT&F&C1&D2 V1 E1 S0=0 S2=128 S7=55 S32=0<cr>
COMMAND_INIT=AT<hwflowcontrol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Practical Peripherals2400 Pkt]
ALIAS=Hayes Compatible 2400

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=PM2400PPM
;----------------------------------------
[Practical Peripherals 2400SA]
;Server:Does not hang up normally. Not supported as a server modem.
;Client side works
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATX3DT
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=2400
MAXCONNECTBPS=2400

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=04-00027-16
DETECT_RESPONSE=AT-C2401-0E

COMMAND_INIT=AT&F&D2 V1 S0=0 S2=128 S7=55 <speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Practical Peripherals 2400MNP]

;Advanced features are disabled.
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=2400
MAXCONNECTBPS=2400

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=04-000

COMMAND_INIT=AT&F&C2&D2 V1 S0=0 S2=128 S7=55 &Q0<cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;--------------------------------------------------------------------------------
; WARNING: The following modem had problems with CALLBACK feature in RAS.
;--------------------------------------------------------------------------------
[Practical Peripherals 9600SA]
<hwflowcontrol_off>=&K0 &Q0
<hwflowcontrol_on>=&K3
<protocol_off>=&Q6
<protocol_on>=&Q5
<compression_off>=S46=136
<compression_on>=S46=138
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=38400

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=PM9600

COMMAND_INIT=AT&F&D2&C1 V1 S0=0 S2=128 S7=55 S95=44<cr>
COMMAND_INIT=AT<protocol><hwflowcontrol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Practical Peripherals 9600FX]
ALIAS=Practical Peripherals 9600SA
DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=PM9600FX

;----------------------------------------
[Practical Peripherals 14400SA]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=38400

<hwflowcontrol_off>=&K0 &Q0
<hwflowcontrol_on>=&K3
<protocol_off>=&Q6
<protocol_on>=&Q5
<compression_off>=S46=0
<compression_on>=S46=2
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=AT X3 DT

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=PM14400FXSA

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55 S95=44<cr>
COMMAND_INIT=AT<protocol><hwflowcontrol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Practical Peripherals 14400FX]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=38400

<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=&Q0
<protocol_on>=&Q5
<compression_off>=S46=0
<compression_on>=S46=2
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=AT X3 DT

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=PM14400FX

COMMAND_INIT=AT&F&C1&D2 V1 W1 S0=0 S2=128 S7=55 S95=44<cr>
COMMAND_INIT=AT<protocol><hwflowcontrol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Practical Peripherals 14400MT]
ALIAS=Practical Peripherals 14400FX
DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=PM14400FXMT

;----------------------------------------
[Practical Peripherals PC288MT]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=28800
MAXCONNECTBPS=57600

<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=&Q0
<protocol_on>=&Q5
<compression_off>=S46=0
<compression_on>=S46=2
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=AT X3 DT

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=PC288MT

COMMAND_INIT=AT&F&C1&D2 V1 W1 S0=0 S2=128 S7=55 S95=44<cr>
COMMAND_INIT=AT<protocol><hwflowcontrol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Practical Peripherals PM288PKT]
ALIAS=Practical Peripherals PC288MT
DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=PM288PPM

;----------------------------------------
[Practical Peripherals PC288SA]
ALIAS=Practical Peripherals PC288MT
DETECT_STRING=ATI<cr>
DETECT_RESPONSE=28800
DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=PC288SA

;----------------------------------------
[Practical ProClass 144 PCMCIA]
ALIAS=Hayes Optima 14400

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=PC144T2
DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=PC144T2Statistics

;----------------------------------------
[Racal GSM w/ Hayes Ultra]

;This entry uses the Racal GuardData Gateway Security Module with the
;Hayes Ultra 9600 modem.
;The macro definitions, <xxx_xx>=, and COMMAND_INIT= lines must be
;changed in order to use other modems with the GSM.
;Do not give callback permission to accounts used with the GSM.
;Set GSM ports to fixed 19200 bps (not autobaud).

DEFAULTOFF=compression
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=&Q0
<protocol_on>=&Q5
<compression_off>=S46=136
<compression_on>=S46=2
<speaker_off>=M0
<speaker_on>=M1

COMMAND_INIT=AT&F&C1&D2 V1 X4 S0=0 S2=128 S7=55 W1 S95=44<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>

COMMAND_LISTEN=ATE0Q1S0=1<cr>
LOOP=<h0d><ignore>
CONNECT=<match>"DIALIN_GATEWAY"
CONNECT=<?><?><?><?><hC0><h21><ignore>
CONNECT=<?><?><?><hC0><h21><ignore>
CONNECT=<?><?><hC0><h21><ignore>


;----------------------------------------
[Racal RMD 2412]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCONNECTBPS=9600
MAXCARRIERBPS=2400

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=*F2
<hwflowcontrol_off>=*F0
<compression_on>=*D0
<compression_off>=*D1
<protocol_on>=*E1
<protocol_off>=*E0
<autodial_on>=ATDT
<autodial_off>=AT X3DT

COMMAND_INIT=AT&F&C1&D2 X4 V1 S0=0 S2=128 S7=55 <cr>
COMMAND_INIT=AT<hwflowcontrol><compression><protocol><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>

;----------------------------------------
[Racal RMD 2422]
ALIAS=Racal RMD 2412

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=246

;----------------------------------------
[Racal RMD 2412/2]
Toggled MAXCONNECTBPS back to 2400
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCONNECTBPS=2400
MAXCARRIERBPS=2400

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=*F2
<hwflowcontrol_off>=*F0
<compression_on>=*D0
<compression_off>=*D1
<protocol_on>=*E1
<protocol_off>=*E0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=247

COMMAND_INIT=AT&F&C1&D2 X4 V1 S0=0 S2=128 S7=55 <cr>
COMMAND_INIT=AT<hwflowcontrol><compression><protocol><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>

;----------------------------------------
[Racal RMD 3221]
;Set MAXCONNECTBPS to disable unsupported baud rate of 12000 bps.
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=9600

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=*F2
<hwflowcontrol_off>=*F0
<compression_on>=*D1
<compression_off>=*D0
<protocol_on>=*E1
<protocol_off>=*E0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=RACAL

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<speaker><hwflowcontrol><compression><protocol><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Racal RMD 3222]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=19200
MAXCONNECTBPS=38400

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q1
<hwflowcontrol_off>=\\Q0
<compression_on>=\\M0
<compression_off>=\\M1\\C4
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=096

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<speaker><hwflowcontrol><compression><protocol><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps><cr><lf><append>\
<cr><lf>V42bis <connectbps><cr><lf>
CONNECT=\
<cr><lf>CONNECT <carrierbps><cr><lf><append>\
<cr><lf>BUFFER <connectbps><cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps><cr><lf><append>\
<cr><lf>V42 <connectbps><cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps><cr><lf><append>\
<cr><lf>MNP <connectbps><cr><lf>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps><cr><lf><append>\
<cr><lf>V42bis <connectbps><cr><lf>
CONNECT=\
<cr><lf>CONNECT <carrierbps><cr><lf><append>\
<cr><lf>BUFFER <connectbps><cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps><cr><lf><append>\
<cr><lf>V42 <connectbps><cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps><cr><lf><append>\
<cr><lf>MNP <connectbps><cr><lf>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>

;----------------------------------------
[Racal RMD 3226]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=14400

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K3
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=3226

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<speaker><hwflowcontrol><protocol><compression><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps><cr><lf><append>\
<cr><lf>V42bis <connectbps><cr><lf>
CONNECT=\
<cr><lf>CONNECT <carrierbps><cr><lf><append>\
<cr><lf>BUFFER <connectbps><cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps><cr><lf><append>\
<cr><lf>V42 <connectbps><cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps><cr><lf><append>\
<cr><lf>MNP <connectbps><cr><lf>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps><cr><lf><append>\
<cr><lf>V42bis <connectbps><cr><lf>
CONNECT=\
<cr><lf>CONNECT <carrierbps><cr><lf><append>\
<cr><lf>BUFFER <connectbps><cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps><cr><lf><append>\
<cr><lf>V42 <connectbps><cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps><cr><lf><append>\
<cr><lf>MNP <connectbps><cr><lf>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
;----------------------------------------
[Racal ALM 3226]
ALIAS=Racal RMD 3226

DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=3226

;----------------------------------------
[Racal RMD 3223]
ALIAS=Racal RMD 3222

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=960
;----------------------------------------
[Racal RMD 9632PA]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=38400

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q1
<hwflowcontrol_off>=\\Q0
<compression_on>=\\C5
<compression_off>=\\C4
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=RACAL

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<speaker><hwflowcontrol><compression><protocol><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps><cr><lf><append>\
<cr><lf>MNP <connectbps><cr><lf>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps><cr><lf><append>\
<cr><lf>MNP <connectbps><cr><lf>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>

;----------------------------------------
[Racal RMD 9642PA]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=19200

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q1
<hwflowcontrol_off>=\\Q0
<compression_on>=\\C5
<compression_off>=\\C4
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATX3

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=096

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<speaker><hwflowcontrol><compression><protocol><cr>

;Following line disables error correction, compression. To enable, delete
;the following line and use rasphone interface.
COMMAND_INIT=AT \\N0 <cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps><cr><lf><append>\
<cr><lf>MNP <connectbps><cr><lf>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps><cr><lf><append>\
<cr><lf>MNP <connectbps><cr><lf>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>

;----------------------------------------
[SD ACM400 w/ AT&T 3820]

;This entry uses the Security Dynamics ACM/400 with the
;AT&T Comsphere 3820 modem.
;The macro definitions, <xxx_xx>=, and COMMAND_INIT= lines must be
;changed in order to use other modems with the ACM/400.
;Set ACM/400 ports to fixed 19200 bps (not autobaud).
;Do not use Destination IDs with ACM/400 accounts.

DEFAULTOFF=compression
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1"H3
<compression_off>=%C0"H0
<protocol_on>=\\N5
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT&F&C1&D2 V1 X7 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><compression><protocol><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>

COMMAND_LISTEN=ATE0Q1S0=1<cr>
CONNECT=<match>"DIALIN_GATEWAY"
CONNECT=<?><?><?><?><hC0><h21><ignore>
CONNECT=<?><?><?><hC0><h21><ignore>
CONNECT=<?><?><hC0><h21><ignore>

;----------------------------------------
[Supra COM CARD 144 PCMCIA]
ALIAS=Megahertz XJack PCMCIA 144
DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=Supra Corporation
DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=RC144DPL

;----------------------------------------
[SupraModem 2400]
ALIAS=Hayes Compatible 2400

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=249
;----------------------------------------
[Supra Fax Modem 9624 Internal]
ALIAS=Hayes Compatible 2400

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=AFEP-C2501-H0
;----------------------------------------
[Supra Fax Modem V32]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=38400

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI5<cr>
DETECT_RESPONSE=Supra

COMMAND_INIT=AT&F2&C1&D2 V1 W1 Q0 S7=55 <cr>
COMMAND_INIT=AT S2=128 S11=55 S95=44 S0=0<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Supra Fax Modem V32bis]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=38400

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C3
<compression_off>=%C0
<protocol_on>=
;<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI5<cr>
DETECT_RESPONSE=Supra

COMMAND_INIT=AT&F2&C1&D2 S7=55 <cr>
COMMAND_INIT=ATS2=128 S11=55 S95=44 S0=0<speaker><cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Supra Fax Modem 288]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=28800
MAXCONNECTBPS=57600

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI5<cr>
DETECT_RESPONSE=Supra
DETECT_STRING=ATI<cr>
DETECT_RESPONSE=28800

COMMAND_INIT=AT&F2&C1&D2 S7=55 <cr>
COMMAND_INIT=ATS2=128 S11=55 S95=44 S0=0<speaker><cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Supra Fax Modem 288 internal]
ALIAS=Supra Fax Modem 288

DETECT_STRING=ATI5<cr>
DETECT_RESPONSE=Supra
DETECT_STRING=ATI<cr>
DETECT_RESPONSE=28800

;----------------------------------------
[Supra Fax Modem Plus]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=2400
MAXCONNECTBPS=9600

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=TR00
DETECT_STRING=ATI5<cr>
DETECT_RESPONSE=Supra

COMMAND_INIT=AT&F&C1&D2 V1 W1 Q0 <cr>
COMMAND_INIT=ATS7=55 S2=128 S11=55 S95=44 S0=0<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Telebit QBlazer]
;Not tested as a server modem.
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=38400

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=S58=2
<hwflowcontrol_off>=S58=0
<compression_on>=S190=1
<compression_off>=S190=0
<protocol_on>=S180=2
<protocol_off>=S180=0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=QBlazer

COMMAND_INIT=AT&F &C1 &D2 S0=0 S2=128 S7=55 S59=11 X4<cr>
COMMAND_INIT=AT <hwflowcontrol><compression><protocol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Telebit T1000]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=9600
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=FA2.10

COMMAND_INIT=AT~&F S53=1 S52=1 S58=0 S0=0 S55=3 S54=3 S7=55<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Telebit T1500]
;Server:untested
;This modem has not been tested as a server modem. This modem is not
;supported as a server modem.

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=9600

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=S58=2 S68=255
<hwflowcontrol_off>=S58=0 S68=255
<compression_on>=S97=1 S106=1 S98=0
<compression_off>=S98=0
<protocol_on>=S95=2 S96=1
<protocol_off>=S96=0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=T1500

COMMAND_INIT=AT~&F X13 S131=1 S52=1 S55=3<cr>
COMMAND_INIT=ATS110=0 S0=0 S55=3 S7=55<cr>
COMMAND_INIT=AT<speaker><hwflowcontrol><protocol><compression><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Telebit T1600]
;Advanced features are disabled

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=38400

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=S58=2
<hwflowcontrol_off>=S58=0
<compression_on>=S190=1
<compression_off>=S190=0
<protocol_on>=S180=2
<protocol_off>=S180=0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=T1600

COMMAND_INIT=AT&F &C1 &D2 S0=0 S2=128 S7=55 S59=11 X11 S58=0 S180=0 S181=0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Telebit T2000]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=2400
MAXCONNECTBPS=9600

<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=Version BC4.01

COMMAND_INIT=AT &F S52=1 S2=255 S0=0 S54=3 S7=55 S58=0 S180=0 S181=0<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Telebit T2500]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=19200

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=S58=2 S68=255
<hwflowcontrol_off>=S58=0 S68=255
<compression_on>=S96=1 S98=3
<compression_off>=S96=0 S98=0
<protocol_on>=S66=2 S95=2 S97=1 S106=1
<protocol_off>=S66=0 S95=0 S97=0 S106=0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=T2500

COMMAND_INIT=AT~&F <cr>
COMMAND_INIT=ATX14 S131=1 S52=1 S55=3 S55=3 S7=55 S50=6 S92=1<cr>
COMMAND_INIT=AT<compression><protocol><hwflowcontrol><speaker> S50=6 <cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Telebit T3000]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=19200
MAXCONNECTBPS=38400

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=S58=2 S68=255
<hwflowcontrol_off>=S58=0 S68=255
<compression_on>=S190=1 S180=2
<compression_off>=S190=0
<protocol_on>=S180=2
<protocol_off>=S180=0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=T3000

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT&C1&D2 X11 S0=0 S2=128 S7=55 S50=7 S59=9<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Telebit TrailBlazer Plus]
;PEP disabled with S50=3 S92=1. To re-enable PEP for 9600 baud
;connection with another Telebit, delete the string S50=3 S92=1.
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=19200

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=S58=2 S68=255
<hwflowcontrol_off>=S58=0 S68=255
<compression_off>=S98=0 S110=0
<compression_on>=S98=3
<protocol_on>=S97=1 S106=1 S95=2
<protocol_off>=S97=0 S106=0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=GF7.03-TBSA

COMMAND_INIT=AT~&F S52=4 S131=3<cr>
COMMAND_INIT=ATS51=255 S2=255 S0=0 S7=55 X3<cr>
COMMAND_INIT=AT<hwflowcontrol><compression><speaker>S50=3 S92=1<cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Telebit WorldBlazer]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=38400

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=S58=2 S68=255
<hwflowcontrol_off>=S58=0 S68=255
<compression_on>=S180=2 S190=1
<compression_off>=S190=0
<protocol_on>=S180=2 S190=0
<protocol_off>=S180=0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=WorldBlazer

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT&C1&D2 X11 S0=0 S2=128 S94=1 S92=1 S50=7<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Telebit WorldBlazer-Rackmount]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=38400

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=S58=2 S68=255
<hwflowcontrol_off>=S58=0 S68=255
<compression_on>=S180=2 S190=1
<compression_off>=S190=0
<protocol_on>=S180=2 S190=0
<protocol_off>=S180=0
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT&C1&D3 X11 S0=0 S2=128 S94=1 S92=1 S50=7<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker>Q0<cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[UDS Motorola CELLect 144]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=38400
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N7
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=AT%V<cr>
DETECT_RESPONSE=UDS CELLect 14.4

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT&C1&D2 \\V1 V3 S0=0 S2=128 S7=30<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[UDS Motorola FasTalk II]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=38400
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N6
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=UDS-144VBIS

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT&C1&D2 \\V1 V3 S0=0 S2=128 S7=30<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[UDS Motorola V.3225]

;Advanced features disabled.
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=9600
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=AT%V<cr>
DETECT_RESPONSE=V3225

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55 %C0 \\N1<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[UDS Motorola V.3227]
;Server:
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
;MAXCONNECTBPS set to 9600 for reasons of stability.
MAXCONNECTBPS=9600
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N7
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=AT%V<cr>
DETECT_RESPONSE=V.3227

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT&C1&D2 \\V1 S0=0 S2=128 S7=30<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[UDS Motorola V.3229]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=38400
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N7
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT&C1&D2 \\V1 S0=0 S2=128 S50=7 <cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[UDS Motorola FasTalk V.32/42b]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=9600
;Maxconnect set down to 9600 and advanced features disabled for stability.
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=AT%V<cr>
DETECT_RESPONSE=FASTALK V.32/42b

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT&C1&D2 \\V1 \\Q0 %C0 \\N0 S0=0 S2=128<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/REL<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/LAPM<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/REL<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/LAPM<cr><lf>

;----------------------------------------
[UDS Motorola V.3400]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=28800
MAXCONNECTBPS=57600
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N7
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=AT%V<cr>
DETECT_RESPONSE=V.3400

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT&C1&D2 \\V1 S0=0 S2=128 S7=30<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

[USRobotics General]

; This selection can be used by almost ALL USRobotics modems.
;
; A MAXCONNECTBPS of 38400 allows this to be used by older modems such
; as the HST 14400.
;
; Compression is off by default because of the lower DTE-DCE rate.
;
; ITU-T standards are on by default to ensure compatibility with
; non-USR modems.
;
; X4 is set to ensure compatibility with Sportster modems. Advanced
; dial features for Courier can be activated by placing X7 in the dial
; string. (e.g. phone number field contains "1-708-676-1059X7")

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=28800
MAXCONNECTBPS=38400
<speaker_on>=m1
<speaker_off>=m0
<hwflowcontrol_on>=&h1&r2
<hwflowcontrol_off>=&h0&r1
<compression_on>=&k3
<compression_off>=&k0
<protocol_on>=&m4
<protocol_off>=&m0
<autodial_on>=ATdt
<autodial_off>=ATd
;removed s47=2 because most of the newer modems don't support it
;COMMAND_INIT=AT&f&a3x4e1q0v1s0=0s7=55s2=128s47=2<cr>
COMMAND_INIT=AT&f&a3x4e1q0v1s0=0s7=55s2=128<cr>
COMMAND_INIT=AT&b1&c1&d2b0x4<hwflowcontrol><compression><protocol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[US Robotics Courier Dual]
ALIAS=US Robotics Courier V.32bis

DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=USRobotics Courier 16800 HST Dual
						
;----------------------------------------
[US Robotics Courier HST]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=USRobotics Courier 14400 HST

COMMAND_INIT=AT&F&C1&D2  V1 &B0 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[US Robotics Courier V.32bis]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=19200
MAXCONNECTBPS=38400

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&R2&H1
<hwflowcontrol_off>=&R1&H0
<compression_on>=&K1
<compression_off>=&K0
<protocol_on>=&M4
<protocol_off>=&M0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=USRobotics Courier V.32

COMMAND_INIT=ATE1&F&C1 &D2 &A1 &B1 V1 Q0 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><compression><protocol><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/ARQ<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/ARQ<cr><lf>


;----------------------------------------
[US Robotics Sportster 2400]
ALIAS=Hayes Compatible 2400

DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=SSi 73D2404
;----------------------------------------
[US Robotics Sportster 9600]

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=38400
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&H1&R2
<hwflowcontrol_off>=&H0&R1
<compression_on>=&K1
<compression_off>=&K0
<protocol_on>=&M4
<protocol_off>=&M0
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[US Robotics Sportster 14400]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=19200
MAXCONNECTBPS=38400
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&H1&R2
<hwflowcontrol_off>=&H0&R1
<compression_on>=&K1
<compression_off>=&K0
<protocol_on>=&M4
<protocol_off>=&M0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=Sportster 14,400

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker>&B1<cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=\
<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=\
<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ<cr><lf>

;----------------------------------------
[US Robotics V32bis Quad Digital]
ALIAS=US Robotics Sportster 14400

;----------------------------------------
[US Robotics Worldport 14400]
ALIAS=USR Worldport 14400 - UK
DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=WorldPort 14,400

;----------------------------------------
[US Robotics Sportster 28800 VFC]
ALIAS=USRobotics General

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=Sportster 28,800

;----------------------------------------
[US Robotics 288 PCMCIA]
ALIAS=USRobotics General

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=Sportster 28800
DETECT_RESPONSE=Sportster 33600
DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=Sportster PCMCIA 28800
DETECT_RESPONSE=Sportster PCMCIA 33600

;----------------------------------------
[US Robotics Sportster 28800 V34]
ALIAS=USRobotics General

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=Sportster 28800
DETECT_RESPONSE=Sportster 33600

;----------------------------------------
[Ven-Tel 9600 Plus II]
;Compression forced ON.
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATX3DT

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=38400

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=EC9600 Plus II

COMMAND_INIT=AT&F&C1&D2<cr>
COMMAND_INIT=AT V1 X4 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT \\Q3 \\N3 %C1 <cr>
COMMAND_INIT=AT<speaker> <cr>
COMMAND_DIAL=<autodial><phonenumber><cr>

CONNECT=<cr><lf>COMPRESSION NOT AVAILABLE<cr><lf>\
<cr><lf>CONNECT <carrierbps><cr><lf>

CONNECT=\
<cr><lf>CONNECT <carrierbps><cr><lf>

CONNECT=\
<cr><lf>COMPRESSION NOT AVAILABLE<cr><lf>\
<cr><lf>CONNECT <carrierbps> TRELLIS<cr><lf>

CONNECT=\
<cr><lf>CONNECT <carrierbps> TRELLIS<cr><lf>

CONNECT_EC=\
<cr><lf>COMPRESSION NOT AVAILABLE<cr><lf>\
<cr><lf>CONNECT <carrierbps> TRELLIS/LAPM<cr><lf>

CONNECT_EC=<cr><lf>CONNECT <carrierbps> TRELLIS/LAPM<cr><lf>

CONNECT_EC=\
<cr><lf>COMPRESS V.42bis<cr><lf><append>\
<cr><lf>CONNECT <carrierbps> TRELLIS<cr><lf>

CONNECT_EC=\
<cr><lf>COMPRESS V.42bis<cr><lf><append>\
<cr><lf>CONNECT <carrierbps> TRELLIS/LAPM<cr><lf>

CONNECT_EC=\
<cr><lf>COMPRESS V.42bis<cr><lf><append>\
<cr><lf>CONNECT <carrierbps> TRELLIS<cr><lf>

CONNECT_EC=\
<cr><lf>COMPRESS MNP5<cr><lf><append>\
<cr><lf>CONNECT <carrierbps> TRELLIS/LAPM<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>COMPRESSION NOT AVAILABLE<cr><lf>\
<cr><lf>CONNECT <carrierbps><cr><lf>

CONNECT=\
<cr><lf>CONNECT <carrierbps><cr><lf>

CONNECT=\
<cr><lf>COMPRESSION NOT AVAILABLE<cr><lf>\
<cr><lf>CONNECT <carrierbps> TRELLIS<cr><lf>

CONNECT=\
<cr><lf>CONNECT <carrierbps> TRELLIS<cr><lf>

CONNECT_EC=\
<cr><lf>COMPRESSION NOT AVAILABLE<cr><lf>\
<cr><lf>CONNECT <carrierbps> TRELLIS/LAPM<cr><lf>

CONNECT_EC=<cr><lf>CONNECT <carrierbps> TRELLIS/LAPM<cr><lf>

CONNECT_EC=\
<cr><lf>COMPRESS V.42bis<cr><lf><append>\
<cr><lf>CONNECT <carrierbps> TRELLIS<cr><lf>

CONNECT_EC=\
<cr><lf>COMPRESS V.42bis<cr><lf><append>\
<cr><lf>CONNECT <carrierbps> TRELLIS/LAPM<cr><lf>

CONNECT_EC=\
<cr><lf>COMPRESS V.42bis<cr><lf><append>\
<cr><lf>CONNECT <carrierbps> TRELLIS<cr><lf>

CONNECT_EC=\
<cr><lf>COMPRESS MNP5<cr><lf><append>\
<cr><lf>CONNECT <carrierbps> TRELLIS/LAPM<cr><lf>


;----------------------------------------
[Ven-Tel Pocket 24 V.42bis FAX]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C3
<compression_off>=%C0
<protocol_on>=&Q5
<protocol_off>=&Q0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=2400
MAXCONNECTBPS=9600

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=TR00

COMMAND_INIT=AT&F&C1&D2<cr>
COMMAND_INIT=AT V1 X4 S0=0 S2=128 S7=55 S95=44<cr>
;COMMAND_INIT=AT<speaker><hwflowcontrol><cr>
COMMAND_INIT=AT<speaker><hwflowcontrol><protocol><compression><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>


;----------------------------------------
[Ven-Tel 14400 Fax]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=&Q5
<protocol_off>=&Q0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=38400

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=TR14

COMMAND_INIT=AT&F&C1&D2<cr>
COMMAND_INIT=AT V1 X4 W0 S0=0 S2=128 S7=55 S95=44<cr>
COMMAND_INIT=AT<speaker><hwflowcontrol><compression><protocol><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Ven-Tel 14400 Fax Internal]
ALIAS=Ven-Tel 14400 Fax

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=TR14

;----------------------------------------
[Ven-Tel ECV 32bis II]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=%F0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=
MAXCARRIERBPS=14400
MAXCONNECTBPS=38400

DETECT_STRING=ATI<cr>
DETECT_RESPONSE=ECV.32bis II

COMMAND_INIT=AT&F&C1&D2<cr>
COMMAND_INIT=AT V1 X4 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<speaker><hwflowcontrol><compression><protocol><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>

CONNECT=<cr><lf>COMPRESSION NOT AVAILABLE<cr><lf>\
<cr><lf>CONNECT <carrierbps><cr><lf>

CONNECT=\
<cr><lf>CONNECT <carrierbps><cr><lf>

CONNECT=\
<cr><lf>COMPRESSION NOT AVAILABLE<cr><lf>\
<cr><lf>CONNECT <carrierbps> TRELLIS<cr><lf>

CONNECT=\
<cr><lf>CONNECT <carrierbps> TRELLIS<cr><lf>

CONNECT_EC=\
<cr><lf>COMPRESSION NOT AVAILABLE<cr><lf>\
<cr><lf>CONNECT <carrierbps> TRELLIS/LAPM<cr><lf>

CONNECT_EC=<cr><lf>CONNECT <carrierbps> TRELLIS/LAPM<cr><lf>

CONNECT_EC=<cr><lf>CONNECT <carrierbps> TRELLIS/LAPM<cr><lf>~<h0

CONNECT_EC=<cr><lf>CONNECT <carrierbps> TRELLIS/REL<cr><lf>

CONNECT_EC=\
<cr><lf>COMPRESS V.42bis<cr><lf><append>\
<cr><lf>CONNECT <carrierbps> TRELLIS<cr><lf>

CONNECT_EC=\
<cr><lf>COMPRESS V.42bis<cr><lf><append>\
<cr><lf>CONNECT <carrierbps> TRELLIS/LAPM<cr><lf>

CONNECT_EC=\
<cr><lf>COMPRESS V.42bis<cr><lf><append>\
<cr><lf>CONNECT <carrierbps> TRELLIS<cr><lf>

CONNECT_EC=\
<cr><lf>COMPRESS MNP5<cr><lf><append>\
<cr><lf>CONNECT <carrierbps> TRELLIS/LAPM<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>COMPRESSION NOT AVAILABLE<cr><lf>\
<cr><lf>CONNECT <carrierbps><cr><lf>

CONNECT=\
<cr><lf>CONNECT <carrierbps><cr><lf>

CONNECT=\
<cr><lf>COMPRESSION NOT AVAILABLE<cr><lf>\
<cr><lf>CONNECT <carrierbps> TRELLIS<cr><lf>

CONNECT=\
<cr><lf>CONNECT <carrierbps> TRELLIS<cr><lf>

CONNECT_EC=\
<cr><lf>COMPRESSION NOT AVAILABLE<cr><lf>\
<cr><lf>CONNECT <carrierbps> TRELLIS/LAPM<cr><lf>

CONNECT_EC=<cr><lf>CONNECT <carrierbps> TRELLIS/LAPM<cr><lf>

CONNECT_EC=<cr><lf>CONNECT <carrierbps> TRELLIS/LAPM<cr><lf>~<h0

CONNECT_EC=<cr><lf>CONNECT <carrierbps> TRELLIS/REL<cr><lf>

CONNECT_EC=\
<cr><lf>COMPRESS V.42bis<cr><lf><append>\
<cr><lf>CONNECT <carrierbps> TRELLIS<cr><lf>

CONNECT_EC=\
<cr><lf>COMPRESS V.42bis<cr><lf><append>\
<cr><lf>CONNECT <carrierbps> TRELLIS/LAPM<cr><lf>

CONNECT_EC=\
<cr><lf>COMPRESS V.42bis<cr><lf><append>\
<cr><lf>CONNECT <carrierbps> TRELLIS<cr><lf>

CONNECT_EC=\
<cr><lf>COMPRESS MNP5<cr><lf><append>\
<cr><lf>CONNECT <carrierbps> TRELLIS/LAPM<cr><lf>

;----------------------------------------
[ViVa 144 Fax]
ALIAS=Hayes Optima 14400

;----------------------------------------
[Western Datacom Worldcom]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N7
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=19200
MAXCONNECTBPS=38400

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=WESTERN DATACOM WORLDCOM

COMMAND_INIT=AT&F&C1&D2<cr>
COMMAND_INIT=AT V1 W1 X4 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: MNP REL<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: V42<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: V42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: ALT<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: MNP REL<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: V42<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: V42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: ALT<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf><cr><lf>

CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>

;Not supported as a server modem.
COMMAND_LISTEN=ATS0=1<cr>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: MNP REL<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: V42<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: V42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: ALT<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: MNP REL<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: V42<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: V42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: ALT<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf><cr><lf>

CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>

;----------------------------------------
[Xircom Ethernet+Modem PCMCIA]
<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=&Q0
<protocol_on>=&Q5
<compression_off>=S46=136
<compression_on>=S46=2
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATX3D

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=19200
MAXCONNECTBPS=38400

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=CreditCard Ethernet+Modem

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Zoom AFX]
ALIAS=Hayes Compatible 2400

;----------------------------------------
[Zoom FX 9624V]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=2400
MAXCONNECTBPS=9600

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=096

COMMAND_INIT=AT&F&C1&D2<cr>
COMMAND_INIT=AT V1 X4 S0=0 S2=128 S7=55 S95=44<cr>
COMMAND_INIT=AT<speaker><hwflowcontrol><compression><protocol><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Zoom VFX V.32bis]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=&Q5
<protocol_off>=&Q0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=38400

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=VFX14.4
DETECT_RESPONSE=TR14

COMMAND_INIT=AT&F&C1&D2<cr>
COMMAND_INIT=AT V1 X4 S0=0 S2=128 S7=55 S95=44 <cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Zoom VFP 28.8 internal]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C3
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=28800
MAXCONNECTBPS=57600

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=VFP
DETECT_RESPONSE=VFC
DETECT_STRING=ATI<cr>
DETECT_RESPONSE=28800

COMMAND_INIT=AT&F&C1&D2<cr>
COMMAND_INIT=AT V1 W1 X4 S0=0 S2=128 S7=55 S95=44 <cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: ALT<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: ALT<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

;----------------------------------------
[ZyXel U-1496]
;Cannot toggle EC and DC entirely independently in ZyXel.
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&H3
<hwflowcontrol_off>=&H0
<compression_on>=&K4
<compression_off>=&K0
<protocol_on>=&K3
<protocol_off>=&K0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=
MAXCARRIERBPS=19200
MAXCONNECTBPS=38400

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=1496

COMMAND_INIT=AT&F&C1&D2<cr>
COMMAND_INIT=ATV1 X5 S0=0S2=128 S7=55 S35=2<cr>
COMMAND_INIT=AT<speaker><hwflowcontrol><protocol><compression><cr>
COMMAND_LISTEN=ATS0=1<cr>
COMMAND_DIAL=<autodial><phonenumber><cr>

;----------------------------------------
[ZyXel U-1496B]
ALIAS=ZyXel U-1496

;----------------------------------------
[ZyXel U-1496E]
ALIAS=ZyXel U-1496
DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=1496E

;----------------------------------------
[ZyXel U-1496]
ALIAS=ZyXel U-1496

;----------------------------------------
[ZyXel U-1496E+]
ALIAS=ZyXel U-1496

;----------------------------------------
[ZyXel U-1496B+]
ALIAS=ZyXel U-1496

;----------------------------------------
[ZyXel U-1496+]
ALIAS=ZyXel U-1496

;----------------------------------------
[ZyXel U-1496P]
ALIAS=ZyXel U-1496

;----------------------------------------
; UK MODEMS
;----------------------------------------

;----------------------------------------
[Hayes Ultra 14400 - UK]
ALIAS=Hayes Optima 14400

;----------------------------------------
[Smartlink Pocket 2400 - UK]
ALIAS=Hayes Compatible 2400

;----------------------------------------
[Smartlink V32Bis/Fax - UK]
CALLBACKTIME=30
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=19200

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C3
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT&F.
COMMAND_INIT=AT&C1&D2 \\V1 X1 W2 Q0 S0=0 S2=128 S7=60<cr>
COMMAND_INIT=AT<speaker><compression><hwflowcontrol><protocol><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/REL<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/REL<cr><lf>

;----------------------------------------
[Dataflex Rapier+ V32Bis - UK]
CALLBACKTIME=30
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=19200

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C3
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT&F&C1&D2Q0V1E1\\J1S0=0S2=128 S7=55<cr>
COMMAND_INIT=AT<speaker><compression><hwflowcontrol><protocol><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>

;----------------------------------------
[Psion Dacom PDM 50F - UK]
CALLBACKTIME=30
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=19200

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C3
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT&F&C1&D2Q0V1E1S0=0S2=128 S7=55<cr>
COMMAND_INIT=AT<speaker><compression><hwflowcontrol><protocol><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>

;----------------------------------------
;Please note that this modem does NOT support 14,400bps DTE speed.
[Andest Rocket - UK]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=$F4
<hwflowcontrol_off>=$F5
<compression_on>=$C1
<compression_off>=$C0
<protocol_on>=$E3
<protocol_off>=$E0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=30
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F&C1&D2 $X2 V1 S0=0 S2=128 S7=60<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps> ALT<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps> ALT /MNP 5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps> LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps> LAPM /V.42bis<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps> ALT<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps> ALT /MNP 5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps> LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps> LAPM /V.42bis<cr><lf>

;----------------------------------------
[Intel SatisFaxtion - UK]
ALIAS=Hayes Compatible 2400

;---------------------------------------------------------------------------
; This modem does not support callback when connecting to MS RAS 1.x Servers
;---------------------------------------------------------------------------
[USR Worldport 14400 - UK]
CALLBACKTIME=30
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=19200

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&R2&H1
<hwflowcontrol_off>=&R1&H0
<compression_on>=&K1
<compression_off>=&K0
<protocol_on>=&M4
<protocol_off>=&M0
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT&F&C1 &D2 &A3 &B1 V1 Q0 S0=0 S2=128 S7=60<cr>
COMMAND_INIT=AT<hwflowcontrol><compression><protocol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>

CONNECT=\
<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/NONE<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/V32/NONE<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/V32<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/LAPM<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/LAPM/V42BIS<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/V32/LAPM<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/V32/LAPM/V42BIS<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/MNP<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/MNP/MNP5<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/V32/MNP<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/V32/MNP/MNP5<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>

CONNECT=\
<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/NONE<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/V32/NONE<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/V32<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/LAPM<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/LAPM/V42BIS<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/V32/LAPM<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/V32/LAPM/V42BIS<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/MNP<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/MNP/MNP5<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/V32/MNP<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/V32/MNP/MNP5<cr><lf>


;----------------------------------------
; SWEDISH MODEMS
;----------------------------------------

;----------------------------------------
[GVC SM2400 - SWE]
ALIAS=Hayes Compatible 2400
;----------------------------------------
[GVC SM96 - SWE]
CALLBACKTIME=30
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=19200

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N6
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT&F&C1&D2Q0V1E1S0=0S2=128S7=60<speaker><cr>
COMMAND_INIT=AT<compression><hwflowcontrol><protocol><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP/COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>
CONNECT=<cr><lf><cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf><cr><lf>CONNECT <carrierbps>/MNP<cr><lf>
CONNECT_EC=<cr><lf><cr><lf>CONNECT <carrierbps>/MNP/COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf><cr><lf>CONNECT <carrierbps>/MNP COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf><cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf><cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP/COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>
CONNECT=<cr><lf><cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf><cr><lf>CONNECT <carrierbps>/MNP<cr><lf>
CONNECT_EC=<cr><lf><cr><lf>CONNECT <carrierbps>/MNP/COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf><cr><lf>CONNECT <carrierbps>/MNP COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf><cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf><cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>

;----------------------------------------
[GVC FM14400 - SWE]
CALLBACKTIME=30
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=19200

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N6
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT&F&C1&D2Q0V1E1S0=0S2=128 S7=60 S95=44<cr>
COMMAND_INIT=AT<speaker><compression><hwflowcontrol><protocol><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP/COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP/COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>

;----------------------------------------
[Hidem 14400/FAX - SWE]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N6
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=30
DEFAULTOFF=compression
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F&C1&D2 \\V1 V1 W2S0=0 S2=128 S7=60 <cr>
COMMAND_INIT=AT<compression><hwflowcontrol><protocol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP4<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP4<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>

;----------------------------------------
;Hardware flow control and error correction are set ON for stability.
;For stability keep DTE at 9600bps.

[Hidem 2442P/FAX - SWE]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q3
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N7
<protocol_off>=\\N7

<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=30
DEFAULTOFF=compression
MAXCARRIERBPS=2400
MAXCONNECTBPS=9600
COMMAND_INIT=AT&F&C1&D2 \\V1 V1 X4S0=0 S2=128 S7=60 <cr>
COMMAND_INIT=AT<compression><hwflowcontrol><protocol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
ERROR_NO_CARRIER=<cr><lf><cr><lf>NO CARRIER<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP4<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
ERROR_NO_CARRIER=<cr><lf><cr><lf>NO CARRIER<cr><lf>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP4<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>


;----------------------------------------
[LASAT Unique 144 - SWE]
<speaker_on>=L2M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C2
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=30
DEFAULTOFF=speaker compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=19200
COMMAND_INIT=AT&F&C1&D2W1<cr>
COMMAND_INIT=AT V1 X4 S0=0 S2=128 S7=60<cr>
COMMAND_INIT=AT<speaker><hwflowcontrol><compression><protocol><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;---------------------------------------------------------------------------
; This modem does not support callback when connecting to MS RAS 1.x Servers
;---------------------------------------------------------------------------
[LIGHTFAX 1440LC - SWE]
CALLBACKTIME=15
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=14400
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT&F&C1&D2 E1 V1 W1 X4 S0=0 S7=60 S2=128<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>



;-------------------------------------------
[MultiTech MT932 - SWE]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&E4
<hwflowcontrol_off>=&E3
<compression_on>=&E15
<compression_off>=&E14
<protocol_on>=&E1
<protocol_off>=&E0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=30
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=19200

COMMAND_INIT=AT&SF1&S0&W<cr>
COMMAND_INIT=AT E1<cr>
COMMAND_INIT=AT &F &C1 V1 &D2 &Q0 X4 &S0 S0=0 S2=128 S7=60 $BA0<cr>
COMMAND_INIT=AT<compression><hwflowcontrol><protocol><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM COMPRESSED<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> RELIABLE COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps> LAPM COMPRESSED<cr><lf>

;------------------------------------------------------------------------
; Hardware flow control and error correction are set ON for stability.
;
; Connecting to modems with Advanced features may fail due to Guard tone
; feature.
;------------------------------------------------------------------------
[UCOM FASTLINK 144 - SWE]
<speaker_on>=L2M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K3
<compression_on>=%C2
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N3
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=30
DEFAULTOFF=speaker compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=14400
COMMAND_INIT=AT&F&C1&D2N0&G0W1<cr>
COMMAND_INIT=AT V1 X4 S0=0 S2=128 S7=60<cr>
COMMAND_INIT=AT<speaker><hwflowcontrol><compression><protocol><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[UCOM TRAVELLER 144 - SWE]
alias=UCOM FASTLINK 144 - SWE

;----------------------------------------
[UDS Motorola FasTalk V32- SWE]
CALLBACKTIME=20
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=9600
;Maxconnect set down to 9600 and advanced features disabled for stability.
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT&C1&D2 \\V1 \\Q0 %C0 \\N0 S0=0 S2=128<cr>
COMMAND_INIT=AT<speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/REL<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/LAPM<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/REL<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/LAPM<cr><lf>


;---------------------------------------------------------------------------
; Please note that this modem does NOT support 14,400bps DTE speed.
;---------------------------------------------------------------------------
; This modem does not support callback when connecting to MS RAS 1.x Servers
;---------------------------------------------------------------------------
[UFOMATE P1496MX - SWE]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=$F4
<hwflowcontrol_off>=$F5
<compression_on>=$C1
<compression_off>=$C0
<protocol_on>=$E3
<protocol_off>=$E0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=30
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F&C1&D2 $X2 V1 S0=0 S2=128 S7=60<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps> ALT<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps> ALT /MNP 5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps> LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps> LAPM /V.42bis<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps> ALT<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps> ALT /MNP 5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps> LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps> LAPM /V.42bis<cr><lf>


;----------------------------------------
[USR Courier V.32bis - SWE]
CALLBACKTIME=30
DEFAULTOFF=compression
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&R2&H1
<hwflowcontrol_off>=&R1&H0
<compression_on>=&K1
<compression_off>=&K0
<protocol_on>=&M4
<protocol_off>=&M0
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT&F&C1 &D2 &A1 &B1 V1 Q0 S0=0 S2=128 S7=60<cr>
COMMAND_INIT=AT<hwflowcontrol><compression><protocol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/ARQ<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/ARQ<cr><lf>

;----------------------------------------
;Please note that this modem does NOT support 14,400bps DTE speed.
[USR Sportster 14400 - SWE]
CALLBACKTIME=30
DEFAULTOFF=compression
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&H1&R2
<hwflowcontrol_off>=&H0&R1
<compression_on>=&K1
<compression_off>=&K0
<protocol_on>=&M4
<protocol_off>=&M0
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT&F&C1&D2 &A3V1 S0=0 S2=128 S7=60<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker>&B1<cr>
COMMAND_DIAL=<autodial><phonenumber><cr>

CONNECT=\
<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/NONE<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/V32/NONE<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/V32<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/LAPM<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/LAPM/V42BIS<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/V32/LAPM<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/V32/LAPM/V42BIS<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/MNP<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/MNP/MNP5<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/V32/MNP<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/V32/MNP/MNP5<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>

CONNECT=\
<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/NONE<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/V32/NONE<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/V32<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/LAPM<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/LAPM/V42BIS<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/V32/LAPM<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/V32/LAPM/V42BIS<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/MNP<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/MNP/MNP5<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/V32/MNP<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/V32/MNP/MNP5<cr><lf>

;----------------------------------------
[USR Worldport 14400 - SWE]
CALLBACKTIME=30
DEFAULTOFF=compression
MAXCARRIERBPS=19200
MAXCONNECTBPS=19200

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&R2&H1
<hwflowcontrol_off>=&R1&H0
<compression_on>=&K1
<compression_off>=&K0
<protocol_on>=&M4
<protocol_off>=&M0
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT&F&C1 &D2 &A3 &B1 V1 Q0 S0=0 S2=128 S7=60<cr>
COMMAND_INIT=AT<hwflowcontrol><compression><protocol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>

CONNECT=\
<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/NONE<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/V32/NONE<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/V32<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/LAPM<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/LAPM/V42BIS<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/V32/LAPM<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/V32/LAPM/V42BIS<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/MNP<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/MNP/MNP5<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/V32/MNP<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/V32/MNP/MNP5<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>

CONNECT=\
<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/NONE<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/V32/NONE<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/V32<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/LAPM<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/LAPM/V42BIS<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/V32/LAPM<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/V32/LAPM/V42BIS<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/MNP<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/MNP/MNP5<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/V32/MNP<cr><lf>
CONNECT_EC=\
<cr><lf>CONNECT <carrierbps>/ARQ/V32/MNP/MNP5<cr><lf>


;----------------------------------------
[DYNALINK - SWE]
CALLBACKTIME=30
DEFAULTOFF=
MAXCARRIERBPS=14400
MAXCONNECTBPS=38400
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT&F&C1&D2 L3 V1 W1 S0=0 S2=43 S7=55 S95=5<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>

COMMAND_LISTEN=ATS0=1<cr>


[SBN 2314C - SWE]
CALLBACKTIME=30
DEFAULTOFF=
MAXCARRIERBPS=14400
MAXCONNECTBPS=14400
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT &F &D2  +Q3 V1 S0=1 S2=128 S7=60 <cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT=<cr><lf>CONNECT <carrierbps>/<connectbps><cr><lf>
CONNECT=<cr><lf>CONNECT <carrierbps>/<connectbps>/TCM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> V.42BIS<cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> V.42BIS/TCM<cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> V.42BIS/TCM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps>/ V.42BIS/TCM<cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> LAPM<cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> LAPM/TCM<cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> LAPM/TCM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps><cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps><cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT=<cr><lf>CONNECT <carrierbps>/<connectbps><cr><lf>
CONNECT=<cr><lf>CONNECT <carrierbps>/<connectbps>/TCM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> V.42BIS<cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> V.42BIS/TCM<cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> V.42BIS/TCM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps>/ V.42BIS/TCM<cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> LAPM<cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> LAPM/TCM<cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> LAPM/TCM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps><cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps><cr><lf>




[SEMAFOR 2324C - SWE]
CALLBACKTIME=30
DEFAULTOFF=
MAXCARRIERBPS=2400
MAXCONNECTBPS=9600
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT &F &D2 +Q2 V1 S0=1 S2=128 S7=60 +C1<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT=<cr><lf>CONNECT <carrierbps>/<connectbps><cr><lf>
CONNECT=<cr><lf>CONNECT <carrierbps>/<connectbps>/TCM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> V.42BIS<cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> V.42BIS/TCM<cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> V.42BIS/TCM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps>/ V.42BIS/TCM<cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> LAPM<cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> LAPM/TCM<cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> LAPM/TCM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps><cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps><cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT=<cr><lf>CONNECT <carrierbps>/<connectbps><cr><lf>
CONNECT=<cr><lf>CONNECT <carrierbps>/<connectbps>/TCM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> V.42BIS<cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> V.42BIS/TCM<cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> V.42BIS/TCM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps>/ V.42BIS/TCM<cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> LAPM<cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> LAPM/TCM<cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> LAPM/TCM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps><cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps><cr><lf>

[SEMAFOR 1496A - SWE]
CALLBACKTIME=30
DEFAULTOFF=
MAXCARRIERBPS=9600
MAXCONNECTBPS=9600
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT &F &D2  +Q3 V1 S0=1 S2=128 S7=60 <cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT=<cr><lf>CONNECT <carrierbps>/<connectbps><cr><lf>
CONNECT=<cr><lf>CONNECT <carrierbps>/<connectbps>/TCM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> V.42BIS<cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> V.42BIS/TCM<cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> V.42BIS/TCM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps>/ V.42BIS/TCM<cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> LAPM<cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> LAPM/TCM<cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> LAPM/TCM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps><cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps><cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT=<cr><lf>CONNECT <carrierbps>/<connectbps><cr><lf>
CONNECT=<cr><lf>CONNECT <carrierbps>/<connectbps>/TCM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> V.42BIS<cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> V.42BIS/TCM<cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> V.42BIS/TCM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps>/ V.42BIS/TCM<cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> LAPM<cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> LAPM/TCM<cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps> LAPM/TCM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps><cr><lf><h11>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL/<connectbps><cr><lf>
;----------------------------------------

;----------------------------------------
;   AUSTRALIAN MODEMS
;----------------------------------------

;----------------------------------------
[Avtek CD900 - AUS]

CALLBACKTIME=30
DEFAULTOFF=compression
MAXCARRIERBPS=2400
MAXCONNECTBPS=2400

<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT&F+C61B0X1&C1&D2 S0=0 S7=60<speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/ARP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>

COMMAND_LISTEN=ATS0=2<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/ARP<cr><lf>



;--------------------------------------
; This modem does not support callback
;--------------------------------------
[Avtek CD930 - AUS]

<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=\\N0
<protocol_on>=\\N3
<compression_off>=%C0
<compression_on>=%C3
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATX1D

CALLBACKTIME=30
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=9600

COMMAND_INIT=AT&F&C1&D2 X1 W2 S0=0 S2=128 S7=60<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
LOOP=<cr><lf>RINGING<cr><lf>
COMMAND_LISTEN=ATS0=2<cr>
LOOP=<cr><lf>RINGING<cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: LAP-M/HDX<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: LAP-M/HDX<cr><lf>\
<cr><lf>COMPRESSION: MNP5<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: MNP5<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: LAP-M/HDX<cr><lf>\
<cr><lf>COMPRESSION: MNP4<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: MNP4<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps>/ARQ<cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: LAP-M/HDX<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>


;--------------------------------------
; This modem does not support callback
;--------------------------------------
[Banksia XM124/R FAXMODEM- AUS]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=30

MAXCARRIERBPS=2400
MAXCONNECTBPS=2400
DEFAULTOFF=compression
COMMAND_INIT=AT&F&C1&D2 S0=0 V1 X1 S2=128 S7=60<speaker><cr>
COMMAND_LISTEN=ATS0=2<cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/ARP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>

COMMAND_LISTEN=ATS0=2<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/ARP<cr><lf>

;----------------------------------------

[Banksia MX-6 V.32bis - AUS]
<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=\\N0
<protocol_on>=\\N3
<compression_off>=%C0
<compression_on>=%C3
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=30
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F&C1&D2 X1 V1 N1 S0=0 S7=60<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><h5C>/ARQ<cr><lf>\
CONNECT_EC=<cr><lf>CONNECT <connectbps><h5C>/ARQ<cr><lf>\

COMMAND_LISTEN=ATS0=2<cr>
CONNECT=<cr><lf>CONNECT <connectbps><h5C>/ARQ<cr><lf>\
CONNECT_EC=<cr><lf>CONNECT <connectbps><h5C>/ARQ<cr><lf>\

; V.42BIS Compression with Protocol ALT,MNP5,LAP-M,MNP4,MNP3,MNP2,NONE

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>PROTOCOL: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>PROTOCOL: MNP2<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>PROTOCOL: MNP3<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>PROTOCOL: MNP4<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>PROTOCOL: MNP5<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>COMPRESSION: VVV.42BIS<cr><lf>\
<cr><lf>PROTOCOL: ALT<cr><lf>\
<cr><lf>CONNECT <connectbps>/ARQ<cr><lf>

; End of compression for V.42bis

; CLASS5 Compression with Protocol ALT,MNP5,LAP-M,MNP4,MNP3,MNP2,NONE

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>COMPRESSION: CLASS5<cr><lf>\
<cr><lf>PROTOCOL: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>COMPRESSION: CLASS5<cr><lf>\
<cr><lf>PROTOCOL: MNP2<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>COMPRESSION: CLASS5<cr><lf>\
<cr><lf>PROTOCOL: MNP3<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>COMPRESSION: CLASS5<cr><lf>\
<cr><lf>PROTOCOL: MNP4<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>COMPRESSION: CLASS5<cr><lf>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>COMPRESSION: CLASS5<cr><lf>\
<cr><lf>PROTOCOL: MNP5<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>COMPRESSION: CLASS5<cr><lf>\
<cr><lf>PROTOCOL: ALT<cr><lf>\
<cr><lf>CONNECT <connectbps>/ARQ<cr><lf>

; End of compression for CLASS5 Compression.

; NONE Compression with Protocol ALT,MNP5,LAP-M,MNP4,MNP3,MNP2,NONE

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>PROTOCOL: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>PROTOCOL: MNP2<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>PROTOCOL: MNP3<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>PROTOCOL: MNP4<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>PROTOCOL: MNP5<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>PROTOCOL: ALT<cr><lf>\
<cr><lf>CONNECT <connectbps>/ARQ<cr><lf>


; End of compression for NONE Compression.

;----------------------------------------

[Maestro RC224FMI - AUS]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=30
DEFAULTOFF=compression
MAXCARRIERBPS=2400
MAXCONNECTBPS=2400

COMMAND_INIT=AT&F&C1&D2 V1 X1 S0=0 S2=128 S7=55<speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/ARP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>

COMMAND_LISTEN=ATS0=2<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/ARP<cr><lf>

;----------------------------------------

[Maestro 144FMEI - AUS]
<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=\\N0
<protocol_on>=\\N3
<compression_off>=%C0
<compression_on>=%C1
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=30
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F&C1&D2 X1 S0=0 S2=128 S7=60 <speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/ARP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>

COMMAND_LISTEN=ATS0=2<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/ARP<cr><lf>

;------------------------------------------------------

[Netcomm Pocket Rocket PA- AUS]
<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=\\N0
<protocol_on>=\\N3
<compression_off>=%C0
<compression_on>=%C3
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=30
DEFAULTOFF=compression
MAXCARRIERBPS=9600
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F&C1&D2 V1 X1 W1 S95=2 S0=0 S7=60<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/ARP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>

COMMAND_LISTEN=ATS0=2<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/ARP<cr><lf>

;----------------------------------------

[Netcomm Smartmodem E7F - AUS]
<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=\\N0
<protocol_on>=\\N3
<compression_off>=%C0
<compression_on>=%C3
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATX1D

CALLBACKTIME=30
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F.
COMMAND_INIT=AT&C1&D2 X1 \\V1 Q0 S0=0 S7=60<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>

CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/ARP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>

COMMAND_LISTEN=ATS0=2<cr>

CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/ARP<cr><lf>

;---------------------------------------------

[Netcomm Pocket M/F 2400-AUS]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=30
DEFAULTOFF=compression
MAXCARRIERBPS=2400
MAXCONNECTBPS=2400

COMMAND_INIT=AT&F&C1&D2 V1 X1 S0=0 S2=128 S7=55<speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>

CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/ARP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>

COMMAND_LISTEN=ATS0=2<cr>

CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/ARP<cr><lf>


;----------------------------------------
; German Modems
;----------------------------------------




;-----------------
; ComCom - Modems
;-----------------

[ComCom Spirit II - GER]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=*F3
<hwflowcontrol_off>=*F0
<compression_on>=*E9
<compression_off>=
<protocol_on>=*E5
<protocol_off>=*E0
<autodial_on>=ATDP
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=38400

DETECT_STRING=AT*O<cr>
DETECT_RESPONSE=MODEL:SPIRIT II

COMMAND_INIT=AT&F&C1&D2 X3 V1 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT*M1<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[ComCom Spirit TERBO - GER]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=*F3
<hwflowcontrol_off>=*F0
<compression_on>=*E9
<compression_off>=
<protocol_on>=*E5
<protocol_off>=*E0
<autodial_on>=ATDP
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=19200
MAXCONNECTBPS=38400

DETECT_STRING=AT*O<cr>
DETECT_RESPONSE=MODEL:SPIRIT TERBO

COMMAND_INIT=AT&F&C1&D2 X3 V1 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT*M1<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[Compaq SpeedPAQ 144 - GER]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<protocol_on>=\\N3
<protocol_off>=\\N0
<compression_on>=%C1
<compression_off>=%C0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=19200
MAXCONNECTBPS=38400

DETECT_STRING=ATI9<cr>
DETECT_RESPONSE=Compaq

COMMAND_INIT=AT&F&C1&D2 V1 W2S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>


;----------------------------------------
; Creatix Polymedia Modems
;----------------------------------------

[Creatix LC144VF - GER]
<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=\\N0
<protocol_on>=\\N3
<compression_off>=%C0
<compression_on>=%C3
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=57600

DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=Creatix Polymedia GmbH  V1.41  29/11/93
DETECT_RESPONSE=Creatix Polymedia GmbH  V1.5  27/05/94

COMMAND_INIT=AT&F0 W1 S95=46 S7=55 S2=128<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>



;----------------------------------------
[Creatix LC288FC - GER]
<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=\\N0
<protocol_on>=\\N3
<compression_off>=%C0
<compression_on>=%C3
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=28800
MAXCONNECTBPS=115200

DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=Creatix Polymedia GmbH  V0.51  01/05/94

COMMAND_INIT=AT&F0 W1 S95=46 S7=55 S2=128<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;==============
; CTK - Modems
;==============

[CTK SHORTY 144 SL - GER]

DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=FM-VBIS+/R1 V3.1s
DETECT_RESPONSE=PICO T 14.4-<?><?><?><?><?><?>-D-LL

CALLBACKTIME=30
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=19200

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N6
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT&F2X3&C1&D2Q0V1E1S0=0S2=128 S7=60 <cr>
COMMAND_INIT=AT<speaker><compression><hwflowcontrol><protocol><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP/COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP/COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>


;----------------------------------------
; Dr. Neuhaus Modems
;
; Alle folgenden Einstellungen haben in der INIT-Zeile
; COMMAND_INIT den Parameter W0 eingetragen. Das bedeu-
; tet, daá in der Connectmeldung immer die Datenrate
; zwischen dem Modem und dem Rechner angegeben wird.
; Hierdurch, und durch die Einstellung insgesamt, wird
; immer der maximal m”gliche Transferrate (ohne Umschalten)
; erreicht. Auch dann, wenn die Gegenstation evtl. nur mit
; niedrigeren Raten arbeitet.
;
;----------------------------------------
[Dr Neuhaus Fury 14400 TI - GER]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD
<compression_on>=
<compression_off>=
<protocol_on>=\\N6
<protocol_off>=\\N0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
CALLBACKTIME=30
DEFAULTOFF=
MAXCARRIERBPS=38400
MAXCONNECTBPS=38400

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55 W0<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/REL<cr><lf>

;----------------------------------------
[Dr Neuhaus Fury 19200 TI - GER]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD
<compression_on>=
<compression_off>=
<protocol_on>=\\N6
<protocol_off>=\\N0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
CALLBACKTIME=30
DEFAULTOFF=
MAXCARRIERBPS=57600
MAXCONNECTBPS=57600

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55 W0<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/REL<cr><lf>

;----------------------------------------
[Dr Neuhaus Smarty 144 TI - GER]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD
<compression_on>=
<compression_off>=
<protocol_on>=\\N6
<protocol_off>=\\N0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
CALLBACKTIME=30
DEFAULTOFF=
MAXCARRIERBPS=38400
MAXCONNECTBPS=38400

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55 W0<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/REL<cr><lf>

;----------------------------------------
[Dr Neuhaus Smarty 24 TI - GER]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD
<compression_on>=
<compression_off>=
<protocol_on>=
<protocol_off>=
<hwflowcontrol_on>=
<hwflowcontrol_off>=
CALLBACKTIME=30
DEFAULTOFF=
MAXCARRIERBPS=9600
MAXCONNECTBPS=9600

; Bevorzugte Einstellung: V42-Betrieb
COMMAND_INIT=AT&F3 V1 S0=0 S2=128 S7=55 W0<cr>
; Auch m”glich: MNP5-Betrieb
; COMMAND_INIT=AT&F2 V1 S0=0 S2=128 S7=55 W0<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/REL<cr><lf>



[Dr Neuhaus Fury Card 24 - GER]
alias=Dr Neuhaus Smarty 24 TI - GER
[Dr Neuhaus Fury Card 144 - GER]
alias=Dr Neuhaus Smarty 144 TI - GER
[Dr Neuhaus SMARTY 19200 - GER]
alias=Dr Neuhaus FURY 19200 TI - GER

;----------------------------------------
[Dr Neuhaus Niccy 3000 TI - GER]
; obwohl dieses Modem eigentlich in die Gruppe ISDN geh”ren
; k”nnte, wird es genau wie ein Modem angesprochen:

<speaker_on>=
<speaker_off>=
<autodial_on>=ATDT
<autodial_off>=ATD
<compression_on>=
<compression_off>=
<protocol_on>=
<protocol_off>=
<hwflowcontrol_on>=
<hwflowcontrol_off>=
CALLBACKTIME=30
DEFAULTOFF=
MAXCARRIERBPS=38400
MAXCONNECTBPS=38400

COMMAND_INIT=AT<cr>
COMMAND_INIT=AT&C1&D2\\Q3<cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>
CONNECT_EC=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>

;----------------------------------------
[Dr Neuhaus Fury 2403 TI - GER]
<speaker_on>=M1
<speaker_off>=M0
<autodial_on>=ATDT
<autodial_off>=ATD
<compression_on>=&Q5
<compression_off>=&Q0
<protocol_on>=
<protocol_off>=
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
CALLBACKTIME=30
DEFAULTOFF=
MAXCARRIERBPS=9600
MAXCONNECTBPS=9600

COMMAND_INIT=AT&F0&C1&D2 V1 S0=0 S2=128 S7=55 W1<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>


;--------------
; EEH - Modems
;--------------

[EEH Elink 32 - GER]
<hwflowcontrol_off>=\\Q0
<hwflowcontrol_on>=\\Q3
<protocol_off>=\\N0
<protocol_on>=\\N3
<compression_off>=%C0
<compression_on>=%C1
<speaker_off>=M0
<speaker_on>=M1

DETECT_STRING=ATI<cr>
DETECT_RESPONSE=Elink 32

CALLBACKTIME=30
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=57600

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT%C0 S2=128<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>
COMMAND_DIAL=ATD<phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/RELC<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42B<cr><lf>

[EEH Elink 32-3 analog - GER]
<hwflowcontrol_off>=\\Q0
<hwflowcontrol_on>=\\Q3
<protocol_off>=\\N0
<protocol_on>=\\N3
<compression_off>=%C0
<compression_on>=\\N3%C1
<speaker_off>=M0
<speaker_on>=M1

DETECT_STRING=ATI<cr>
DETECT_RESPONSE=Elink 32-3

CALLBACKTIME=30
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=115200

COMMAND_INIT=AT&F
COMMAND_INIT=X1 &B0 %C0 S2=128
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>
COMMAND_DIAL=ATD<phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/REL<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/RELC<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42B<cr><lf>


[EEH Elink 29-3 analog - GER]
<hwflowcontrol_off>=\\Q0
<hwflowcontrol_on>=\\Q3
<protocol_off>=\\N0
<protocol_on>=\\N3
<compression_off>=%C0
<compression_on>=\\N3%C1
<speaker_off>=M0
<speaker_on>=M1

DETECT_STRING=ATI<cr>
DETECT_RESPONSE=Elink 29-3

CALLBACKTIME=30
DEFAULTOFF=compression
MAXCARRIERBPS=2400
MAXCONNECTBPS=115200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=ATX1 &B0 %C0 S2=128<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>
COMMAND_DIAL=ATD<phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/REL<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/RELC<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42B<cr><lf>

[EEH Elink 301 - GER]
<hwflowcontrol_off>=\\Q0
<hwflowcontrol_on>=\\Q3
<protocol_off>=\\N0
<protocol_on>=\\N6
<compression_off>=M
<compression_on>=M
<speaker_off>=M0
<speaker_on>=M1

DETECT_STRING=ATI<cr>
DETECT_RESPONSE=ELINK 301

CALLBACKTIME=30
DEFAULTOFF=compression
MAXCARRIERBPS=64000
MAXCONNECTBPS=115200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=ATX1 \\N6 S12=128 S16=1<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>
COMMAND_DIAL=ATD<phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <connectbps>/V.110<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/X.75<cr><lf>

[EEH Elink 310 - GER]
<hwflowcontrol_off>=\\Q0
<hwflowcontrol_on>=\\Q3
<protocol_off>=&B34
<protocol_on>=&B49
<compression_off>=%C0
<compression_on>=%C1
<speaker_off>=M0
<speaker_on>=M1

DETECT_STRING=ATI<cr>
DETECT_RESPONSE=Elink 310

CALLBACKTIME=30
DEFAULTOFF=compression
MAXCARRIERBPS=64000
MAXCONNECTBPS=115200

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=ATX1 &B49 \\S1 S2=128<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>
COMMAND_DIAL=ATD<phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <connectbps>/V.110<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/X.75<cr><lf>

[EEH Elink 29-3 ISDN - GER]
ALIAS=EEH Elink 310 - GER

DETECT_STRING=ATI<cr>
DETECT_RESPONSE=Elink 29-3

[EEH Elink 32-3 ISDN - GER]
ALIAS=EEH Elink 310 - GER

DETECT_STRING=ATI<cr>
DETECT_RESPONSE=Elink 32-3


;----------------------------------------
;Elsa Modems (Germany)
;----------------------------------------

[ELSA MicroLink 2440T - GER]
<hwflowcontrol_off>=\\Q0
<hwflowcontrol_on>=\\Q3
<protocol_off>=\\N0
<protocol_on>=\\N3
<compression_off>=%C0
<compression_on>=%C3
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=30
DEFAULTOFF=
MAXCARRIERBPS=2400
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F$K0 X3 S0=0 S2=128 S7=55 S95=8\\V1<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL<cr><lf>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL<cr><lf>

DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=MicroLink 2440T


;----------------------------------------
[ELSA MicroLink 2440TR - GER]
ALIAS=ELSA MicroLink 2440T - GER
DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=MicroLink 2440TR

;----------------------------------------
[ELSA MicroLink 2460TL - GER]
<hwflowcontrol_off>=\\Q0
<hwflowcontrol_on>=\\Q3
<protocol_off>=\\N0
<protocol_on>=\\N3
<compression_off>=%C0
<compression_on>=%C3
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=30
DEFAULTOFF=
MAXCARRIERBPS=2400
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F$K0 X3 S0=0 S2=128 S7=55 S95=8\\V1<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL<cr><lf>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL<cr><lf>

DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=MicroLink 2460TL

;----------------------------------------
[ELSA MicroLink 2460PC - GER]
ALIAS=ELSA MicroLink 2460TL - GER

DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=MicroLink 2460TL

;----------------------------------------
[ELSA MicroLink 2460MC - GER]
ALIAS=ELSA MicroLink 2460TL - GER

DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=MicroLink 2460MC

;----------------------------------------
[ELSA MicroLink 14.4 PC - GER]
<hwflowcontrol_off>=\\Q0
<hwflowcontrol_on>=\\Q3
<protocol_off>=\\N0
<protocol_on>=\\N3
<compression_off>=%C0
<compression_on>=%C3
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=30
DEFAULTOFF=
MAXCARRIERBPS=14400
MAXCONNECTBPS=38400

DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=MicroLink 14.4PC

COMMAND_INIT=AT&F$K0 X3 S31=64 S0=0 S2=128 S7=55 S95=8\\V1<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL<cr><lf>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL<cr><lf>

;----------------------------------------
[ELSA MicroLink 14.4 TL - GER]
ALIAS=ELSA MicroLink 14.4 PC - GER
DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=MicroLink 14.4TL

;----------------------------------------
[ELSA MicroLink 14.4 T - GER]
ALIAS=ELSA MicroLink 14.4 PC - GER
DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=MicroLink 14.4T

;----------------------------------------
[ELSA MicroLink 14.4 TM - GER]
ALIAS=ELSA MicroLink 14.4 PC - GER
DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=MicroLink 14.4TM

;----------------------------------------
[ELISA 144 - GER]
ALIAS=ELSA MicroLink 14.4 PC - GER
DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=ELISA 144

;----------------------------------------
[ELSA MicroLink 288ooTL - GER]
<hwflowcontrol_off>=\\Q0
<hwflowcontrol_on>=\\Q3
<protocol_off>=\\N0
<protocol_on>=\\N3
<compression_off>=%C0
<compression_on>=%C3
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=30
DEFAULTOFF=
MAXCARRIERBPS=28800
MAXCONNECTBPS=115200

COMMAND_INIT=AT&F$K0 X3 S0=0 S2=128 S7=55 S31=64 S95=8\\V1<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL<cr><lf>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL<cr><lf>

DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=MicroLink 288ooTL

;----------------------------------------
[ELSA MicroLink 14.4MC - GER]
DEVICETYPE=modem
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=38400

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<protocol_on>=\\N3
<protocol_off>=\\N0
<compression_on>=%C3
<compression_off>=%C0
<autodial_on>=ATDT
<autodial_off>=ATX3D

COMMAND_INIT=AT&F&C1&D2 X3 W2 \\J0 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL<cr><lf>

DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=MicroLink 14.4MC

;----------------------------------------
[ELSA ZIFF 144 - GER]
ALIAS=ELSA MicroLink 14.4MC - GER

DETECT_STRING=ATI6<cr>
DETECT_RESPONSE=ZIFF 144

;----------------------------------------
[ELSA MicroLink ISDN/TL - GER]
<hwflowcontrol_off>=\\Q0
<hwflowcontrol_on>=\\Q3
<protocol_off>=\\N0
<protocol_on>=\\N6
<autodial_on>=ATD
<autodial_off>=ATD

CALLBACKTIME=30
DEFAULTOFF=
MAXCARRIERBPS=64000
MAXCONNECTBPS=57600

COMMAND_INIT=AT&FX3 S0=0 S2=128 \\V1<cr>
COMMAND_INIT=AT<protocol><hwflowcontrol><cr>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL<cr><lf>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL<cr><lf>

COMMAND_DETECT=ATI6<cr>
COMMAND_RESPONSE=MicroLink ISDN/TL

;-------------------------
; ICO Innovative - Modems
;-------------------------

[Telejet 14400 - GER]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=57600

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K
<protocol_on>=\\N5
<protocol_off>=\\N0
<compression_on>=%C3
<compression_off>=%C0
<autodial_on>=ATDP
<autodial_off>=ATD

DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=TELEJET High Speed FaxModem 14400
COMMAND_INIT=AT&F&D2X1Q0N1<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps><cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps><cr><lf>


;---------------------------------
;  KE Kommunikations-Elektronik
;---------------------------------

;----------------------------------------
[LOGEM 914 - GER]
CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=38400

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q2
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N2
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=Version 3.
DETECT_RESPONSE=Version 2.03

COMMAND_INIT=AT&F<cr>
COMMAND_INIT=AT&C2&D2Q0V1E1X1&I1%C1\\Q2S0=0S2=128 S7=55<cr>
COMMAND_INIT=AT<speaker><compression><hwflowcontrol><protocol><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
;CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
;CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL<cr><lf>
;CONNECT_EC=<cr><lf>CONNECT <carrierbps>/COMP<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
;CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
;CONNECT_EC=<cr><lf>CONNECT <carrierbps>/REL<cr><lf>
;CONNECT_EC=<cr><lf>CONNECT <carrierbps>/COMP<cr><lf>

;------------------------------------
[LOGEM 928 - GER]
ALIAS=LOGEM 914 - GER
MAXCARRIERBPS=28800
MAXCONNECTBPS=57600

;------------------------------------
[ke WorldBlazer - GER]
ALIAS=Telebit WorldBlazer

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=T3SA-WB-DEU


;----------------------------------------
[Hayes Optima 9600 - GER]
ALIAS=Hayes Optima 9600

;----------------------------------------
[Hayes Optima 14400 - GER]
ALIAS=Hayes Optima 14400

;----------------------------------------
[Hayes Ultra 9600 - GER]
ALIAS=Hayes Optima 9600

;----------------------------------------
[Hayes Ultra 14400 - GER]
ALIAS=Hayes Optima 14400

;----------------------------------------
;----------------------------------------
; Streetware Modems
;----------------------------------------
[Holmes 14.4 all models - GER]

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATX3D
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=
MAXCARRIERBPS=14400
MAXCONNECTBPS=57600
COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><compression><protocol><speaker><cr>
COMMAND_LISTEN=ATS0=2<cr>
COMMAND_DIAL=<autodial><phonenumber><cr>

;----------------------------------------
[Telelink IMS08 - GER]

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N7
<protocol_off>=\\N0
<autodial_on>=ATX3D
<autodial_off>=ATD

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=\
Copyright 1993, Telelink Communications Inc.<cr><lf>\
IMS-08 FAXLINE REV <?>.<?><?> (D)

CALLBACKTIME=10
DEFAULTOFF=
MAXCARRIERBPS=14400
MAXCONNECTBPS=57600
COMMAND_INIT=AT&F2&C1&D2 V1 S0=0 S2=128 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><compression><protocol><speaker><cr>
COMMAND_LISTEN=ATS0=2<cr>
COMMAND_DIAL=<autodial><phonenumber><cr>

;==============================
; ZyXEL Modems (international)
;==============================

[ZyXEL U-1496 Plus]
;Cannot toggle EC and DC entirely independently in ZyXel.
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&H3
<hwflowcontrol_off>=&H0
<protocol_on>=&K3
<protocol_off>=&K0
<compression_on>=&K4
<compression_off>=
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=compression
MAXCARRIERBPS=19200
MAXCONNECTBPS=57600

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=U1496S  V<?><?><?><?><?><?><?>P
DETECT_STRING=ATI1<cr>
DETECT_RESPONSE=U1496S  V<?><?><?><?><?><?><?>P


COMMAND_INIT=AT &F X5 S41.4=1<cr>
COMMAND_INIT=AT S2=128 S7=55<cr>
COMMAND_INIT=AT<speaker><hwflowcontrol><protocol><compression><cr>
COMMAND_LISTEN=ATS0=1<cr>
COMMAND_DIAL=<autodial><phonenumber><cr>

;----------------------------------------
[ZyXEL U-1496E]
ALIAS=ZyXEL U-1496 Plus
MAXCARRIERBPS=16800
DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=U1496E  V<?><?><?><?><?><?><?>M
DETECT_STRING=ATI1<cr>
DETECT_RESPONSE=U1496E  V<?><?><?><?><?><?><?>M

;----------------------------------------
[ZyXEL U-1496E Plus]
ALIAS=ZyXEL U-1496 Plus
DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=U1496E  V<?><?><?><?><?><?><?>P
DETECT_STRING=ATI1<cr>
DETECT_RESPONSE=U1496E  V<?><?><?><?><?><?><?>P

;----------------------------------------
[ZyXEL U-1496B]
ALIAS=ZyXEL U-1496 Plus
MAXCARRIERBPS=16800
DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=U1496B  V<?><?><?><?><?><?><?>M
DETECT_STRING=ATI1<cr>
DETECT_RESPONSE=U1496B  V<?><?><?><?><?><?><?>M

;----------------------------------------
[ZyXEL U-1496B Plus]
ALIAS=ZyXEL U-1496 Plus
DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=U1496B  V<?><?><?><?><?><?><?>P
DETECT_STRING=ATI1<cr>
DETECT_RESPONSE=U1496B  V<?><?><?><?><?><?><?>P

;----------------------------------------
[ZyXEL U-1496P]
ALIAS=ZyXEL U-1496 Plus
MAXCARRIERBPS=16800
DETECT_STRING=ATI1<cr>
DETECT_RESPONSE=U1496C  V<?><?><?><?><?><?><?>M

;----------------------------------------
[ZyXEL U-1496R]
ALIAS=ZyXEL U-1496 Plus
MAXCARRIERBPS=16800
DETECT_STRING=ATI1<cr>
DETECT_RESPONSE=U1496R  V<?><?><?><?><?><?><?>M

;----------------------------------------
[ZyXEL U-1496R Plus]
ALIAS=ZyXEL U-1496 Plus
DETECT_STRING=ATI1<cr>
DETECT_RESPONSE=U1496R  V<?><?><?><?><?><?><?>P

;----------------------------------------
[ZyXEL U-1496RN]
ALIAS=ZyXEL U-1496 Plus
MAXCARRIERBPS=16800
DETECT_STRING=ATI1<cr>
DETECT_RESPONSE=U1496RN V<?><?><?><?><?><?><?>M

;----------------------------------------
[ZyXEL U-1496RN plus]
ALIAS=ZyXEL U-1496 Plus
DETECT_STRING=ATI1<cr>
DETECT_RESPONSE=U1496RN V<?><?><?><?><?><?><?>P

;----------------------------------------
[ZyXEL U-1496SN Plus]
ALIAS=ZyXEL U-1496 Plus
DETECT_STRING=ATI1<cr>
DETECT_RESPONSE=U1496SN V<?><?><?><?><?><?><?>P

;----------------------------------------
; ZyXEL Modems (Germany)
;----------------------------------------

[ZyXEL U-1496G Plus - GER]
ALIAS=ZyXEL U-1496 Plus
DETECT_STRING=ATI1<cr>
DETECT_RESPONSE=U1496G

;----------------------------------------
[ZyXEL U-1496EG Plus - GER]
ALIAS=ZyXEL U-1496 Plus
DETECT_STRING=ATI1<cr>
DETECT_RESPONSE=U1496EG V<?><?><?><?><?><?><?>P

;----------------------------------------
[ZyXEL U-1496EG - GER]
ALIAS=ZyXEL U-1496 Plus
MAXCARRIERBPS=16800
DETECT_STRING=ATI1<cr>
DETECT_RESPONSE=U1496EG V<?><?><?><?><?><?><?>M


;====================================
;SWISSE-Modems
;====================================

;------------------------------------
; Martignoni Electronics AG - Modems
;------------------------------------

[M. Bullet ModemMan - CH]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=$F4
<hwflowcontrol_off>=$F5
<compression_on>=$C1
<compression_off>=$C0
<protocol_on>=$E3
<protocol_off>=$E0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=
MAXCARRIERBPS=14400
MAXCONNECTBPS=57600

DETECT_STRING=ATI1<cr>
DETECT_RESPONSE=P1496MX

COMMAND_INIT=AT&F&C1&D2 $X1 V1 S0=0<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[M. Bullet E1414MX - CH]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=$F4
<hwflowcontrol_off>=$F5
<compression_on>=$C1
<compression_off>=$C0
<protocol_on>=$E3
<protocol_off>=$E0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=
MAXCARRIERBPS=14400
MAXCONNECTBPS=57600

DETECT_STRING=ATI1<cr>
DETECT_RESPONSE=E1414MX

COMMAND_INIT=AT&F&C1&D2 $X1 V1 S0=0<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[M. Bullet PCMCIA 1414M - CH]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=$F4
<hwflowcontrol_off>=$F5
<compression_on>=$C1
<compression_off>=$C0
<protocol_on>=$E3
<protocol_off>=$E0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=
MAXCARRIERBPS=14400
MAXCONNECTBPS=57600

DETECT_STRING=ATI1<cr>
DETECT_RESPONSE=C1414AX

COMMAND_INIT=AT&F&C1&D2 $X1 V1 S0=0 X3<cr><cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[M. Bullet PC1414MX - CH]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=$F4
<hwflowcontrol_off>=$F5
<compression_on>=$C1
<compression_off>=$C0
<protocol_on>=$E3
<protocol_off>=$E0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=
MAXCARRIERBPS=14400
MAXCONNECTBPS=57600

DETECT_STRING=ATI1<cr>
DETECT_RESPONSE=PC1414MX

COMMAND_INIT=AT&F&C1&D2 $X1 V1 S0=0<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[M. Bullet ModemMan V.terbo - CH]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=$F4
<hwflowcontrol_off>=$F5
<compression_on>=$C1
<compression_off>=$C0
<protocol_on>=$E3
<protocol_off>=$E0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=
MAXCARRIERBPS=19200
MAXCONNECTBPS=57600

DETECT_STRING=ATI1<cr>
DETECT_RESPONSE=P192MX

COMMAND_INIT=AT&F&C1&D2 $X1 V1 S0=0<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[M. Bullet PC192MX V.terbo - CH]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=$F4
<hwflowcontrol_off>=$F5
<compression_on>=$C1
<compression_off>=$C0
<protocol_on>=$E3
<protocol_off>=$E0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=
MAXCARRIERBPS=19200
MAXCONNECTBPS=57600

DETECT_STRING=ATI1<cr>
DETECT_RESPONSE=PC192MX

COMMAND_INIT=AT&F&C1&D2 $X1 V1 S0=0<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[M. Bullet 100E V.34 - CH]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=$F4
<hwflowcontrol_off>=$F5
<compression_on>=$C1
<compression_off>=$C0
<protocol_on>=$E3
<protocol_off>=$E0
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=
MAXCARRIERBPS=28800
MAXCONNECTBPS=115200

DETECT_STRING=ATI1<cr>
DETECT_RESPONSE=BULLET 100E

COMMAND_INIT=AT&F&C1&D2 $X1 V1 S0=0<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[M. CashCom - CH]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C3
<compression_off>=%&C0
<protocol_on>=\\N3
<protocol_off>=\\N1
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=
MAXCARRIERBPS=14400
MAXCONNECTBPS=57600

DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=CashCom

COMMAND_INIT=AT&FW0S0=0<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=2<cr>

;----------------------------------------
[M. SpiderMan - CH]
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C3
<compression_off>=%&C0
<protocol_on>=\\N3
<protocol_off>=\\N1
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=10
DEFAULTOFF=
MAXCARRIERBPS=14400
MAXCONNECTBPS=57600

DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=SpiderMan

COMMAND_INIT=AT&FW0S0=0<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=2<cr>


;----------------------------------------
;AUSTRIAN MODEMS
;----------------------------------------
[ZyXEL U-1496A Plus - AUT]
ALIAS=ZyXEL U-1496 Plus
DETECT_STRING=ATI1<cr>
DETECT_RESPONSE=U1496S  V.AUST P

;----------------------------------------
[ZyXEL U-1496EA Plus - AUT]
ALIAS=ZyXEL U-1496 Plus
DETECT_STRING=ATI1<cr>
DETECT_RESPONSE=U1496E  V.AUST P

;----------------------------------------
[ZyXEL U-1496EA - AUT]
ALIAS=ZyXEL U-1496 Plus
MAXCARRIERBPS=16800
DETECT_STRING=ATI1<cr>
DETECT_RESPONSE=U1496E  V.AUST M

;----------------------------------------
[ZyXEL U-1496R Plus - AUT]
ALIAS=ZyXEL U-1496 Plus
DETECT_STRING=ATI1<cr>
DETECT_RESPONSE=U1496R  V.AUST P

;----------------------------------------
[ZyXEL U-1496R - AUT]
ALIAS=ZyXEL U-1496 Plus
MAXCARRIERBPS=16800
DETECT_STRING=ATI1<cr>
DETECT_RESPONSE=U1496R  V.AUST M

;----------------------------------------
[ZyXEL U-1496RN - AUT]
ALIAS=ZyXEL U-1496 Plus
MAXCARRIERBPS=16800
DETECT_STRING=ATI1<cr>
DETECT_RESPONSE=U1496RN V.AUST M



;----------------------------------------
; FRENCH MODEMS
;----------------------------------------

[Codex 326x - FRN]
ALIAS=Codex 3260

DETECT_STRING=AT&I0<cr>
DETECT_RESPONSE=6510

[Codex 326x FAST - FRN]
ALIAS=Codex 3260 Fast
DETECT_STRING=AT&I0<cr>
DETECT_RESPONSE=7061


;********** BOITIERS KORTEX KXPRO  ****************

[KORTEX KXPRO 9600 - FRN]
CALLBACKTIME=45
DEFAULTOFF=
MAXCARRIERBPS=9600
MAXCONNECTBPS=9600
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C3
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT&F&C1&D2 L3 V1 W1N0 X4 S0=0 S2=43 S7=55 S95=34<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP4<cr><lf>
CONNECT_EC=<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps>/ARQ<cr><lf>


COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP4<cr><lf>
CONNECT_EC=<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps>/ARQ<cr><lf>



[KORTEX KXPRO 144 POCKET - FRN]
alias=KORTEX KXPRO 144 BOX - FRN
DETECT_STRING=ATI<cr>
DETECT_RESPONSE=KORTEX KXPRO 144

[KORTEX NFX 144 POCKET - FRN]
alias=KORTEX KXPRO 144 BOX - FRN
DETECT_STRING=ATI<cr>
DETECT_RESPONSE=KORTEX NFX 144


[KORTEX KXPRO 144 BOX - FRN]
CALLBACKTIME=30
DEFAULTOFF=
MAXCARRIERBPS=14400
MAXCONNECTBPS=19200
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C3
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0\\G1
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI<cr>
DETECT_RESPONSE=KORTEX KXPRO 144


COMMAND_INIT=AT&FL3W0X4S0=2S95=40<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP4<cr><lf>
CONNECT_EC=<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps>/ARQ<cr><lf>

CONNECT_EC=<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>


COMMAND_LISTEN=ATS0=2<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP4<cr><lf>
CONNECT_EC=<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps>/ARQ<cr><lf>

CONNECT_EC=<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>




[KORTEX KXPOCKET 9600 - FRN]
alias=KORTEX KXPRO 9600 - FRN

[KORTEX KXPRO  2400 - FRN]
CALLBACKTIME=45
DEFAULTOFF=
MAXCARRIERBPS=2400
MAXCONNECTBPS=2400
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C3
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI<cr>
DETECT_RESPONSE=KORTEX KXPRO 2400

COMMAND_INIT=AT&F&C1&D2 L3 V1 W1N0 X4 S0=0 S2=43 S7=55 S95=34<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP4<cr><lf>
CONNECT_EC=<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps>/ARQ<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP4<cr><lf>
CONNECT_EC=<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps>/ARQ<cr><lf>

; ************** CARTES KORTEX *********************

[KORTEX NFX 144 CARTES - FRN]
alias=KORTEX KXPRO 144 CARTES - FRN
DETECT_STRING=ATI<cr>
DETECT_RESPONSE=KORTEX KXPRO 144


[KORTEX KXPRO 144 CARTES - FRN]
CALLBACKTIME=30
DEFAULTOFF=
MAXCARRIERBPS=14400
MAXCONNECTBPS=57600
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C3
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0\\G1
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI<cr>
DETECT_RESPONSE=KORTEX KXPRO 144


COMMAND_INIT=AT&FL3W0X4S0=2S95=40<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP4<cr><lf>
CONNECT_EC=<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps>/ARQ<cr><lf>

CONNECT_EC=<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>


COMMAND_LISTEN=ATS0=2<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP4<cr><lf>
CONNECT_EC=<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps>/ARQ<cr><lf>

CONNECT_EC=<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>



;******************************** Modems PNB ********************************

[PNB Baby RIO 14400 - FRN]
CALLBACKTIME=45
DEFAULTOFF=
MAXCARRIERBPS=14400
MAXCONNECTBPS=14400
<speaker_on>=M1
<speaker_off>=M0
;<hwflowcontrol_on>=  Keep the default value
;<hwflowcontrol_off>=  Keep the default value
<hwflowcontrol_on>=
<hwflowcontrol_off>=
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=43 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP4<cr><lf>


COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP4<cr><lf>

[PNB AMAZONE 2400 - FRN]
CALLBACKTIME=45
DEFAULTOFF=
MAXCARRIERBPS=2400
MAXCONNECTBPS=2400
<speaker_on>=M1
<speaker_off>=M0
;<hwflowcontrol_on>=  Keep the default value
;<hwflowcontrol_off>=  Keep the default value
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT&F&C1&D2V1S0=0 S2=43S7=55 \\V1<cr>
;OK=<cr><lf>Direct [unbuffered] Link<cr><lf><cr><lf>OK<cr><lf>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT=<cr><lf>CONNECT <carrierbps>/REL<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP4<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT=<cr><lf>CONNECT <carrierbps>/REL<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP4<cr><lf>


;******************* Modem Anderson Jacobson CXR ***************

[AJ 2423 - FRN]
CALLBACKTIME=45
DEFAULTOFF=
MAXCARRIERBPS=2400
MAXCONNECTBPS=19200
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=*LG2
<hwflowcontrol_off>=*LG0
<compression_on>=*E1
<compression_off>=*E0
<protocol_on>=*T3
<protocol_off>=*M1
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=AJ2423


COMMAND_INIT=AT&F&C1*M2&D0S0=0S2=43S7=55X4V1Q0<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP4<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/LAPM<cr><lf>


COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP4<cr><lf>

[AJ 1445/1446 - FRN]
CALLBACKTIME=45
DEFAULTOFF=
MAXCARRIERBPS=9600
MAXCONNECTBPS=19200
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=*LG2
<hwflowcontrol_off>=*LG0
<compression_on>=*E1
<compression_off>=*E0
<protocol_on>=*T3
<protocol_off>=*M1
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=AJ 1445
DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=AJ 1446


COMMAND_INIT=AT&F&C1*M2&D2S0=0S2=43S7=55X4V1Q0<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP4<cr><lf>


COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP4<cr><lf>


[AJ 9636 - FRN]
CALLBACKTIME=45
DEFAULTOFF=
MAXCARRIERBPS=9600
MAXCONNECTBPS=19200
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=*LG2
<hwflowcontrol_off>=*LG0
<compression_on>=*E1
<compression_off>=*E0
<protocol_on>=*T3
<protocol_off>=*M1
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=AJ 9636


COMMAND_INIT=AT&F&C1*M2&D2S0=0S2=43S7=55X4V1Q0<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP4<cr><lf>


COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP4<cr><lf>


;******************* Modems L.C.E. *******************************
[LCE 126P - FRN]
CALLBACKTIME=45
DEFAULTOFF=
MAXCARRIERBPS=2400
MAXCONNECTBPS=4800
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C3
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT&F&C1&D2L3V1W1N0X4S0=0S2=43S7=55S95=34<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP4<cr><lf>
CONNECT_EC=<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps>/ARQ<cr><lf>


COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP4<cr><lf>
CONNECT_EC=<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps>/ARQ<cr><lf>



[LCE 132P - FRN]
CALLBACKTIME=45
DEFAULTOFF=
MAXCARRIERBPS=9600
MAXCONNECTBPS=9600
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K4
<hwflowcontrol_off>=&K0
<compression_on>=Z12
<compression_off>=Z10
<protocol_on>=Z12
<protocol_off>=Z10
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT&F&C1&D2 L3V1N0Q0S0=0S2=43S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL V42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP4<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP4<cr><lf>
CONNECT_EC=<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL V42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

; ********************** Modems 3X **************************

[3X 396D - FRN]
CALLBACKTIME=45
DEFAULTOFF=
MAXCARRIERBPS=2400
MAXCONNECTBPS=9600
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C3
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT&F&C1&D2 S0=0 S2=43 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP4<cr><lf>


COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP4<cr><lf>

[3X 514D - FRN]
CALLBACKTIME=45
DEFAULTOFF=
MAXCARRIERBPS=14400
MAXCONNECTBPS=19200
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C3
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT&F&C1&D2 S0=0 S2=43 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP4<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP4<cr><lf>

[3X WYSIWYF 514DB - FRN]
ALIAS=3X - FRN

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=3X WYSIWYF 514DB


[3X WYSIWYF 514DBX - FRN]
ALIAS=3X - FRN

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=3X WYSIWYF 514DBX

[3X WYSIWYF 514DP - FRN]
ALIAS=3X - FRN

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=3X WYSIWYF 514DP

[3X WYSIWYF 514DPX - FRN]
ALIAS=3X - FRN

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=3X WYSIWYF 514DPX

[3X WYSIWYF 514DS - FRN]
ALIAS=3X - FRN

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=3X WYSIWYF 514DS

[3X WYSIWYF 514DSX - FRN]
ALIAS=3X - FRN

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=3X WYSIWYF 514DSX

[3X WYSIWYF 496DB - FRN]
ALIAS=3X - FRN

DETECT_STRING=ATI0<cr>
DETECT_RESPONSE=3X WYSIWYF 496DB

[3X WYSIWYF 496D - FRN]
ALIAS=3X - FRN

DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=496


[3X WYSIWYF 514D - FRN]
ALIAS=3X - FRN

DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=514



[3X - FRN]
CALLBACKTIME=45
DEFAULTOFF=
MAXCARRIERBPS=14400
MAXCONNECTBPS=19200
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C3
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD


COMMAND_INIT=AT&F&C1&D2 S0=0 S2=43 S7=55 X0<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP4<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP4<cr><lf>



; **********  Modems COM1 **************************************************

[COM1 MV214 - FRN]
ALIAS=COM1 MV219 - FRN
DETECT_STRING=ATI<cr>
DETECT_RESPONSE= MV214

[COM1 MV215 - FRN]
CALLBACKTIME=30
DEFAULTOFF=
MAXCARRIERBPS=2400
MAXCONNECTBPS=9600
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&E5
<hwflowcontrol_off>=&E0
<compression_on>=&E2
<compression_off>=&E0
<protocol_on>=&E1
<protocol_off>=&E0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI<cr>
DETECT_RESPONSE= MV215

COMMAND_INIT=AT&F X4  S0=0 S2=43 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf><h00>
CONNECT_EC=<cr><lf>CONNECT <connectbps> RELIABLE/COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps> RELIABLE<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf><h00>
CONNECT_EC=<cr><lf>CONNECT <connectbps> RELIABLE/COMPRESSED<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps> RELIABLE<cr><lf>

[COM1 MV216 - FRN]
CALLBACKTIME=30
DEFAULTOFF=
MAXCARRIERBPS=14400
MAXCONNECTBPS=38400
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N7
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI7<cr>
DETECT_RESPONSE=3700 STANDALONE

COMMAND_INIT=AT&F &C1 X7 S0=0 S2=43 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42b<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf><h00>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42b<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf><h00>


[COM1 MV219 - FRN]
CALLBACKTIME=30
DEFAULTOFF=
MAXCARRIERBPS=2400
MAXCONNECTBPS=9600
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1
<compression_off>=%C0
; ne pas activer le V42 si modem MV219 sur le serveur. MNP4 (\N3) OK.
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI<cr>
DETECT_RESPONSE= MV219

COMMAND_INIT=AT&F X0 S0=2 S2=43 S7=55 S95=40<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>PROTOCOL  ALT<cr><lf>\
<cr><lf>COMPRESSION CLASS 5<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>


COMMAND_LISTEN=ATS0=2<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>PROTOCOL  ALT<cr><lf>\
<cr><lf>COMPRESSION CLASS 5<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>



[COM1 MC215 - FRN]
CALLBACKTIME=45
DEFAULTOFF=<protocol><compression>
MAXCARRIERBPS=2400
MAXCONNECTBPS=9600
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
;Problème de connexion si correction et compression activ‚es
;<compression_on>=%C1
;<compression_off>=%C0
;<protocol_on>=\\N7
;<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI<cr>
DETECT_RESPONSE=MC215

COMMAND_INIT=AT&F  S0=0 S2=43 S7=55 S95=40<cr>
COMMAND_INIT=AT<hwflowcontrol><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>PROTOCOL LAP-M<cr><lf>\
<cr><lf>COMPRESSION V.42bis<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>


COMMAND_LISTEN=ATS0=2<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>PROTOCOL LAP-M<cr><lf>\
<cr><lf>COMPRESSION V.42bis<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

[COM1 MC216 - FRN]
ALIAS=COM1 MV216 - FRN

;*********** Modems pour portables TOSHIBA ************

[TOSHIBA SLIM ASYNC - FRN]
ALIAS=COM1 MV216 - FRN

[TOSHIBA SLIM SYNC - FRN]
ALIAS= ARN DX - FRN

[TOSHIBA SLIM FAX / 2400 - FRN]
ALIAS=COM1 MC215 - FRN


; ********** Modems ATTEL *******************


[ATTEL MX 96xxx - FRN]
CALLBACKTIME=30
DEFAULTOFF=
MAXCARRIERBPS=9600
MAXCONNECTBPS=9600
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q2
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N6
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI1<cr>
DETECT_RESPONSE=MX 96

COMMAND_INIT=AT:W1&C1&D2 S0=2 S2=43 S7=55 \\V1 \\M0<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
OK=<lf>OK<cr><lf>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<lf>CONNECT <cr><lf>
CONNECT=<lf>CONNECT <connectbps><cr><lf>
CONNECT=<lf>CONNECT <connectbps> TREILLIS<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<lf>CONNECT <cr><lf>
CONNECT=<lf>CONNECT <connectbps><cr><lf>
CONNECT=<lf>CONNECT <connectbps> TREILLIS<cr><lf>


[ATTEL MX 144_9600bps - FRN]
CALLBACKTIME=30
DEFAULTOFF=
MAXCARRIERBPS=9600
MAXCONNECTBPS=9600
<speaker_on>=M1
<speaker_off>=M0
;Pas de compression ni correction pour ce modem.
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT:W1&C1&D2 S0=2 S2=43 S7=55<cr>
COMMAND_INIT=AT<speaker><cr>
OK=<lf>OK<cr><lf>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<lf>CONNECT <cr><lf>
CONNECT=<lf>CONNECT <connectbps><cr><lf>
CONNECT=<lf>CONNECT <connectbps> TREILLIS<cr><lf>
CONNECT=<lf>CONNECT <connectbps> TCM<cr><lf>

COMMAND_LISTEN=ATS0=2<cr>
CONNECT=<lf>CONNECT <cr><lf>
CONNECT=<lf>CONNECT <connectbps><cr><lf>
CONNECT=<lf>CONNECT <connectbps> TREILLIS<cr><lf>
CONNECT=<lf>CONNECT <connectbps> TCM<cr><lf>

[ATTEL MX 144_14400bps - FRN]
CALLBACKTIME=30
DEFAULTOFF=
MAXCARRIERBPS=14400
MAXCONNECTBPS=14400
<speaker_on>=M1
<speaker_off>=M0
;Pas de compression ni correction pour ce modem.
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT:W1&C1&D2 S0=2 S2=43 S7=55<cr>
COMMAND_INIT=AT<speaker><cr>
OK=<lf>OK<cr><lf>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<lf>CONNECT <cr><lf>
CONNECT=<lf>CONNECT <connectbps><cr><lf>
CONNECT=<lf>CONNECT <connectbps> TREILLIS<cr><lf>
CONNECT=<lf>CONNECT <connectbps> TCM<cr><lf>

COMMAND_LISTEN=ATS0=2<cr>
CONNECT=<lf>CONNECT <cr><lf>
CONNECT=<lf>CONNECT <connectbps><cr><lf>
CONNECT=<lf>CONNECT <connectbps> TREILLIS<cr><lf>
CONNECT=<lf>CONNECT <connectbps> TCM<cr><lf>



;*************************** QUATERNAIRE **********************************
[QUATERNAIRE V32.BIS - FRN]
CALLBACKTIME=45
DEFAULTOFF=
MAXCARRIERBPS=14400
MAXCONNECTBPS=19200
<speaker_on>=M1
<speaker_off>=M0
;<hwflowcontrol_on>=  Keep the default value
;<hwflowcontrol_off>=  Keep the default value
<hwflowcontrol_on>=
<hwflowcontrol_off>=
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI3<cr>
DETECT_RESPONSE=Quaternaire
COMMAND_INIT=AT&F&C1&D2 V1 X1 S0=0 S2=43 S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP4<cr><lf>


COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <carrierbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <carrierbps>/MNP4<cr><lf>




;******************* Modems SAT *******************************

[SAT 14402 - FRN]
CALLBACKTIME=45
DEFAULTOFF=
MAXCARRIERBPS=14400
MAXCONNECTBPS=19200
<speaker_on>=M1
<speaker_off>=M0
;<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
;<compression_on>=%C3
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=TELSAT 14402

; probl‚me de connexion si 0 compression activ‚e !.

COMMAND_INIT=ATF0&C1&D2L3V1W0N0X4S0=2S2=43S7=55S95=34<cr>
COMMAND_INIT=AT<hwflowcontrol><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP4<cr><lf>
CONNECT_EC=<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps>/ARQ<cr><lf>


COMMAND_LISTEN=ATS0=2<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP4<cr><lf>
CONNECT_EC=<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps>/ARQ<cr><lf>


;***************** Modems GENER ********************

[GENFAX 14400 - FRN]
CALLBACKTIME=45
DEFAULTOFF=
MAXCARRIERBPS=14400
MAXCONNECTBPS=19200
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C3
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=GENFAX144

COMMAND_INIT=AT&F&C1&D2L3V1W0X4N1S0=2S2=43S7=55S95=40<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP4<cr><lf>
CONNECT_EC=<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps>/ARQ<cr><lf>

CONNECT_EC=<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>


COMMAND_LISTEN=ATS0=2<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP4<cr><lf>
CONNECT_EC=<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps>/ARQ<cr><lf>

CONNECT_EC=<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

[GENER GE925 - FRN]
CALLBACKTIME=45
DEFAULTOFF=
MAXCARRIERBPS=14400
MAXCONNECTBPS=19200
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=\\N3
<compression_off>=\\N0
<protocol_on>=%C1
<protocol_off>=%C0
<autodial_on>=ATDT
<autodial_off>=ATD

;DETECT_STRING=MP<cr>
;DETECT_RESPONSE=GE 925

COMMAND_INIT=AT&FV1&I2X4N1\\V1S0=2S2=43S7=55<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/REL 5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/REL 4<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/REL LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/REL LAPM COMP<cr><lf>


COMMAND_LISTEN=ATS0=2<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/REL 5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/REL 4<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/REL LAPM<cr><lf>
CONNECT_EC=<cr><lf>CONNEC<T <connectbps>/REL LAPM COMP<cr><lf>

[GENER - Generique 14400 - FRN]
;[GENER - G‚n‚rique 14400 - FRN]
;setup doesn't process extended characters in modem names - ramc
;Script … s‚l‚ctionner si probl‚me de connection avec le GENFAX 14400 uniquement.
;
CALLBACKTIME=35
DEFAULTOFF=
MAXCARRIERBPS=14400
MAXCONNECTBPS=19200
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C3
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

;X0 => Seulement CONNECT de retourn‚.
COMMAND_INIT=AT&F&C1&D2L3V1W0X0N1S0=2S2=43S7=55S95=40<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP4<cr><lf>

COMMAND_LISTEN=ATS0=2<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP4<cr><lf>



;******************************* Modems ARN *************************
[ARN DX - FRN]
CALLBACKTIME=30
DEFAULTOFF=
MAXCARRIERBPS=14400
MAXCONNECTBPS=19200
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C3
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0\\G1
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI5<cr>
DETECT_RESPONSE=ARNDX


COMMAND_INIT=AT&FL3W0X4S0=2S95=40<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP4<cr><lf>
CONNECT_EC=<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL: ALT - CELLULAR<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=<cr><lf>PROTOCOL: ALT - CELLULAR<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=<cr><lf>PROTOCOL: ALT - CELLULAR<cr><lf>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>


CONNECT_EC=<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>


COMMAND_LISTEN=ATS0=2<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP4<cr><lf>
CONNECT_EC=<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps>/ARQ<cr><lf>

CONNECT_EC=<cr><lf>PROTOCOL: ALT - CELLULAR<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=<cr><lf>PROTOCOL: ALT - CELLULAR<cr><lf>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

[ARN Generique - FRN]
;[ARN G‚n‚rique - FRN]
; setup doesn't process extended chars in modem names - ram
;Recommand‚ pour le serveur.
CALLBACKTIME=30
DEFAULTOFF=
MAXCARRIERBPS=14400
MAXCONNECTBPS=19200
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C3
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0\\G1
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI5<cr>
DETECT_RESPONSE=ARNDX

COMMAND_INIT=AT&FL3W0X0S0=2S95=40<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP4<cr><lf>

COMMAND_LISTEN=ATS0=2<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP4<cr><lf>


;******************************************** Modems PIAL *********************
[PIAL FAXMOD PC - FRN]
CALLBACKTIME=30
DEFAULTOFF=
MAXCARRIERBPS=14400
MAXCONNECTBPS=19200
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C3
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0\\G1
<autodial_on>=ATDT
<autodial_off>=ATD

DETECT_STRING=ATI4<cr>
DETECT_RESPONSE=PIAL FAXMOD PC


COMMAND_INIT=AT&FL3W0X4S0=2S95=40<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP4<cr><lf>

CONNECT_EC=<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps>/ARQ<cr><lf>

CONNECT_EC=<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=<cr><lf>PROTOCOL: ALT<cr><lf>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=<cr><lf>PROTOCOL: ALT - CELLULAR<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>PROTOCOL: ALT - CELLULAR<cr><lf>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>


COMMAND_LISTEN=ATS0=2<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP4<cr><lf>
CONNECT_EC=<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps>/ARQ<cr><lf>
CONNECT_EC=<cr><lf>PROTOCOL: ALT<cr><lf>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>

CONNECT_EC=<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>PROTOCOL: ALT - CELLULAR<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>PROTOCOL: ALT - CELLULAR<cr><lf>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps><cr><lf>





;------------------------------------------------
;    ITALIAN Modems
;------------------------------------------------

;-----------------------------------------
[DATACONSYST DAC124 - ITA]
ALIAS=Octocom 8324

;----------------------------------------
[SYSNET SMF-04 - ITA]
<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=\\N0
<protocol_on>=\\N3
<compression_off>=%C0
<compression_on>=%C1
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=30
DEFAULTOFF=compression
MAXCARRIERBPS=2400
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55 W1 S95=44<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;-----------------------------------------
[SYSNET SMF-36 - ITA]
<hwflowcontrol_off>=&K0
<hwflowcontrol_on>=&K3
<protocol_off>=\\N0
<protocol_on>=\\N3
<compression_off>=%C0
<compression_on>=%C1
<speaker_off>=M0
<speaker_on>=M1
<autodial_on>=ATDT
<autodial_off>=ATD

CALLBACKTIME=30
DEFAULTOFF=compression
MAXCARRIERBPS=14400
MAXCONNECTBPS=19200

COMMAND_INIT=AT&F&C1&D2 V1 S0=0 S2=128 S7=55 W1 S95=44<cr>
COMMAND_INIT=AT<protocol><compression><hwflowcontrol><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
COMMAND_LISTEN=ATS0=1<cr>

;----------------------------------------
[CDC 6438 - ITA]
CALLBACKTIME=30
DEFAULTOFF=
MAXCARRIERBPS=2400
MAXCONNECTBPS=2400
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C3
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT&F&C1&D2 L3 V1 W1N0 X4 S0=0 S2=43 S7=55 S95=34<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP4<cr><lf>
CONNECT_EC=<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps>/ARQ<cr><lf>


COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP4<cr><lf>
CONNECT_EC=<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps>/ARQ<cr><lf>


[CDC 6436 - ITA]
CALLBACKTIME=30
DEFAULTOFF=
MAXCARRIERBPS=2400
MAXCONNECTBPS=2400
<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=&K3
<hwflowcontrol_off>=&K0
<compression_on>=%C3
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT&F&C1&D2  W1N0 X4 S0=0 S2=43 S7=55 S95=34<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>

COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP4<cr><lf>
CONNECT_EC=<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps>/ARQ<cr><lf>


COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/V42BIS<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP5<cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/MNP4<cr><lf>
CONNECT_EC=<cr><lf>CARRIER <carrierbps><cr><lf>\
<cr><lf>PROTOCOL: LAP-M<cr><lf>\
<cr><lf>COMPRESSION: V.42BIS<cr><lf>\
<cr><lf>CONNECT <connectbps>/ARQ<cr><lf>

[DIGICOM SNM28 - ITA]
CALLBACKTIME=30
DEFAULTOFF=compression
MAXCARRIERBPS=2400
MAXCONNECTBPS=9600

<speaker_on>=M1
<speaker_off>=M0
<hwflowcontrol_on>=\\Q3
<hwflowcontrol_off>=\\Q0
<compression_on>=%C1
<compression_off>=%C0
<protocol_on>=\\N3
<protocol_off>=\\N0
<autodial_on>=ATDT
<autodial_off>=ATD

COMMAND_INIT=AT&F&C1&D2 V1 W1 Q0 S7=55 <cr>
COMMAND_INIT=AT S2=128 S0=0<cr>
COMMAND_INIT=AT<hwflowcontrol><protocol><compression><speaker><cr>
COMMAND_DIAL=<autodial><phonenumber><cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/REL<cr><lf>
CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: ALT<cr><lf>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps>/REL<cr><lf>
CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: ALT<cr><lf>\
<cr><lf>COMPRESSION: CLASS 5<cr><lf>\
<cr><lf>CONNECT <connectbps>/REL<cr><lf>

COMMAND_LISTEN=ATS0=1<cr>
CONNECT=<cr><lf>CONNECT <connectbps><cr><lf>
CONNECT_EC=<cr><lf>CONNECT <connectbps>/REL<cr><lf>
CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: ALT<cr><lf>\
<cr><lf>COMPRESSION: NONE<cr><lf>\
<cr><lf>CONNECT <connectbps>/REL<cr><lf>
CONNECT_EC=\
<cr><lf>CARRIER <carrierbps><cr><lf><append>\
<cr><lf>PROTOCOL: ALT<cr><lf>\
<cr><lf>COMPRESSION: CLASS 5<cr><lf>\
<cr><lf>CONNECT <connectbps>/REL<cr><lf>


;-----------------------------------------------
; Other intl modems: Dutch
;-----------------------------------------------

[Tornado 2400]
ALIAS=Hayes Compatible 2400

[Tornado 96]
ALIAS=GVC SM96 - SWE

[Tornado FM14400]
ALIAS=GVC FM14400 - SWE
