             +++++++++++++++++++++++++++++++++              ++++
           ++++++++++++++++++++++++++++++++++++           +++++++
          +++++++++++++++++++++++++++++++++++++         ++++++++
          ++++++++++++++++++++++++++++++++++++        ++++++++
                                                   ++++++++
                                                  ++++++++
          +++++++++++++++++++++++++++           ++++++++
          +++++++++++++++++++++++++++++       ++++++++
           +++++++++++++++++++++++++++++     ++++++++
             +++++++++++++++++++++++++++     ++++++++
                                              ++++++++
                                               ++++++++
    ++++++++++++++++++++++++++++++++++++        ++++++++
   +++++++++++++++++++++++++++++++++++++         ++++++++
   ++++++++++++++++++++++++++++++++++++           ++++++++
    +++++++++++++++++++++++++++++++++               +++++

(C)Copyright 1994-1995 SysKonnect,
a business unit of Schneider & Koch & Co. Datensysteme GmbH.
All rights reserved
===============================================================================
SKTOKNT.TXT

Readme-File for Token Ring Device Driver for Windows NT /

Subject: SKTOKNT.SYS is the driver for the SK-NET TR4, SK-NET TR16,
	 SK-NET TR4/16, SK-NET TR4/16+ and SK-NET TR/MC2 token ring
	 adapters under the first release of Windows NT on Intel processors.

	 The driver corresponds to the NDIS 3.0 Specification as delivered
	 with the first release of Windows NT.


Version / Date / Author of this file: v1.02 / 13-Feb-1995 / T. Schuber
Version / Date / Author of the referred subject: v1.02 / 17-Feb-1995 /
T. Schuber

This file contains
(1) overview
(2) installation instructions
(3) troubleshooting

===============================================================================


(1) OVERVIEW
============

This README explains how to install the Token Ring driver SKTOKNT.SYS
for Windows NT.
***


(2) INSTALLATION INSTRUCTIONS
=============================

To install the driver, you need the following files:

	Preferrably in the root of the installation disk
		!SKDD100.cfg	EISA config file for SK-NET TR4/16
		!SKDD300.cfg	EISA config file for SK-NET TR4/16+

	In a single directory
		OEMNADSK.HLP	Help file for SK-NET drivers
		OEMNADSK.DLL	Dialogs for SK-NET drivers
		OEMSETUP.INF	Setup script for ethernet driver
		SKTOKNT.SYS	The driver


How to install:

Step 1:	On an EISA machine the SK-NET ISA adapters should be configured using
	the appropriate EISA configuration file.

Step 2:	After having configured your adapter, please start Windows NT.

Step 3:	Start NETWORK from the CONTROL PANEL.

Step 4: Select ADD ADAPTER and then <OTHER> and type in the path to
	OEMSETUP.INF.  Select the driver presented and select the
	appropriate configuration.

Step 5: Then select OK and restart your system.
	(Protocol software should be installed.)
***


(3)  TROUBLESHOOTING
====================

If you encounter problems using the SK-NET Token Ring adapter under
Windows NT, please re-read carefully the instructions above and the
documentation supplied with the system.  Additionally, you should look
into your system log file (using the event viewer) and check it for
entries from SKTOKNT.  The last 5 DWORDs of the logging data are:
	Slot number (for ISA adapters that are not EISA-configured: -1),
	Interrupt number,
	Dma channel,
	Base I/O port and
	Vendor code (3 bytes) / adapter id (1 byte)
of the adapter that caused the error.
Following is a list of some events, possible reasons (may be
incomplete) and suggestions to fix your problem.

	Event ID:	5000 -	Has encountered a conflict in resources
				and could not load.
	Reason(s):	???
	Help:		???
	---------------
	Event ID:	5001 -	Could not allocate the resources necessary
				for operation.
	Reason(s):	Not enough RAM or pagefile too small.
	Help:		...
	---------------
	Event ID:	5003 -	Could not find an adapter.
	Reason(s):	Wrong slot or IO Port
			Adapter physically not installed.
			System configuration information invalid.
	Help:		Check slot/port settings.
			Look if adapter is physically present.
			Check system configuration.
	---------------
	Event ID:	5004 -	Could not connect to the interrupt number
				supplied.
	Reason(s):	The selected interrupt is already in use.
	Help:		Select free interrupt.
	---------------
	Event ID:	5005 -	Has encountered an internal error and has
				failed.
	Reason(s):	Miscellanuous.
	Help:		???
	---------------
	Event ID:	5007 -	Timed out during an operation.
	Reason(s):	Wrong interrupt, dma channel or base address.
			Cable not connected.
	Help:		Start a driver under DOS (with the same resource usage)
			and look if it works.
			Check cabling.
	---------------
	Event ID:	5009 -	Does not support the configuration supplied.
	Reason(s):	Invalid IRQ or DMA given.
			Old .cfg file used for configuration.
	Help:		Check configuration.
			Please use the new .cfg file supplied with
			this driver or an even newer one.

	If your special problem is not listed or the error persists, please
	send us your system log file or at least the event id number and the
	logging data (as dwords) of the entries written by SKTOKNT.

*** End of information file ***
