; Windows Modem Setup File
; Copyright (c) 1993-1995 Microsoft Corporation
; Manufacturer:   MultiTech

[Version]
Signature="$CHICAGO$"
Class=Modem
ClassGUID={4D36E96D-E325-11CE-BFC1-08002BE10318}
Provider=%Mfg%

[Manufacturer]
%Mfg% = Models

; Modem models

[Models]
%Modem2% = Modem2,UNIMODEM7896F369		; MT1432MG
%Modem1% = Modem1,Multi_Modem1,UNIMODEM7130E8D2	; MT1432BG


; Installation sections

[Modem2]	; MT1432MG
AddReg=All, MfgAddReg, Modem1.AddReg, External


[Modem1]	; MT1432BG
AddReg=All, MfgAddReg, Modem1.AddReg, External


; AddReg sections

[Modem1.AddReg]	; MT1432BG
HKR,, Properties, 1, 80,01,00,00, 64,00,00,00, ff,00,00,00, 07,00,00,00, 0f,00,00,00, 37,03,00,00, 00,96,00,00, 40,38,00,00
HKR,, FClass, 1, 09,00,00,00

[Modem2.AddReg]	; MT1432MG
HKR,, Properties, 1, 80,01,00,00, 64,00,00,00, ff,00,00,00, 07,00,00,00, 0f,00,00,00, 37,03,00,00, 00,e1,00,00, 40,38,00,00
HKR,, FClass, 1, 09,00,00,00
HKR, Settings, FlowControl_Off,, "&E3"


; User visible strings

[Strings]
ClassName = "Modem"
Mfg = "MultiTech (Ger)"

; Model strings

Modem2="Multitech MT1432MG"
Modem1="Multitech MT1432BG"


[All]
HKR,,FriendlyDriver,,unimodem.vxd
HKR,,DevLoader,,*vcomm
HKR,,PortSubClass,1,02
HKR,,ConfigDialog,,modemui.dll
HKR,,EnumPropPages,,"modemui.dll,EnumPropPages"
HKR, Init,      1,, "AT<cr>"
HKR, Responses, "<cr><lf>OK<cr><lf>", 1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>ERROR<cr><lf>", 1, 03, 00, 00,00,00,00, 00,00,00,00

[EXTERNAL]
HKR,, DeviceType, 1, 01

[MfgAddReg]
HKR,, InactivityScale, 1, 3c,00,00,00
HKR, Init,      2,, "AT &F S0=0 <cr>"
HKR, Monitor,   1,, "None"
HKR, Hangup,    1,, "AT H <cr>"
HKR, Answer,    1,, "AT A <cr>"
HKR,, Reset,, "ATZ<cr>"
HKR, Settings, Prefix,, "AT"
HKR, Settings, Terminator,, "<cr>"
HKR, Settings, DialPrefix,, "D"
HKR, Settings, DialSuffix,, 
HKR, Settings, SpeakerVolume_Low,, ""
HKR, Settings, SpeakerVolume_Med,, ""
HKR, Settings, SpeakerVolume_High,, ""
HKR, Settings, SpeakerMode_Off,, "M0"
HKR, Settings, SpeakerMode_Dial,, "M1"
HKR, Settings, SpeakerMode_On,, "M2"
HKR, Settings, SpeakerMode_Setup,, "M3"
HKR, Settings, FlowControl_Off,, "&E0"
HKR, Settings, FlowControl_Hard,, "&E4"
HKR, Settings, FlowControl_Soft,, "&E5"
HKR, Settings, ErrorControl_On,, "&E1"
HKR, Settings, ErrorControl_Off,, "&E0"
HKR, Settings, ErrorControl_Forced,, "&E2"
HKR, Settings, Compression_On,, "&E15"
HKR, Settings, Compression_Off,, "&E14"
HKR, Settings, Modulation_CCITT,, 
HKR, Settings, Modulation_Bell,, 
HKR, Settings, SpeedNegotiation_Off,, 
HKR, Settings, SpeedNegotiation_On,, 
HKR, Settings, Pulse,, "P"
HKR, Settings, Tone,, "T"
HKR, Settings, Blind_Off,, "X4"
HKR, Settings, Blind_On,, "X3"
HKR, Settings, CallSetupFailTimer,, "S7=<#>"
HKR, Settings, InactivityTimeout,, "S30=<#>"

HKR, Responses,"<cr><lf>OK<cr><lf>",           1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>RING<cr><lf>",        1, 08, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO CARRIER<cr><lf>",  1, 04, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>ERROR<cr><lf>",       1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO DIALTONE<cr><lf>", 1, 05, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO DIAL TONE<cr><lf>",1, 05, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>BUSY<cr><lf>",        1, 06, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO ANSWER<cr><lf>",   1, 07, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>FAX<cr><lf>",         1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>DATA<cr><lf>",        1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NUMBER DELAYED:TIMER<cr><lf>", 1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NUMBER LOCKED OUT<cr><lf>", 1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CALL LOCKED:BLACKLISTED<cr><lf>", 1, 01, 00, 00,00,00,00, 00,00,00,00 
HKR, Responses, "<cr><lf>DALAYED<cr><lf>", 1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>BLACKLISTED<cr><lf>", 1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>+FCERROR<cr><lf>", 1, 03, 00, 00,00,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT LAPM<cr><lf>", 1, 02, 02, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 1200 LAPM<cr><lf>", 1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 2400 LAPM<cr><lf>", 1, 02, 02, 00,00,00,00, 60,09,00,00
HKR, Responses, "<cr><lf>CONNECT 4800 LAPM<cr><lf>", 1, 02, 02, 00,00,00,00, c0,12,00,00
HKR, Responses, "<cr><lf>CONNECT 7200 LAPM<cr><lf>", 1, 02, 02, 00,00,00,00, 20,1c,00,00
HKR, Responses, "<cr><lf>CONNECT 9600 LAPM<cr><lf>", 1, 02, 02, 00,00,00,00, 80,25,00,00
HKR, Responses, "<cr><lf>CONNECT 14400 LAPM<cr><lf>", 1, 02, 02, 00,00,00,00, 40,38,00,00

HKR, Responses, "<cr><lf>CONNECT RELIABLE<cr><lf>", 1, 02, 02, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 1200 RELIABLE<cr><lf>", 1, 02, 02, 00,00,00,00, b0,04,00,00
HKR, Responses, "<cr><lf>CONNECT 2400 RELIABLE<cr><lf>", 1, 02, 02, 00,00,00,00, 60,09,00,00
HKR, Responses, "<cr><lf>CONNECT 4800 RELIABLE<cr><lf>", 1, 02, 02, 00,00,00,00, c0,12,00,00
HKR, Responses, "<cr><lf>CONNECT 7200 RELIABLE<cr><lf>", 1, 02, 02, 00,00,00,00, 20,1c,00,00
HKR, Responses, "<cr><lf>CONNECT 9600 RELIABLE<cr><lf>", 1, 02, 02, 00,00,00,00, 80,25,00,00
HKR, Responses, "<cr><lf>CONNECT 14400 RELIABLE<cr><lf>", 1, 02, 02, 00,00,00,00, 40,38,00,00


HKR, Responses, "<cr><lf> CONNECT 1200 LAPM COMPRESSED<cr><lf>", 1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 2400 LAPM COMPRESSED<cr><lf>", 1, 02, 03, 00,96,00,00, 60,09,00,00
HKR, Responses, "<cr><lf>CONNECT 4800 LAPM COMPRESSED<cr><lf>", 1, 02, 03, 00,96,00,00, c0,12,00,00
HKR, Responses, "<cr><lf>CONNECT 7200 LAPM COMPRESSED<cr><lf>", 1, 02, 03, 00,96,00,00, 20,1c,00,00
HKR, Responses, "<cr><lf>CONNECT 9600 LAPM COMPRESSED<cr><lf>", 1, 02, 03, 00,96,00,00, 80,25,00,00
HKR, Responses, "<cr><lf>CONNECT 14400 LAPM COMPRESSED<cr><lf>", 1, 02, 03, 00,96,00,00, 40,38,00,00

HKR, Responses, "<cr><lf>CONNECT 1200<cr><lf>", 1, 02, 00, 00,96,00,00, b0,04,00,00
HKR, Responses, "<cr><lf>CONNECT 1275<cr><lf>", 1, 02, 00, 00,96,00,00, b0,04,00,00
HKR, Responses, "<cr><lf>CONNECT 2400<cr><lf>", 1, 02, 00, 00,96,00,00, 60,09,00,00
HKR, Responses, "<cr><lf>CONNECT 4800<cr><lf>", 1, 02, 00, 00,96,00,00, c0,12,00,00
HKR, Responses, "<cr><lf>CONNECT 7200<cr><lf>", 1, 02, 00, 00,96,00,00, 20,1c,00,00
HKR, Responses, "<cr><lf>CONNECT 9600<cr><lf>", 1, 02, 00, 00,96,00,00, 80,25,00,00
HKR, Responses, "<cr><lf>CONNECT 14400<cr><lf>", 1, 02, 00, 00,96,00,00, 40,38,00,00
