[Ports]
9600,n,8,1,p

[Commands]
Init
Dial
Listen

[Init]
AT&F&C1&D2 V1 &K3 S0=0 S2=128 S7=55 S95=44<cr>

[Dial]
ATDT<#><cr>

[Listen]
ATS0=1<cr>

[Responses]
OK
Loop
Error
No_Carrier
No_Dialtone
Busy
No_Answer
Connect

[OK]
<cr><lf>OK<cr><lf>

[Loop]
<cr><lf>RING<cr><lf>

[Error]
<cr><lf>ERROR<cr><lf>

[No_Carrier]
<cr><lf>NO CARRIER<cr><lf>

[No_Dialtone]
<cr><lf>NO DIALTONE<cr><lf>

[Busy]
<cr><lf>BUSY<cr><lf>

[No_Answer]
<cr><lf>NO ANSWER<cr><lf>

[Connect]
<cr><lf>CONNECT <connectbps><cr><lf>
<cr><lf>CARRIER <carrierbps><cr><lf>

