; MODEMS.INF 

; Please note that the format of the modem script is not final.

[Version]
Signature="$CHICAGO$"
Class=Modem
Provider=Microsoft

[Manufacturer]
%M1% = M1
%M2% = M2
%M3% = M3
%M4% = M4
%M5% = M5
%M6% = M6
%M7% = M7
%M8% = M8
%M9% = M9
%M10% = M10
%M11% = M11
%M12% = M12
%M13% = M13
%M14% = M14
%M15% = M15
%M16% = M16
%M17% = M17
%M18% = M18
%M19% = M19
%M20% = M20
%M21% = M21
%M22% = M22
%M23% = M23
%M24% = M24
%M25% = M25
%M26% = M26
%M27% = M27
%M28% = M28
%M29% = M29
%M30% = M30
%M31% = M31
%M33% = M33
%M34% = M34
%M35% = M35
%M36% = M36
%M37% = M37
%M40% = M40
%M41% = M41
%M42% = M42
%M43% = M43

[M1]
%M100% = M100

[M2]
%M200% = M200
%M201% = M201

[M3]
%M300% = M300
%M301% = M303
%M302% = M303
%M303% = M303
%M304% = M303
%M305% = M305
%M306% = M306
; The script for this modem has not been tested.
%M307% = M307, "PCMCIA\AT&T_PARADYNE-KEEPINTOUCH_CARD-0C7A"

[M4]
%M400% = M400

[M5]
%M500% = M1702
%M501% = M501
%M502% = M502
%M503% = M503

[M6]
%M600% = M600
%M601% = M601
%M602% = M602
%M603% = M602
%M604% = M602
%M605% = M602
%M606% = M602
%M607% = M607
%M608% = M607
%M609% = M607
%M610% = M607
%M611% = M607
%M612% = M612

[M7]
%M700% = M700

[M8]
%M800% = M800

[M9]
%M900% = M900

[M10]
%M1001% = M1001
%M1002% = M1002

[M11]
%M1100% = M1100
%M1101% = M1101

[M12]
%M1200% = M1200
%M1201% = M1201

[M13]
%M1300% = M1300

[M14]
%M1400% = M1702
%M1401% = M1702
%M1402% = M1402

[M15]
%M1500% = M1500

[M16]
%M1600% = M1702
%M1601% = M1601
%M1602% = M1602

[M17]
%M1701% = M1701
%M1702% = M1702
%M1703% = M1703

[M18]
%M1800% = M1702
%M1801% = M1702
%M1802% = M1703
%M1803% = M1803
%M1804% = M1804
%M1805% = M1803
%M1806% = M1804
%M1807% = M1803
%M1808% = M1804
%M1809% = M1803
%M1810% = M1804

[M19]
%M1900% = M1702
%M1901% = M1901
%M1902% = M1902
%M1903% = M1901
; The script for this modem has not been tested
%M1904% = M1904, "PCMCIA\INTEL-MODEM_2400+-68F4"

[M20]
%M2000% = M2000
%M2001% = M1702

[M21]
%M2100% = M2101
%M2101% = M2101
%M2102% = M2101
%M2103% = M2101
; The script for this modem has not been tested
%M2104% = M2104, "PCMCIA\MEGAHERTZ-XJ1144-38BA"
; The script for this modem has not been tested
%M2105% = M2105, "PCMCIA\MEGAHERTZ-CC3144-A42D"

[M22]
%M2200% = M2200
%M2201% = M2201

[M23]
%M2300% = M2300
%M2301% = M2301

[M24]
%M2400% = M2400

[M25]
%M2500% = M2500
%M2501% = M2501

[M26]
%M2600% = M2600
%M2601% = M2601

[M27]
%M2700% = M2700

[M28]
%M2800% = M2800
%M2801% = M2801

[M29]
%M2900% = M2900

[M30]
%M3000% = M1702
%M3001% = M3001
%M3002% = M3002
%M3003% = M3003
%M3004% = M3004
%M3005% = M3005
%M3006% = M3006

[M31]
%M3101% = M3101
%M3102% = M3102
%M3103% = M3103
%M3104% = M3104
%M3105% = M3105
%M3106% = M3104
%M3107% = M3107
%M3108% = M3108

[M33]
%M3300% = M1702

[M34]
%M3400% = M1702
%M3401% = M3401
%M3402% = M3402
%M3403% = M3403

[M35]
%M3500% = M3500
%M3501% = M3501
%M3502% = M3502
%M3503% = M3503
%M3504% = M3504
%M3505% = M3505
%M3506% = M3506
%M3507% = M3507
%M3508% = M3508
%M3509% = M3508

[M36]
%M3600% = M3600
%M3601% = M3601
%M3602% = M3602
%M3603% = M3603

[M37]
%M3700% = M3702
%M3701% = M3701
%M3702% = M3702
%M3703% = M3702
%M3704% = M3704
%M3705% = M3705

[M40]
%M4000% = M1702
%M4001% = M4001
%M4002% = M4002

[M41]
%M4100% = M4100
%M4101% = M4100

[M42]
; The script for this modem has not been tested.
%M4200% = M4200, "PCMCIA\TDK-DF1414A_DATA/FAX_MODEM-889D"

[M43]
; The script for this modem has not been tested.
%M4300% = M4300, "PCMCIA\PSION_DACOM-GOLD_CARD_PCMCIA_MODEM-DAA9"

[M100]
AddReg=All, M100Reg, 19200, Common
[M200]
AddReg=All, M200Reg, 9600, ATI, Common
[M201]
AddReg=All, M201Reg, 19200, ATI, Common
[M300]
AddReg=All, M300Reg, 2400, ATT, Common
[M303]
AddReg=All, M303Reg, 19200, ATT, Common
[M305]
AddReg=All, M305Reg, 19200, ATT, Common
[M306]
AddReg=All, M306Reg, 2400, ATT, Common
[M307]
AddReg=All, M1703, 9600, PCMCIA, Common
[M400]
AddReg=All, M400Reg, 19200, Common
[M501]
AddReg=All, M501Reg, 19200, Common
[M502]
AddReg=All, M502Reg, 19200, Common
[M503]
AddReg=All, M503Reg, 19200, Common
[M600]
AddReg=All, M600Reg, 9600, Codex, Common
[M601]
AddReg=All, M601Reg, 19200, Codex, Common
[M602]
AddReg=All, M602Reg, 19200, Codex, Common
[M607]
AddReg=All, M607Reg, 19200, Codex, Common
[M612]
AddReg=All, M612Reg, 19200, Codex, Common
[M700]
AddReg=All, M700Reg, 19200, Common
[M800]
AddReg=All, M800Reg, 19200, Common
[M900]
AddReg=All, M900Reg, 19200, Common
[M1001]
AddReg=All, M1001Reg, 2400, Common
[M1002]
AddReg=All, M1002Reg, 9600, Common
[M1100]
AddReg=All, M1100Reg, 19200, Digicom, Common
[M1101]
AddReg=All, M1101Reg, 19200, Digicom, Common
[M1200]
AddReg=All, M1200Reg, 19200, Common
[M1201]
AddReg=All, M1201Reg, 19200, Common
[M1300]
AddReg=All, M1300Reg, 19200, Common
[M1402]
AddReg=All, M1402Reg, 2400, Common
[M1500]
AddReg=All, M1500Reg, 19200, Common
[M1601]
AddReg=All, M1601Reg, 19200, Common
[M1602]
AddReg=All, M1602Reg, 19200, Common
[M1701]
AddReg=All, M1701Reg, 1200, Common
[M1702]
AddReg=All, M1702Reg, 2400, Common
[M1703]
AddReg=All, M1703Reg, 9600, Common
[M1803]
AddReg=All, M1803Reg, 19200, Common
[M1804]
AddReg=All, M1804Reg, 19200, Common
[M1901]
AddReg=All, M1901Reg, 19200, Common
[M1902]
AddReg=All, M1902Reg, 19200, Common
[M1904]
AddReg=All, M1702Reg, 2400, PCMCIA, Common
[M2000]
AddReg=All, M2000Reg, 19200, Common
[M2100]
AddReg=All, M2101Reg, 19200, Common
[M2101]
AddReg=All, M2101Reg, 19200, Common
[M2104]
AddReg=All, M2104Reg, 19200, PCMCIA, Common
[M2105]
AddReg=All, M2104Reg, 9600, PCMCIA, Common
[M2200]
AddReg=All, M2200Reg, 19200, Common
[M2201]
AddReg=All, M2201Reg, 9600, Common
[M2300]
AddReg=All, M2300Reg, 19200, Common
[M2301]
AddReg=All, M2301Reg, 19200, Common
[M2400]
AddReg=All, M2400Reg, 9600, Common
[M2500]
AddReg=All, M2500Reg, 19200, Common
[M2501]
AddReg=All, M2501Reg, 19200, Common
[M2600]
AddReg=All, M2600Reg, 19200, NEC, Common
[M2601]
AddReg=All, M305Reg, 19200, PCMCIA, ATT, Common
[M2700]
AddReg=All, M2700Reg, 9600
[M2800]
AddReg=All, M2800Reg, 9600, Common
[M2801]
AddReg=All, M2801Reg, 19200, Common
[M2900]
AddReg=All, M2900Reg, 9600, Common
[M3001]
AddReg=All, M3001Reg, 2400, Common
[M3002]
AddReg=All, M3002Reg, 2400, Common
[M3003]
AddReg=All, M3003Reg, 19200, Common
[M3004]
AddReg=All, M3004Reg, 19200, Common
[M3005]
AddReg=All, M3005Reg, 19200, Common
[M3006]
AddReg=All, M3006Reg, 19200, Common
[M3101]
AddReg=All, M3101Reg, 9600, Racal, Common
[M3102]
AddReg=All, M3102Reg, 2400, Racal, Common
[M3103]
AddReg=All, M3103Reg, 9600, Racal, Common
[M3104]
AddReg=All, M3104Reg, 19200, Racal, Common
[M3105]
AddReg=All, M3105Reg, 14400, Racal, Common
[M3107]
AddReg=All, M3107Reg, 19200, Racal, Common
[M3108]
AddReg=All, M3108Reg, 19200, Racal, Common
[M3401]
AddReg=All, M3401Reg, 19200, Common
[M3402]
AddReg=All, M3402Reg, 19200, Common
[M3403]
AddReg=All, M3403Reg, 9600, Common
[M3500]
AddReg=All, M3500Reg, 19200, Telebit, Common
[M3501]
AddReg=All, M3501Reg, 9600, Telebit, Common
[M3502]
AddReg=All, M3502Reg, 9600, Telebit, Common
[M3503]
AddReg=All, M3503Reg, 19200, Telebit, Common
[M3504]
AddReg=All, M3504Reg, 9600, Telebit, Common
[M3505]
AddReg=All, M3505Reg, 19200, Telebit, Common
[M3506]
AddReg=All, M3506Reg, 19200, Telebit, Common
[M3507]
AddReg=All, M3507Reg, 19200, Telebit, Common
[M3508]
AddReg=All, M3508Reg, 19200, Telebit, Common
[M3600]
AddReg=All, M3600Reg, 9600, UDS, Common
[M3601]
AddReg=All, M3601Reg, 9600, UDS, Common
[M3602]
AddReg=All, M3602Reg, 19200, UDS, Common
[M3603]
AddReg=All, M3603Reg, 9600, UDS, Common
[M3700]
AddReg=All, M3702Reg, 19200, USR, Common
[M3701]
AddReg=All, M3701Reg, 19200, USR, Common
[M3702]
AddReg=All, M3702Reg, 19200, USR, Common
[M3704]
AddReg=All, M3704Reg, 19200, USR, Common
[M3705]
AddReg=All, M3705Reg, 19200, USR, Common
[M4001]
AddReg=All, M4001Reg, 9600, Common
[M4002]
AddReg=All, M4002Reg, 19200, Common
[M4100]
AddReg=All, M4100Reg, 19200, ZyXel, Common
[M4200]
AddReg=All, M1703Reg, 9600, PCMCIA, Common
[M4300]
AddReg=All, M1703Reg, 9600, PCMCIA, Common

[All]
HKR,,FriendlyDriver,,Unimodem.386
HKR,,DevLoader,,VCOMM

[Common]
HKR,Dial, "ATDT<#><cr>",,
HKR,Listen, "ATS0=1<cr>",,
HKR,Responses\OK, "<cr><lf>OK<cr><lf>",,
HKR,Responses\OK, "<hFF><cr><lf>OK<cr><lf>",,
HKR,Responses\Loop, "<cr><lf>RING<cr><lf>",,
HKR,Responses\Loop, "<cr><lf>RRING<cr><lf>",,
HKR,Responses\Loop, "<cr><lf>RINGING<cr><lf>",,
HKR,Responses\Loop, "<cr><lf>DIALING<cr><lf>",,
HKR,Responses\Error, "<cr><lf>ERROR<cr><lf>",,
HKR,Responses\Error, "<cr><lf>VOICE<cr><lf>",,
HKR,Responses\Error, "<cr><lf>ABORTED<cr><lf>",,
HKR,Responses\Error, "<cr><lf>NO PROMPTTONE<cr><lf>",,
HKR,Responses\Error, "<cr><lf>ERROR DATA Button not defined<cr><lf>",,
HKR,Responses\No_Carrier, "<cr><lf>NO CARRIER<cr><lf>",,
HKR,Responses\No_Dialtone, "<cr><lf>NO DIALTONE<cr><lf>",,
HKR,Responses\No_Dialtone, "<cr><lf>NO DIAL TONE<cr><lf>",,
HKR,Responses\Busy, "<cr><lf>BUSY<cr><lf>",,
HKR,Responses\No_Answer, "<cr><lf>NO ANSWER<cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE><cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CARRIER <DCE><cr><lf>",,

[PCMCIA]
HKR,,PortDriver,,Serial.386
HKR,,PortName,,COM5

[ATT]
;AT&T ARK DM 424
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE> EC<cr><lf>",,

;AT&T Dataports like an extra space
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE> <cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE> <cr><lf><cr><lf>",,

[Telebit]
;Telebits
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/<DCE><cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/LAPM<cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/LAPM/<DCE><cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/LAPM/COMP/<DCE><cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/REL/COMP/<DCE><cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/REL/<DCE><cr><lf>",,

[Digicom]
;;Digicom Scout
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE><hFF>",,
HKR,Responses\Connect,"<cr><lf>CONNECT<cr><lf>",,
HKR,Responses\Connect,"<cr><lf>PLEASE SET TO <DTE><cr><lf>",,
HKR,Responses\Connect,"<cr><lf>PROTOCOL: NONE<cr><lf><cr><lf>CONNECT <DTE><cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CONNECT FAST<cr><lf>",,

[Racal]
;Racal RMD
HKR,Responses\Connect,"<cr><lf>CONNECT <DCE> MNP <DTE><cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DCE> V.42 <DTE><cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DCE> V.42 bis <DTE><cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DCE> V.42bis <DTE><cr><lf>",,

[UDS]
;UDS Motorola
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/REL<cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/LAPM<cr><lf>",,

[USR]
;USRobotics modems

HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/ARQ<cr><lf>",,

[Codex]
;Codex 3261Fast returns this if *XC1
;Codex 2264 also returns this

HKR,Responses\Connect,"<cr><lf>CONNECT <DTE> RELIABLE<cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/V32/NONE<cr><lf>",,

[ATI]
;;ATIs use this string

HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/LAP-M <cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/LAP-M <cr><lf><cr><lf>OK<cr><lf>",,

HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/LAPM/COMP<cr><lf>",,

[ZyXel]
;ZyXel U-1496

HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/V32b <DCE>/MNP5<cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/V32b <DCE>/MNP4<cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/V32b <DCE>/MNP3<cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/V32b <DCE>/V42b<cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/V32b <DCE>/V42 <cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/V32b <DCE>/NONE<cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/V.32 <DCE>T/MNP5<cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/V.32 <DCE>T/MNP4<cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/V.32 <DCE>T/MNP3<cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/V.32 <DCE>T/V42b<cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/V.32 <DCE>T/V42 <cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/V.32 <DCE>T/NONE<cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/V.22b <DCE>/MNP5<cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/V.22b <DCE>/MNP4<cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/V.22b <DCE>/MNP3<cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/V.22b <DCE>/V42b<cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/V.22b <DCE>/V42 <cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/V.22b <DCE>/NONE<cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/ZyXEL <DCE>/V42<cr><lf>",,

[NEC]
;NEC modems

HKR,Responses\Connect,"<cr><lf>CARRIER <CE><cr><lf><cr><lf>CONNECT <TE>/V.42bis<cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CARRIER <DCE><cr><lf><cr><lf>CONNECT <DTE>/V.42<cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CARRIER <DCE><cr><lf><cr><lf>CONNECT <DTE><cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CARRIER <DCE><cr><lf><cr><lf>CONNECT <DTE>/REC<cr><lf>",,
HKR,Responses\Connect,"<cr><lf>CARRIER <DCE><cr><lf><cr><lf>CONNECT <DTE>/REL<cr><lf>",,

[TI]
;Texas Instruments Internal
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/REL",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/REL MNP",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/REL V.42",,
HKR,Responses\Connect,"<cr><lf>CONNECT <DTE>/V.42",,

;                                                                                                       ByteSize (Number of bits/byte, 4-8)
;                                                                                                          Parity (0-4=None,Odd,Even,Mark,Space)
;                                                                                                              StopBits (0,1,2 = 1, 1.5, 2)
;             | DCBLength     | BaudRate      | Bit Mask      | XonLim        | XoffLim       | wRsvd |   |   |   |Xon|Xof|Err|Eof|Evt|Evt|Rsv| RlsTimeout    | CtsTimeout    | DsrTimeout   | TxDelay        |

[110] 
HKR,, DCB, HEX, 30, 00, 00, 00, 10, FF, 00, 00, 09, 40, 00, 00, 0a, 00, 00, 00, 0a, 00, 00, 00, 00, 00, 08, 00, 00, 11, 13, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00

[300]
HKR,, DCB, HEX, 30, 00, 00, 00, 11, FF, 00, 00, 09, 40, 00, 00, 0a, 00, 00, 00, 0a, 00, 00, 00, 00, 00, 08, 00, 00, 11, 13, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00

[600]
HKR,, DCB, HEX, 30, 00, 00, 00, 12, FF, 00, 00, 09, 40, 00, 00, 0a, 00, 00, 00, 0a, 00, 00, 00, 00, 00, 08, 00, 00, 11, 13, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00

[1200]
HKR,, DCB, HEX, 30, 00, 00, 00, 13 FF, 00, 00, 09, 40, 00, 00, 0a, 00, 00, 00, 0a, 00, 00, 00, 00, 00, 08, 00, 00, 11, 13, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00

[2400]
HKR,, DCB, HEX, 30, 00, 00, 00, 14, FF, 00, 00, 09, 40, 00, 00, 0a, 00, 00, 00, 0a, 00, 00, 00, 00, 00, 08, 00, 00, 11, 13, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00

[4800]
HKR,, DCB, HEX, 30, 00, 00, 00, 15, FF, 00, 00, 09, 40, 00, 00, 0a, 00, 00, 00, 0a, 00, 00, 00, 00, 00, 08, 00, 00, 11, 13, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00

[9600]
HKR,, DCB, HEX, 30, 00, 00, 00, 16, FF, 00, 00, 09, 40, 00, 00, 0a, 00, 00, 00, 0a, 00, 00, 00, 00, 00, 08, 00, 00, 11, 13, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00

[14400]
HKR,, DCB, HEX, 30, 00, 00, 00, 17, FF, 00, 00, 09, 40, 00, 00, 0a, 00, 00, 00, 0a, 00, 00, 00, 00, 00, 08, 00, 00, 11, 13, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00

[19200]
HKR,, DCB, HEX, 30, 00, 00, 00, 18, FF, 00, 00, 09, 40, 00, 00, 0a, 00, 00, 00, 0a, 00, 00, 00, 00, 00, 08, 00, 00, 11, 13, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00

[38400]
HKR,, DCB, HEX, 30, 00, 00, 00, 1B, FF, 00, 00, 09, 40, 00, 00, 0a, 00, 00, 00, 0a, 00, 00, 00, 00, 00, 08, 00, 00, 11, 13, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00

[56000]
HKR,, DCB, HEX, 30, 00, 00, 00, 1F, FF, 00, 00, 09, 40, 00, 00, 0a, 00, 00, 00, 0a, 00, 00, 00, 00, 00, 08, 00, 00, 11, 13, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00

[128000]
HKR,, DCB, HEX, 30, 00, 00, 00, 23, FF, 00, 00, 09, 40, 00, 00, 0a, 00, 00, 00, 0a, 00, 00, 00, 00, 00, 08, 00, 00, 11, 13, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00

[256000]
HKR,, DCB, HEX, 30, 00, 00, 00, 27, FF, 00, 00, 09, 40, 00, 00, 0a, 00, 00, 00, 0a, 00, 00, 00, 00, 00, 08, 00, 00, 11, 13, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00, 00


[M100Reg]
HKR, Init, "AT&F&C1&D2 L3 V1 W2 S0=0 S2=128 S7=55 &K3 \N7 &U0 M1<cr>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/V42<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/V42BIS<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/REL5<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/REL4<cr><lf>",,

[M200Reg]
HKR, Init, "AT&F&C1&D2 X4 W0 V1 S0=0 S2=128 S7=55 &K3 &U0 &Q6 M1<cr>",,

[M201Reg]
HKR, Init, "AT&F&C1&D2 W0 X4 V1 S0=0 S2=128 S7=55 &K3 &Q6 &U0 M1<cr>",,

[M300Reg]
HKR, Init, "AT&F&C1&D2 V1 X4 S0=0 S2=128 S7=55 \Q3 \N3 M1<cr>",,

[M303Reg]
HKR, Init, "AT&F&C1&D2 V1 X7 S0=0 S2=128 S7=55 \Q3 \N5 M1<cr>",,

[M305Reg]
HKR, Init, "AT&F&C1&D2 V1 X7 S0=0 S2=128 S7=55 \Q3 %C0 \N5 M1<cr>",,

[M306Reg]
; This guy might be broken
HKR, Init, "ATE1Q0V1X4Y0S0=0 S7=15 &D2&C1&M0 M1<cr>",,
HKR, Listen, "ATS0=2<cr>"

[M400Reg]
HKR, Init, "AT&F&C1&D2S0=0 V1 X4 E1 S7=55 S2=128 &K3 \N3 %C0 M1<cr>",,

[M501Reg]
HKR, Init, "AT&F&C1&D2 V1 S0=0 S2=128 S7=55 M1 &H1&I1 &M4 &M4<cr>",,

[M502Reg]
HKR, Init, "AT&F&C1&D2 V1 S0=0 S2=128 S7=55M1 &K3 \N3 %C0<cr>",,

[M503Reg]
;Compression turned off for stability.
;Maximum DTE speed set to 19200
HKR, Init, "AT&F&C1&D2 V1 S0=0 S2=128 S7=55M1 &K0 \N0 %C0<cr>",,

[M600Reg]
HKR, Init, "AT&F&C1&D2S0=0 V1 *XC1 E1 S7=55 S2=128 *FL3 *SM0 *SM2 M1<cr>",,


[M601Reg]
HKR, Init, "AT&F&C1&D2 V1 X4 *XC1 S0=0 S2=128 S7=55 *FL3 *SM3 *DC0 M1<cr>",,

[M602Reg]
HKR, Init, "AT&F&C1&D2 V1 *XC1 S0=0 S2=128 S7=55*FL3 *SM3 *DC0 M1<cr>",,

[M607Reg]
HKR, Init, "AT&F S0=0 &C1 &D2 V1 X4 S2=128 *XC1 S7=55 M1 *SM3 *FL3 *DC0<cr>",,

[M612Reg]
HKR, Init, "AT&F&C1&D2 V1 X4 *XC1 S0=0 S2=128 S7=55 *FL3 *SM3 *DC0 M1<cr>",,

[M700Reg]
HKR, Init, "AT&F&C1&D2 V1 W2S0=0 S2=128 S7=55 \Q3 \N3 %C0 M1<cr>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,

[M800Reg]
HKR, Init, "AT&F1&C1&D2 *V1 *N1 S0=0 S2=128 S7=55 *LR2*LG2 *M2 M1 *E0<cr>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DTE>/V42BIS<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DTE>/V42BIS<cr><lf>",,

[M900Reg]
HKR, Init, "AT&F&C1&D2 V1 S0=0 S2=128 S7=55 W0 \Q3 \N3 %C0 M1<cr>",,

[M1001Reg]
HKR, Init, "AT&F&C1&D2 V1 S0=0 S2=128 S7=55 M1-M0\V0%C0<cr>",,
HKR, Responses\Connect, "<cr><lf>CONNECT <DCE><cr><lf>",,
HKR, Responses\Connect, "<cr><lf>CONNECT <DCE><cr><lf>",,

[M1002Reg]
HKR, Init, "AT&F&C1&D2 V1 S0=0 S2=128 S7=55 \Q3 \N3 M1-M0 \V0<cr>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,

[M1100Reg]
HKR, Init, "AT&F&C1&D2 V1 S0=0 S2=128 S7=55 *M0 *F3 *E5 M1<cr>",,

[M1101Reg]
HKR, Init, "AT&F&C1&D2 V1 S0=0 S2=128 S7=55 *M0 *F3 *E5 M1<cr>",,

[M1200Reg]
HKR, Init, "AT&F&C1&D2 V1 S0=0 S2=128 S7=55 *M0 *F3 *E5 M1<cr>",,

[M1201Reg]
HKR, Init, "AT&F&C1&D2 V1 S0=0 S2=128 S7=55 *M0 *F3 *E5 M1<cr>",,

[M1300Reg]
HKR, Init, "AT&F&C1&D2 $X1 V1 S0=0 S2=128 S7=55 $F4 $C0 $E3 M1<cr>",,

[M1402Reg]
HKR, Init, "AT&F &C1 &D2 Q0 V1 \N1 S0=0 S2=128 S7=55 M1<cr>",,

[M1500Reg]
HKR, Init, "AT&F&C1&D2 V1 S0=0 S2=128 S7=55 W0 S95=0 \N3 %C0 &K3 M1<cr>",,


[M1601Reg]
HKR, Init, "AT&F&C1&D2Q0V1E1S0=0S2=128S7=55M1%C0\Q3\N6<cr>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/MNP<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/MNP/COMPRESSED<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/MNP COMPRESSED<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/V42<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/V42BIS<cr><lf>",,
HKR, Responses\Connect,"<cr><lf><cr><lf>CONNECT <DCE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf><cr><lf>CONNECT <DCE>/MNP<cr><lf>",,
HKR, Responses\Connect,"<cr><lf><cr><lf>CONNECT <DCE>/MNP/COMPRESSED<cr><lf>",,
HKR, Responses\Connect,"<cr><lf><cr><lf>CONNECT <DCE>/MNP COMPRESSED<cr><lf>",,
HKR, Responses\Connect,"<cr><lf><cr><lf>CONNECT <DCE>/V42<cr><lf>",,
HKR, Responses\Connect,"<cr><lf><cr><lf>CONNECT <DCE>/V42BIS<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/MNP<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/MNP/COMPRESSED<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/MNP COMPRESSED<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/V42<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/V42BIS<cr><lf>",,
HKR, Responses\Connect,"<cr><lf><cr><lf>CONNECT <DCE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf><cr><lf>CONNECT <DCE>/MNP<cr><lf>",,
HKR, Responses\Connect,"<cr><lf><cr><lf>CONNECT <DCE>/MNP/COMPRESSED<cr><lf>",,
HKR, Responses\Connect,"<cr><lf><cr><lf>CONNECT <DCE>/MNP COMPRESSED<cr><lf>",,
HKR, Responses\Connect,"<cr><lf><cr><lf>CONNECT <DCE>/V42<cr><lf>",,
HKR, Responses\Connect,"<cr><lf><cr><lf>CONNECT <DCE>/V42BIS<cr><lf>",,
                                                            
[M1602Reg]
HKR, Init, "AT&F&C1&D2Q0V1E1S0=0S2=128 S7=55 S95=0 M1 %C0 \Q3 \N6 <cr>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/MNP<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/MNP/COMPRESSED<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/MNP COMPRESSED<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/V42<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/V42BIS<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/MNP<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/MNP/COMPRESSED<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/MNP COMPRESSED<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/V42<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/V42BIS<cr><lf>",,

[M1701Reg]
HKR, Init, "ATQ0V1E1S0=0S2=128 S7=55 M1<cr>",,

[M1702Reg]
HKR, Init, "AT&F&C1&D2 V1 S0=0 S2=128 S7=55 M1<cr>",,

[M1703Reg]
HKR, Init, "AT&F&C1&D2 V1 S0=0 S2=128 S7=55 M1<cr>",,

[M1803Reg]
HKR, Init, "AT&F&C1&D2 V1 X4 S0=0 S2=128 S7=55 W0 S95=0 &Q5<cr>",,
HKR, Init, "ATS46=136 &K3 M1<cr>",,

[M1804Reg]
HKR, Init, "AT&F&C1&D2 V1 X4 S0=0 S2=128 S7=55 W0 S95=0 &Q5<cr>",,
HKR, Init, "ATS46=136 &K3 M1<cr>",,

[M1901Reg]
HKR, Init, "AT&F&C1&D2 V1 \V3 S0=0 S2=128 S7=55 M1 \Q3 \N3<cr>",,

[M1902Reg]
HKR, Init, "AT&F&C1&D2V1S0=0 X4 \V2 S2=128 S7=55 \Q3 \N3 M1<cr>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/REL<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/REL-LAPM<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/REL-MNP<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/REL-LAPM-COMP<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/REL-MNP-COMP<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/REL<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/REL-LAPM<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/REL-MNP<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/REL-LAPM-COMP<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/REL-MNP-COMP<cr><lf>",,

[M2000Reg]
HKR, Init, "AT&F&C1&D2 V1 S0=0 S2=128 S7=55 &K3 &Q5 %C0 M1<cr>",,

[M2101Reg]
HKR, Init, "AT&F&C1&D2 W2\G0\J0 S0=0 S2=128 S7=55 \Q3 \N7 %C0 M1<cr>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/REL<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/REL<cr><lf>",,

[M2104Reg]
HKR, Init, "AT&F&C1&D2 X4 S0=0 S2=128 S7=55 \N3 %C0 M1<cr>",,

[M2200Reg]
HKR, Init, "AT&F&C1&D2 W0 V1 \V1 \N0 \Q0 \J1 %C0 S0=0 S2=128 S7=55 M1<cr>",,

[M2201Reg]
HKR, Init, "AT&F&C1&D2 V1 \V1 S0=0 S2=128 S7=55 M1 %C0 \Q3 \N3<cr>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/REL<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/REL<cr><lf>",,

[M2300Reg]
HKR, Init, "AT&F&C1&D2 V1 S0=0 S2=128 S7=55 W0 &K3 &Q5 %C0 M1<cr>",,
HKR, Responses\Connect, "<cr><lf>CONNECT <DCE><cr><lf>",,
HKR, Responses\Connect, "<cr><lf>CONNECT <DCE><cr><lf>",,

[M2301Reg]
HKR, Init, "AT&F&C1&D2 V1 S0=0 S2=128 S7=55 W0 &K3 &Q5 %C0 M1<cr>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,

[M2400Reg]
HKR, Init, "AT&F&C1&D2 V1 \V1 S0=0 S2=128 S7=55 \Q3 \N3 %C0 M1<cr>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/REL<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/REL<cr><lf>",,


[M2500Reg]
HKR, Init, "AT&F E1 &C1 V1 &D2 &Q1 X4 S0=0 S2=128 S7=55<cr>",,
HKR, Init, "AT$BA0 &E14 &E1 &E4 M1<cr>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE> RELIABLE<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE> LAPM<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE> RELIABLE COMPRESSED<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE> LAPM COMPRESSED<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE> RELIABLE<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE> LAPM<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE> RELIABLE COMPRESSED<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE> LAPM COMPRESSED<cr><lf>",,


[M2501Reg]
HKR, Init, "AT&SF1&S0&WE1&F&C1V1&D2&Q0X4&S0S0=0S2=128S7=55<cr>",,
HKR, Init, "AT$BA0 &E14 &E4 &E1 M1<cr>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE> RELIABLE<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE> LAPM<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE> RELIABLE COMPRESSED<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE> LAPM COMPRESSED<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE> RELIABLE<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE> LAPM<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE> RELIABLE COMPRESSED<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE> LAPM COMPRESSED<cr><lf>",,

[M2600Reg]
HKR, Init, "AT&F&C1&D2 \V3 V1 S0=0 S2=128 S7=55 %C0 \Q3 \N6 M1<cr>",,

[M2700Reg]
HKR, Init, "None",,
HKR, Init, "NoResponse",,
HKR, Listen, "None",,
HKR, Responses\Connect,"CLIENT",,
HKR, Responses\Connect, "<h00>CLIENT",,
HKR, Listen, "CLIENTSERVER",,
HKR, Listen, "NoResponse",,
HKR, Dial, "CLIENT",,
HKR, Responses\Connect,"SERVER",,

[M2800Reg]
HKR, Init, "AT&F &C3 &D2 &I2 V1 E1 S0=0 S2=128 S7=55 &K3 &E1 *E0 M1<cr>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DTE>/LAP-M ACTIVE<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DTE>/LAP-M ACTIVE<cr><lf>",,

[M2801Reg]
HKR, Init, "AT&F &C3 &D2 &I2 V1 E1 S0=0 S2=128 S7=55 &K3 &E1 *E0 M1<cr>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DTE>/LAP-M ACTIVE<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DTE>/LAP-M ACTIVE<cr><lf>",,

[M2900Reg]
HKR, Init, "AT&F&C1&D2 V1 E1 S0=0 S2=128 S7=55 S32=0 &K3 M1<cr>",,

[M3001Reg]
HKR, Init, "AT&F&D2 V1 S0=0 S2=128 S7=55 M1<cr>",,


[M3002Reg]
HKR, Init, "AT&F&C2&D2 V1 S0=0 S2=128 S7=55 &Q0<cr>",,

[M3003Reg]
HKR, Init, "AT&F&D2&C1 V1 S0=0 S2=128 S7=55 S95=0 &Q5 &K3 S46=136 M1<cr>",,

[M3004Reg]
HKR, Init, "AT&F&C1&D2 V1 S0=0 S2=128 S7=55 S95=0 &Q5 &K3 S46=0 M1<cr>",,

[M3005Reg]
HKR, Init, "AT&F&C1&D2 V1 W0 S0=0 S2=128 S7=55 S95=0 &Q5 &K3 S46=0 M1<cr>",,

[M3006Reg]
HKR, Init, "AT&F&C1&D2 V1 W0 S0=0 S2=128 S7=55 S95=0 &Q5 &K3 S46=0 M1<cr>",,

[M3101Reg]
HKR, Init, "AT&F&C1&D2 X4 V1 S0=0 S2=128 S7=55 *F2 *D1 *E1 M1<cr>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,

[M3102Reg]
HKR, Init, "AT&F&C1&D2 X4 V1 S0=0 S2=128 S7=55 *F2 *D1 *E1 M1<cr>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,

[M3103Reg]
; The compression setting may be a bug on this one or the previous 2
HKR, Init, "AT&F&C1&D2 V1 S0=0 S2=128 S7=55 M1 *F2 *D0 *E1<cr>",,

[M3104Reg]
HKR, Init, "AT&F&C1&D2 V1 S0=0 S2=128 S7=55 M1 \Q1 \M1\C4 \N3<cr>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <CE><cr><lf><append><cr><lf>V42bis <TE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <CE><cr><lf><append><cr><lf>BUFFER <TE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <CE><cr><lf><append><cr><lf>V42 <DTE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <CE><cr><lf><append><cr><lf>MNP <DTE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <CE><cr><lf>",,

[M3105Reg]
HKR, Init, "AT&F&C1&D2 V1 S0=0 S2=128 S7=55 M1 &K3 \N3 %C0<cr>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <CE><cr><lf><append><cr><lf>V42bis <TE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <CE><cr><lf><append><cr><lf>BUFFER <TE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf><append><cr><lf>V42 <DTE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf><append><cr><lf>MNP <DTE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,

[M3107Reg]
HKR, Init, "AT&F&C1&D2 V1 S0=0 S2=128 S7=55 M1 \Q1 \C4 \N3<cr>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf><append><cr><lf>MNP <DTE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,

[M3108Reg]
HKR, Init, "AT&F&C1&D2 V1 S0=0 S2=128 S7=55 M1 \N0 \Q1 \C4<cr>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf><append><cr><lf>MNP <DTE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,

[M3401Reg]
HKR, Init, "AT&F2&C1&D2 V1 W0 Q0 S7=55 S2=128 S11=55 S95=0<cr>",,
HKR, Init, "ATS0=0 &K3 %C0 \N3 M1<cr>",,

[M3402Reg]
HKR, Init, "AT&F2&C1&D2 S7=55 S2=128 S11=55 S95=0 S0=0 &K3 \N3 %C0 M1<cr>",,

[M3403Reg]
HKR, Init, "AT&F&C1&D2 V1 W0 Q0 S7=55 S2=128 S11=55 S95=0<cr>",,
HKR, Init, "ATS0=0 &K3 %C0 \N3 M1<cr>",,

[M3500Reg]
HKR, Init, "AT&F &C1 &D2 S0=0 S2=128 S7=55 S59=11 X4 S58=2<cr>",,
HKR, Init, "ATS190=0 S180=2 M1<cr>",,

[M3501Reg]
HKR, Init, "AT~&F S53=1 S52=1 S58=0 S0=0 S55=3 S54=3 S7=55 M1<cr>",,

[M3502Reg]
HKR, Init, "AT~&F X13 S131=1 S52=1 S55=3 S110=0 S0=0 S55=3 S7=55<cr>",,
HKR, Init, "ATM1 S58=2 S68=255 S98=0 S95=2 S96=1<cr>",,

[M3503Reg]
HKR, Init, "AT&F &C1 &D2 S0=0 S2=128 S7=55<cr>",,
HKR, Init, "ATS59=11 X11 S58=0 S180=0 S181=0 M1<cr>",,

[M3504Reg]
HKR, Init,"AT&F S52=1 S2=255 S0=0 S54=3 S7=55 S58=0 S180=0 S181=0 M1<cr>",,

[M3505Reg]
HKR, Init,"AT~&F X14 S131=1 S52=1 S55=3 S55=3 S7=55 S50=6 S92=1 S96=0<cr>",,
HKR, Init,"ATS98=0 S66=2 ATS95=2 S97=1 S106=1 S58=2 S68=255 M1 S50=6 <cr>",,

[M3506Reg]
HKR, Init, "AT&F &C1&D2 X11 S0=0 S2=128 S7=55 S50=7 S59=9 S58=2<cr>",,
HKR, Init, "ATS68=255 S180=2 S190=0 M1<cr>",,

[M3507Reg]
HKR, Init, "AT~&F S52=4 S131=3 S51=255 S2=255 S0=0 S7=55 X3 S58=2<cr>",,
HKR, Init, "ATS68=255 S98=0 S110=0<cr>",,

[M3508Reg]
HKR, Init, "AT&F &C1&D2 X11 S0=0 S2=128 S94=1 S92=1 S50=7<cr>",,
HKR, Init, "ATS58=2 S68=255  S180=2 S190=0 M1<cr>",,

[M3600Reg]
HKR, Init, "AT&F&C1&D2 V1 S0=0 S2=128 S7=55 %C0 \N1 M1<cr>",,

[M3601Reg]
;; MAXCONNECTBPS set to 9600 for reasons of stability.
HKR, Init, "AT&F &C1&D2 \V1 S0=0 S2=128 S7=30 \Q3 \N7 %C0 M1<cr>",,

[M3602Reg]
HKR, Init, "AT&F &C1&D2 \V1 S0=0 S2=128 S50=7 \Q3 \N7 %C0 M1<cr>",,

[M3603Reg]
;Maxconnect set down to 9600 and advanced features disabled for stability.
HKR, Init, "AT&F &C1&D2 \V1 \Q0 %C0 \N0 S0=0 S2=128 M1<cr>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/REL<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/LAPM<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/REL<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/LAPM<cr><lf>",,

[M3701Reg]
HKR, Init, "AT&F&C1&D2  V1 &B0 S0=0 S2=128 S7=55 M1<cr>",,

[M3702Reg]
HKR, Init, "AT&F&C1 &D2 &A1 &B1 V1 Q0 S0=0 S2=128 S7=55<cr>",,
HKR, Init, "AT&R2&H1 &K0 &M4 M1<cr>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/ARQ<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/ARQ<cr><lf>",,

[M3704Reg]
HKR, Init, "AT&F&C1&D2 V1 S0=0 S2=128 S7=55 &H1&R2 &K0 &M4 M1<cr>",,

[M3705Reg]
HKR, Init, "AT&F&C1&D2 V1 S0=0 S2=128 S7=55 &H1&R2 &K0 &M4 M1&B1<cr>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/ARQ<cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE><cr><lf>",,
HKR, Responses\Connect,"<cr><lf>CONNECT <DCE>/ARQ<cr><lf>",,

[M4001Reg]
HKR, Init, "AT&F&C1&D2 V1 X4 S0=0 S2=128 S7=55 S95=0 M1 &K3 %C0 \N3 <cr>",,

[M4002Reg]
HKR, Init, "AT&F&C1&D2 V1 X4 S0=0 S2=128 S7=55 S95=0 &K3 %C0 &Q5 M1<cr>",,

[M4100Reg]
HKR, Init, "AT&F&C1&D2 V1 X5 S0=0S2=128 S7=55 M1 &H3 &K3 &K0 <cr>",,

[Strings]
M1 = "Angia"
M100 = "Angia DataStart for Compaq LTE"
M2 = "ATI"
M200 = "ATI 2400 etc/e"
M201 = "ATI 9600 etc/e"
M3 = "AT&T"
M300 =  "AT&T 2224 CEO"
M301 = "AT&T Comsphere 3810"
M302 = "AT&T Comsphere 3811"
M303 = "AT&T Comsphere 3820"
M304 = "AT&T Comsphere 3830"
M305 = "AT&T Dataport"
M306 = "AT&T 4024"
M307 = "AT&T /Paradyne Keep In Touch PCMCIA card"
M4 = "Bocamodem"
M400 = "Bocamodem M1440"
M5 = "Cardinal"
M500 = "Cardinal 2400e"
M501 = "Cardinal 9600"
M502 = "Cardinal 14400"
M503 = "Cardinal 14400 Internal"
M6 = "Motorola Codex"
M600 = "Motorola Codex 2264"
M601 = "Motorola Codex 3220"
M602 = "Motorola Codex 3260"
M603 = "Motorola Codex 3261"
M604 = "Motorola Codex 3262"
M605 = "Motorola Codex 3263"
M606 = "Motorola Codex 3265"
M607 = "Motorola Codex 3260 Fast"
M608 = "Motorola Codex 3261 Fast"
M609 = "Motorola Codex 3262 Fast"
M610 = "Motorola Codex 3263 Fast"
M611 = "Motorola Codex 3265 Fast"
M612 = "Motorola Codex 3220 Plus"
M7 = "Compaq"
M700 = "Compaq SpeedPAQ 144"
M8 = "CXR"
M800 = "CXR Telcom 1445"
M9 = "DataRace"
M900 = "DataRace RediModem V.32bis"
M10 = "Datatrek"
M1001 = "Datatrek Elite 624D"
M1002 = "Datatrek V.32"
M11 = "Digicom"
M1100 = "Digicom Scout"
M1101 = "Digicom Scout Plus"
M12 = "DSI"
M1200 = "DSI 9624LE Plus"
M1201 = "DSI 9624E"
M13 = "ETech"
M1300 = "ETech UFOMATE P1496MX"
M14 = "Evercom"
M1400 = "Evercom 24"
M1401 = "Evercom 24E"
M1402 = "Evercom 24E+"
M15 = "Gateway 2000"
M1500 = "Gateway Telepath Internal"
M16 = "GVC"
M1600 = "GVC SM2400"
M1601 = "GVC SM96"
M1602 = "GVC FM14400"
M17 = "Generic"
M1701 = "Hayes Compatible 1200"
M1702 = "Hayes Compatible 2400"
M1703 = "Hayes Compatible 9600"
M18 = "Hayes"
M1800 = "Hayes Pocket Modem 2400"
M1801 = "Hayes Smartmodem 2400"
M1802 = "Hayes Smartmodem 9600"
M1803 = "Hayes Optima 9600"
M1804 = "Hayes Optima 14400"
M1805 = "Hayes Ultra 9600"
M1806 = "Hayes Ultra 14400"
M1807 = "Hayes Accura 96+FAX96"
M1808 = "Hayes Accura 144+FAX144"
M1809 = "Hayes Accura 96B+FAX96"
M1810 = "Hayes Accura 144B+FAX144"
M19 = "Intel"
M1900 = "Intel SatisFaxtion 100"
M1901 = "Intel SatisFaxtion 400e"
M1902 = "Intel 9600EX"
M1903 = "Intel 14400EX"
M1904 = "Intel 2400 PCMCIA card"
M20 = "Macronix"
M2000 = "Macronix Maxlite Fax 9696"
M2001 = "Macronix VOMAX 2000"
M21 = "Megahertz"
M2100 = "Megahertz C2144 Pocket Faxmodem"
M2101 = "Megahertz T3144 for Toshiba"
M2102 = "Megahertz Z3144 for Zenith"
M2103 = "Megahertz C5144 for Compaq LTE"
M2104 = "Megahertz 14400 PCMCIA card with XJACK"
M2105 = "Megahertz 9600 Data/Fax PCMCIA card"
M22 = "MicroCom"
M2200 = "MicroCom QX 4232bis"
M2201 = "MicroCom QX 4232HS"
M23 = "MicroGate"
M2300 = "MicroGate MG96"
M2301 = "MicroGate MG144"
M24 = "MicroPorte"
M2400 = "MicroPorte 1042"
M25 = "MultiTech"
M2500 = "MultiTech MultiModem 224"
M2501 = "MultiTech MultiModem MT932"
M26 = "NEC"
M2600 =  "NEC 9635E Plus"
M2601 = "NEC 14.4 Data/Fax PCMCIA Card"
M27 = "Local (no modems)"
M2700 ="Direct connection between 2 PCs"
M28 = "Octocom"
M2800 = "Octocom 8324"
M2801 = "Octocom 8396"
M29 = "PDI (IBX)"
M2900= "IBX 1000"
M30 = "Practical Peripherals"
M3000 = "Practical Modem 2400 Pocket"
M3001 = "Practical Modem 2400SA"
M3002 = "Practical Modem 2400MNP"
M3003 = "Practical Modem 9600SA"
M3004 = "Practical Modem 14400SA"
M3005 = "Practical Modem 9600FXMT"
M3006 = "Practical Modem 14400FXMT"
M31 = "Racal"
M3101 = "Racal RMD 2412"
M3102 = "Racal RMD 2412/2"
M3103 = "Racal RMD 3221"
M3104 = "Racal RMD 3222"
M3105 = "Racal RMD 3226"
M3106 = "Racal RMD 3223"
M3107 = "Racal RMD 9632PA"
M3108 = "Racal RMD 9642PA"
M33 = "SupraModem"
M3300 = " 2400"
M34 = "Supra"
M3400 = "Supra Fax Modem 9624 Internal"
M3401 = "Supra Fax Modem V32"
M3402 = "Supra Fax Modem V32bis"
M3403 = "Supra Fax Modem Plus"
M35 = "Telebit"
M3500 = "Telebit QBlazer"
M3501 = "Telebit T1000"
M3502 = "Telebit T1500"
M3503 = "Telebit T1600"
M3504 = "Telebit T2000"
M3505 = "Telebit T2500"
M3506 = "Telebit T3000"
M3507 = "Telebit TrailBlazer Plus"
M3508 = "Telebit WorldBlazer"
M3509 = "Telebit WorldBlazer-Rackmount"
M36 = "UDS Motorola"
M3600 = "UDS Motorola V.3225"
M3601 = "UDS Motorola V.3227"
M3602 = "UDS Motorola V.3229"
M3603 = "UDS Motorola FasTalk V.32/42b"
M37 = "US Robotics"
M3700 = "US Robotics Courier Dual"
M3701 = "US Robotics Courier HST"
M3702 = "US Robotics Courier V.32bis"
M3703 = "US Robotics Sportster 2400"
M3704 = "US Robotics Sportster 9600"
M3705 = "US Robotics Sportster 14400"
M40 = "Zoom"
M4000 = "Zoom AFX"
M4001 = "Zoom FX 9624V"
M4002 = "Zoom VFX V.32bis"
M41 = "ZyXel"
M4100 = "ZyXel U-1496"
M4101 = "ZyXel U-1496E"
M42 = "TDK"
M4200= "TDK DATA/FAX PCMCIA card" 
M43 = "Psion"
M4300 = "Psion Dacom Gold PCMCIA Card"



