;  Adapter Description File   Version 1.2 93/08/26 
;  device name: SK-NET FDDI-FM
;  file name: @0083.adf
;  Copyright (c) 1992 by Schneider & Koch
;-------------------------------------------------------------------------------

;-------------------------------------------------------------------------------

AdapterID 00083h

;-------------------------------------------------------------------------------

AdapterName "SK-NET FDDI-FM/FDDI Network Adapter"

;-------------------------------------------------------------------------------

NumBytes 3

;-------------------------------------------------------------------------------
FixedResources

;POS_PROG_EN disabled
     POS[1]=0XXXXXXXb

;POS_PAGE<2..0> = 0
     POS[1]=XXXXX000b
;-------------------------------------------------------------------------------

NamedItem Prompt "I/O Port Address Location"

  Choice "0200-03ff" POS[2]=XX000000b IO  00200h-003ffh
  Choice "0600-07ff" POS[2]=XX000001b IO  00600h-007ffh
  Choice "0a00-0bff" POS[2]=XX000010b IO  00a00h-00bffh
  Choice "1200-13ff" POS[2]=XX000100b IO  01200h-013ffh
  Choice "2200-23ff" POS[2]=XX001000b IO  02200h-023ffh
  Choice "4200-43ff" POS[2]=XX010000b IO  04200h-043ffh
  Choice "8200-83ff" POS[2]=XX100000b IO  08200h-083ffh
  Choice "fe00-ffff" POS[2]=XX111111b IO  0fe00h-0ffffh
  Choice "fa00-fbff" POS[2]=XX111110b IO  0fa00h-0fbffh
  Choice "f600-f7ff" POS[2]=XX111101b IO  0f600h-0f7ffh
  Choice "ee00-efff" POS[2]=XX111011b IO  0ee00h-0efffh
  Choice "de00-dfff" POS[2]=XX110111b IO  0de00h-0dfffh
  Choice "be00-bfff" POS[2]=XX101111b IO  0be00h-0bfffh
  Choice "7e00-7fff" POS[2]=XX011111b IO  07e00h-07fffh

  Help "I/O Port Address Location : Each FDDI adapter installed is assigned
        a unique address location.

        I/O Port address location needs only to be changed if it is in conflict
        with another adapter.
        Conflicting assignments are marked with an asterisk.

        The assignment may be changed by selecting 'Change Configuration' and
        and then using the F5=Previous and the F6=Next keys."

;-------------------------------------------------------------------------------

NamedItem Prompt "Interrupt Level"

  Choice "Interrupt 9"  POS[2]=11XXXXXXb INT 9d
  Choice "Interrupt 10" POS[2]=10XXXXXXb INT 10d
  Choice "Interrupt 11" POS[2]=01XXXXXXb INT 11d
  Choice "Interrupt 3"  POS[2]=00XXXXXXb INT 3d

  Help "Interrupt Level:  This FDDI Network adapter can operate
        on one of four interrupt levels: 3, 9, 10, or 11.

        The assignment may be changed by selecting 'Change Configuration' and
        and then using the F5=Previous and the F6=Next keys."

;-------------------------------------------------------------------------------

NamedItem Prompt "EPROM Address location"

  Choice "EPROM Disabled" POS[1]=X000XXXXb
  Choice "C4000-C7FFF"    POS[1]=X001XXXXb MEM 0C4000h - 0C7FFFh
  Choice "C8000-CBFFF"    POS[1]=X010XXXXb MEM 0C8000h - 0CBFFFh
  Choice "CC000-CFFFF"    POS[1]=X011XXXXb MEM 0CC000h - 0CFFFFh
  Choice "D0000-D3FFF"    POS[1]=X100XXXXb MEM 0D0000h - 0D3FFFh
  Choice "D4000-D7FFF"    POS[1]=X101XXXXb MEM 0D4000h - 0D7FFFh
  Choice "D8000-DBFFF"    POS[1]=X110XXXXb MEM 0D8000h - 0DBFFFh
  Choice "DC000-DFFFF"    POS[1]=X111XXXXb MEM 0DC000h - 0DFFFFh

  Help "EPROM Address Location:  There are 7 possible 16K blocks of PC
        memory that can be assigned for accessing the EPROM area of the
        FDDI Network adapter.

        The assignement needs only to be changed if it is in conflict
        with another adapter.
        Conflicting assignments are marked with an asterisk.

        The assignment may be changed by selecting 'Change Configuration' and
        and then using the F5=Previous and the F6=Next keys."

;-------------------------------------------------------------------------------

NamedItem Prompt "Remote boot on/off"

  Choice "Remote boot on"    POS[1]=XXXX1XXXb
  Choice "Remote boot off"   POS[1]=XXXX0XXXb

  Help "Enables/disables booting from network.

        The assignment may be changed by selecting 'Change Configuration' and
        and then using the F5=Previous and the F6=Next keys."

;-------------------------------------------------------------------------------

NamedItem Prompt "Bus Master Arbitration Level"

  Choice "Level 8"   POS[0]=000XXXXXb ARB 8
  Choice "Level 9"   POS[0]=001XXXXXb ARB 9
  Choice "Level 10"  POS[0]=010XXXXXb ARB 10
  Choice "Level 11"  POS[0]=011XXXXXb ARB 11
  Choice "Level 12"  POS[0]=100XXXXXb ARB 12
  Choice "Level 13"  POS[0]=101XXXXXb ARB 13
  Choice "Level 14"  POS[0]=110XXXXXb ARB 14

  Help "Arbitration level: Each Busmaster and/or DMA device is assigned an
        unique arbitration level in order to arbitrate conflicting requests.

        The assignment needs only to be changed if it is in conflict with
        another adapter.
        Conflicting assignments are marked with an asterisk.

        The assignment may be changed by selecting 'Change Configuration' and
        and then using the F5=Previous and the F6=Next keys."

;-------------------------------------------------------------------------------

NamedItem Prompt "Fairness on/off"

  Choice "Fairness ON"   POS[0]=XXX1XXXXb
  Choice "Fairness OFF"  POS[0]=XXX0XXXXb


  Help "Fairness on/off: By arbitration level each participant is assigned
        his priority.

        Fairness on:  The priority defines the seqence of granting the bus
        on conflicting requests.
        The latency time on bus requests is calculable.

        Fairness off: Higher priority gives more time on the bus.
        The latency time on bus requests is NOT calculable.

        Recommended is to enable fairness.

        The assignment may be changed by selecting 'Change Configuration' and
        and then using the F5=Previous and the F6=Next keys."

;-------------------------------------------------------------------------------

NamedItem Prompt "Streaming data enable/disable"

  Choice "Streaming data disable"   POS[0]=XXXXXX0Xb
  Choice "Streaming data enable"    POS[0]=XXXXXX1Xb

  Help  "

        The assignment may be changed by selecting 'Change Configuration' and
        and then using the F5=Previous and the F6=Next keys."
;-------------------------------------------------------------------------------

NamedItem Prompt "Check on forbidden 8-Bit accesses"

  Choice "Check on"    POS[0]=XXXX1XXXb
  Choice "Check off"   POS[0]=XXXX0XXXb

  Help "Working as busmaster the adapter supports accesses to 32-Bit and
        16-Bit memory slaves.
        If the adapter performs an access to an 8-Bit slave an interrupt
        may be asserted and reported (check on) or not (check off).
        Recommended is to enable this check.

        The assignment may be changed by selecting 'Change Configuration' and
        and then using the F5=Previous and the F6=Next keys."

;-------------------------------------------------------------------------------

NamedItem Prompt "Check CHCK"

  Choice "Check on"    POS[0]=XXXXX1XXb
  Choice "Check off"   POS[0]=XXXXX0XXb

  Help "Working as busmaster the adapter may check the control line 'CHCK'.
        If the check is enabled the adapter asserts an interrupt and reports
        this event.
        Recommended is to enable this check.

        The assignment may be changed by selecting 'Change Configuration' and
        and then using the F5=Previous and the F6=Next keys."

;-------------------------------------------------------------------------------

