;
; Version: 1.10
;
; (C) Copyright International Business Machines Corporation 1993
; All Rights Reserved
;
AdapterId 08FA0h

AdapterName "IBM LANStreamer MC 32 Adapter "

NumBytes 4
FixedResources
  pos[0]=1xxxxxxxb
  pos[2]=xxxx0xx1b
;pos 2 = set preempt time=max, enable busmaster mode
Begin NoDMA
NamedItem Prompt "Adapter Data Rate"
  Choice "16 Mbps"      pos[1]=1xxxxxxxb
  Choice " 4 Mbps"      pos[1]=0xxxxxxxb

  Help "Adapter Data Rate:  This Token-Ring Network Adapter
        can operate at two different data rates:  4 Mbps or 16 Mbps.
        The adapter data rate MUST be set to the rate of the
        Token-Ring Network LAN segment to which you are connecting the
        adapter.  The assignment for this data rate can be changed by
        selecting 'Change Configuration' and then using the
        F5=Previous and the F6=Next keys."

NamedItem Prompt "Adapter Media Type Selection"

  Choice "STP"          pos[2]=0xxxxxxxb
  Choice "UTP"          pos[2]=1xxxxxxxb

  Help "Media Type Selection:  This Token-Ring Network Adapter
        supports two media types,  STP and UTP.
        The media type selected MUST be cable connected to
        the token ring. If not the adapter will exhibit a
        LOBE MEDIA FAILURE.
        The assignment for the media type can be changed by
        selecting 'Change Configuration' and then using the
        F5=Previous and the F6=Next keys."



NamedItem Prompt "Adapter I/O address Range"
  Choice "1C00-1CFF"    pos[0]=x000111xb   io 01C00h-01CFFh
  Choice "2000-20FF"    pos[0]=x001000xb   io 02000h-020FFh
  Choice "2400-24FF"    pos[0]=x001001xb   io 02400h-024FFh
  Choice "2800-28FF"    pos[0]=x001010xb   io 02800h-028FFh
  Choice "2C00-2CFF"    pos[0]=x001011xb   io 02C00h-02CFFh
  Choice "3000-30FF"    pos[0]=x001100xb   io 03000h-030FFh
  Choice "3400-34FF"    pos[0]=x001101xb   io 03400h-034FFh
  Choice "3800-38FF"    pos[0]=x001110xb   io 03800h-038FFh
  Choice "3C00-3CFF"    pos[0]=x001111xb   io 03C00h-03CFFh
  Choice "4000-40FF"    pos[0]=x010000xb   io 04000h-040FFh
  Choice "4400-44FF"    pos[0]=x010001xb   io 04400h-044FFh
  Choice "4800-48FF"    pos[0]=x010010xb   io 04800h-048FFh
  Choice "4C00-4CFF"    pos[0]=x010011xb   io 04C00h-04CFFh
  Choice "5000-50FF"    pos[0]=x010100xb   io 05000h-050FFh
  Choice "5400-54FF"    pos[0]=x010101xb   io 05400h-054FFh
  Choice "5800-58FF"    pos[0]=x010110xb   io 05800h-058FFh
  Choice "5C00-5CFF"    pos[0]=x010111xb   io 05C00h-05CFFh
  Choice "6000-60FF"    pos[0]=x011000xb   io 06000h-060FFh
  Choice "FC00-FCFF"    pos[0]=x111111xb   io 0FC00h-0FCFFh

  Help "The Adapter I/O address field is a six bit field that selects
        the I/O address of the adapter. For Micro Channel I/O
        cycles, this Token-Ring Network adapter is selected when the Micro
        Channel I/O address is within a 256 byte region. If more than
        one adapter in your computer is used, each adapter must be
        assigned a separate I/O address range. The assignment for the
        I/O address range can be changed by selecting 'Change Configuration'
        and then using the F5=Previous and the F6=Next keys.
        If an assignment has an asterisk (*) by it, it is in
        conflict with another assignment and the I/O address range
        must be changed.  If a conflict continues to exist, you may
        need to change the assignments for other options that are in
        your computer to resolve the conflict."

NamedItem Prompt "Interrupt Level"
  Choice "Interrupt  3" pos[1]=xx01xxxxb  int 03h
  Choice "Interrupt  2" pos[1]=xx00xxxxb  int 02h
  Choice "Interrupt 10" pos[1]=xx10xxxxb  int 0Ah
  Choice "Interrupt 11" pos[1]=xx11xxxxb  int 0Bh

  Help "INTERRUPT LEVEL:  This Token-Ring Network Adapter can
        operate on one of four interrupt levels:  2, 3, 10 or 11.
        The preferred interrupt level is 3, but the adapter can
        operate on any of the four levels if necessary.
        The assignment for the interrupt level can be changed by
        selecting 'Change Configuration' and then using the
        F5=Previous and the F6=Next keys.
        If an assignment has an asterisk (*) by it, it is in
        conflict with another assignment and must be changed."

NamedItem Prompt "Fairness/Streaming Data Select"
  Choice "Fairness ON/Streaming ON"    pos[3]=xx10xxxxb
  Choice "Fairness ON/Streaming OFF"   pos[3]=xx00xxxxb
  Choice "Fairness OFF/Streaming ON"   pos[3]=xx11xxxxb
  Choice "Fairness OFF/Streaming OFF"  pos[3]=xx01xxxxb


  Help "FAIRNESS/STREAMING DATA: This Token-Ring Network Adapter can operate
        with or without arbitration fairness and with or without
        Data Streaming. This selection
        can be changed by selecting 'Change Configuration'
        and then using the F5=Previous and the F6=Next keys."


NamedItem Prompt "Arbitration Level"

  Choice "Level 1"      pos[3]=xxxx0001b  arb 01h
  Choice "Level 2"      pos[3]=xxxx0010b  arb 02h
  Choice "Level 3"      pos[3]=xxxx0011b  arb 03h
; Choice "Level 4"      pos[3]=xxxx0100b  arb 04h
  Choice "Level 5"      pos[3]=xxxx0101b  arb 05h
  Choice "Level 6"      pos[3]=xxxx0110b  arb 06h
  Choice "Level 7"      pos[3]=xxxx0111b  arb 07h
  Choice "Level 8"      pos[3]=xxxx1000b  arb 08h
  Choice "Level 9"      pos[3]=xxxx1001b  arb 09h
  Choice "Level A"      pos[3]=xxxx1010b  arb 0Ah
  Choice "Level B"      pos[3]=xxxx1011b  arb 0Bh
  Choice "Level C"      pos[3]=xxxx1100b  arb 0Ch
  Choice "Level D"      pos[3]=xxxx1101b  arb 0Dh
  Choice "Level E"      pos[3]=xxxx1110b  arb 0Eh

  Help "ARBITRATION LEVEL: This Token-Ring Network Adapter
        can operate on one of thirteen arbitration levels: 1, 2, 3 or
        5 thru E. If more than one adapter is used in your computer,
        each adapter must be assigned a separate arbitration level.
        Assignment for the arbitration level can be changed by
        selecting 'Change Configuration' and then using the F5=Previous
        and the F6=Next keys.
        If an assignment has an asterisk (*) by it, it is in
        conflict with another assignment and the arbitration level
        must be changed.  If a conflict continues to exist, you may
        need to change the assignments for other adapters or options
        that are in your computer to resolve the conflict."

NamedItem Prompt "Remote Program Load Address Range"

  Choice "Disabled"     pos[1]=xxxx0000b
  Choice "C0000-C3FFF"  pos[1]=xxxx0001b  mem 0C0000h-0C3FFFh
  Choice "C4000-C7FFF"  pos[1]=xxxx0011b  mem 0C4000h-0C7FFFh
  Choice "C8000-CBFFF"  pos[1]=xxxx0101b  mem 0C8000h-0CBFFFh
  Choice "CC000-CFFFF"  pos[1]=xxxx0111b  mem 0CC000h-0CFFFFh
  Choice "D0000-D3FFF"  pos[1]=xxxx1001b  mem 0D0000h-0D3FFFh
  Choice "D4000-D7FFF"  pos[1]=xxxx1011b  mem 0D4000h-0D7FFFh
  Choice "D8000-DBFFF"  pos[1]=xxxx1101b  mem 0D8000h-0DBFFFh
  Choice "DC000-DFFFF"  pos[1]=xxxx1111b  mem 0DC000h-0DFFFFh

  Help   "This Token-Ring Network adapter Remote Program Load
          (RPL) ROM is relocatable within Micro Channel memory space.
          The adapter RPL ROM may be located on any 16K boundary
          from hex 000C 000 to 000D C000.
          The address assignment can be changed by selecting
          'Change Configuration' and then using the
          F5=Previous and the F6=Next keys.
          If an assignment has an asterisk (*) by it, it is in
          conflict with another assignment and must be changed."

NamedItem Prompt "Parity Enable/Monitor Feedback"

  Choice "Parity OFF/Monitor OFF"    pos[2]=xxxxx00xb
  Choice "Parity ON/Monitor OFF "    pos[2]=xxxxx10xb
  Choice "Parity OFF/Monitor ON "    pos[2]=xxxxx01xb
  Choice "Parity ON/Monitor ON"      pos[2]=xxxxx11xb

  Help   "Micro Channel Parity Enable/Monitor Slave devices feedback signal:
          This Token-Ring Adapter
          provides the capability of generating and checking data and
          address parity.
          The assignment for parity checking can be changed by selecting
          'Change Configuration' and then using the F5=Previous and the
          F6=Next keys. This adapter also provides the capability
          of monitoring slave device's Selected Feedback Return
          Exception signals during DMA operations.
          The assignment can be changed by selecting 'Change Configuration'
          and then using the F5=Previous and the F6=Next keys."

End
