       -----------------------------------------------------------
                    Microsoft Windows 95 README for Networks
                                   August 1996
       -----------------------------------------------------------

                    (c) Copyright Microsoft Corporation, 1996


This document provides complementary or late-breaking information 
to supplement the Microsoft Windows 95 documentation.


HOW TO USE THIS DOCUMENT
========================

To view Networks.txt on screen in Notepad, maximize the Notepad window.

To print Networks.txt, open it in Notepad or another word processor,
and then use the Print command on the File menu.


CONTENTS
========

CLIENT FOR NETWARE
  Windows 95 and NetWare 3.12 and 4.01 Servers
  Opening Files on NetWare 3.11 Servers
  Lowercase Extended-Character Passwords on NetWare 4.1 Servers
  Client for NetWare and Programs That Use External Files
  Novell NetWare Login Scripts
  Installing Novell Client32 Overwrites 
    NetWare Directory Services Files
  Upgrading Over an Earlier Beta Version of Windows
  Printing to NetWare Directory Services Printers
PLUG AND PLAY NETWORK CARDS AND 16-BIT REAL-MODE DRIVERS
INTEL ETHEREXPRESS 16 NICs AND PCI COMPUTERS
WINDOWS FOR WORKGROUP SHARES
RUNNING WINDOWS 95 FROM A SERVER
  To Install Windows 95 over Previous Builds
SUPPORT FOR THIRD-PARTY NETWORKS
  LANDESK 2.0
  SunSelect PC-NFS
  Banyan VINES
  DEC Pathworks
  Artisoft LANtastic
PRINTING TO A NETWORK PRINTER
PROBLEMS PRINTING TO POSTSCRIPT PRINTERS OVER A NETWARE NETWORK
ISSUES AND INSTALLATION OF MS-DLC WITH WINDOWS 95
MICROSOFT TCP/IP PROTOCOL
USER PROFILES OVER THE NETWORK
NETWORK BACKUP AGENTS
  Arcada Backup Exec Network Backup Agent
  Cheyenne ARCserve Network Backup Agent
REAL-MODE PROTOCOLS: WARNING ICONS ON YOUR NETWORK ADAPTER
USING AN IBM THINKPAD WITH A DOCK II
INTEL ETHEREXPRESS PRO /100B CARD NOT CORRECTLY DETECTED
SETTING UP A WINS SERVER
INTERLNK
USING COMSPEC VARIABLES POINTING TO NETWORK COMMAND.COM FILES


CLIENT FOR NETWARE
==================

Windows 95 and NetWare 3.12 and 4.01 Servers
--------------------------------------------
Windows 95 with Microsoft Client for NetWare can experience 
problems with NetWare 3.12 and 4.01 servers if packet burst is 
turned on. This is a known problem with these servers that Novell 
has fixed and posted on their forums. Download the file Pburst.exe 
from the Novell NetWare Forum on Compuserve or the Novell Web site 
(Ftp.Novell.com). 

Pburst.exe contains the patch for the affected servers.

Opening Files on NetWare 3.11 Servers
-------------------------------------
Programs that open a large number of files consecutively in rapid
succession might have occasional problems opening files on NetWare 3.11 
servers. This can also happen when opening a file in a folder for which
you do not have file scan rights, such as an MS Mail shared post office.

Possible error messages:

- "File not found" error on a file you know exists
- "Sharing violation" or "Lock violation" error
- "Unable to open file" error
- "File in use" error

There are two solutions to these problems:

- Obtain a patch file from Novell for the NetWare 3.11 server. Using 
  FTP, connect to ftp.novell.com. Go to /pub/netware/nwos/nw311/osnlm 
  and run 311ptd.exe. This program will extract the file os2opnfx.nlm. 
  Then, load the .nlm file onto the NetWare 3.11 server. 
  ("load os2opnfx.nlm")

- Disable long filename support in Client for NetWare. This means that 
  you will not be able to use long filenames on any NetWare servers 
  from Windows 95. To disable long-filename support, carry out the 
  following steps:

  1. Click the Start menu, click Run, and then type Regedit.
  2. Go to 
     HKEY_Local_Machine\System\CurrentControlSet\Services\VxD\NWRedir
  3. Create a new binary value named supportLFN with a value of 0.

Lowercase Extended-Character Passwords on NetWare 4.1 Servers
-------------------------------------------------------------
In a NetWare 4.1 environment, Client for NetWare does not support 
passwords that use certain lowercase extended characters. Users 
need to change their password to all uppercase characters.

Client for NetWare and Programs That Use External Files
-------------------------------------------------------
If you are using Microsoft Client for NetWare, and you run a program 
that needs to access an auxiliary file, your program will have problems 
if the auxiliary file is on a drive other than the one the program is 
on. This is because only the current drive is searched for auxiliary 
files; the search path is not searched. If you experience this problem, 
make sure the program and any auxiliary files are on the same drive.

Novell NetWare Login Scripts
----------------------------
The Login Script Processor for the Microsoft Client for NetWare should
correctly process all commands in your login scripts. However, you 
cannot load memory-resident programs (TSRs) from these scripts. 

Installing Novell Client32 Overwrites 
NetWare Directory Services Files
-------------------------------------
When you install Novell Client32, the Novell setup program replaces 
the Microsoft file Netdef.inf and renames it Netdef.bnw, and deletes 
the NDS setup file Nwnds.dll. The result is that after uninstalling 
Novell Client32, Service for NetWare Directory Services will not 
install.

To work around this problem, carry out the following steps:

1. Find the file Netdef.bnw and rename it Netdef.inf.

2. Copy the Nwnds.dll file to the Windows\System directory on your 
   your hard disk by carrying out the following procedure:

   1. Insert your Windows 95 installation CD into the CD-ROM drive.
   2. Open an MS-DOS window.
   3. Change to the Win95 directory on your CD-ROM, and then type the 
      following at the command prompt:

      extract /l c:\windows\system precopy2.cab nwnds.dll

Upgrading Over an Earlier Beta Version of Windows
-------------------------------------------------
If you upgrade this release of Windows over an earlier beta release, 
and you have Service for NetWare Directory Services installed, you 
will be prompted about version conflicts for the following files:

- Nwnp32.dll (v. 4.0.969)
- Nwlsproc.exe (v. 4.0.968)
- Netware.tmp (v. 4.0.968)

When you see the version conflict prompt, click No. After Windows is 
installed, you need to reinstall Service for NetWare Directory Services. 
To do this, carry out the following steps:

1. In Control Panel, double-click the Network icon.
2. Click Add, click Service, and then click Add.
3. Follow the instructions on your screen.

Printing to NetWare Directory Services Printers
-----------------------------------------------
You cannot install Client for NetWare Networks and Service for NetWare 
Directory Services (NDS) during the same installation session. If you 
do, your NDS printers will appear to be offline.

If your printers appear to be offline, try carrying out the following 
steps:

1. In Control Panel, double-click the Network icon.
2. Remove both Client for NetWare Networks and Service for NDS.
3. Restart your computer.
4. In Control Panel, double-click the Network icon.
5. Add Service for NDS.
6. Restart your computer.

NOTE:
If your local area network is using NetWare 4.1 or later, there is no 
need to install Client for NetWare Networks separately. When you install 
Service for NDS, it also installs the Client for NetWare Networks.


PLUG AND PLAY NETWORK CARDS AND 16-BIT REAL-MODE DRIVERS
========================================================

When you run the 16-bit real-mode driver for your Plug and Play 
network interface card (NIC), your Plug and Play card might appear 
not to function.

The reason the card appears to malfunction is that on most computers, 
the Plug and Play card is inactive until Windows 95 enables it. 16-bit 
NIC drivers load before Windows 95 can turn on Plug and Play cards. 
Some 16-bit NIC drivers do not recognize Plug and Play cards (most 
NE2000 Plug and Play clones fall into this category). In this case, 
follow these steps to use your Plug and Play card with a 16-bit NIC 
driver:

1. Run the Softset utility that comes with your Plug and Play card, 
   and then set the card to non-Plug and Play mode.
2. Remove the network card from the list of devices in the Device 
   Manager listing: In Control Panel, double-click the System icon, 
   click the Device Manager tab, select the network card, and then 
   click Remove.
3. Reinstall the network card using the Add New Hardware icon in 
   Control Panel.

When you install a 32-bit protect mode NIC driver in the future, you 
can rerun Softset to turn on Plug and Play mode for your card. This 
problem does not happen if you are using a 32-bit protect-mode NIC 
driver.


INTEL ETHEREXPRESS 16 NICs AND PCI COMPUTERS
============================================

If you are using an Intel EtherExpress 16-network interface card (NIC) 
in a PCI computer that has a Diamond Speed Star PCI video card, your 
system might hang or not initialize properly. These problems, according 
to Intel customer support, are not related to Windows 95 and happen
on a variety of operating systems. 

If you have one of the following video cards, contact your vendor to 
obtain a new video BIOS update:

   * Diamond Speed Star PCI video card with BIOS version 1.01
   * Diamond Viper PCI VGA Video Adapter
   * Diamond Stealth video card, BIOS v1.03

Other PCI video cards might also cause problems with this Intel NIC.
In general, if you experience problems with your EtherExpress 16 in 
a PCI computer other than those described above, please replace the 
card before reporting the problem to Microsoft.


WINDOWS FOR WORKGROUP SHARES
============================

When you upgrade to Windows 95 from Windows for Workgroups, your 
shares are not maintained. The folders/directories you shared in 
Windows for Workgroups need to be reshared. 


RUNNING WINDOWS 95 FROM A SERVER
================================

Windows 95 can be set up to run from a network server. The Windows 95 
Resource Kit contains complete instructions for installing Windows 
in this environment (see Chapter 4, "Server Based Setup for Windows 95").

The following configurations are supported:

- Booting from hard disk using:
  - Client for Microsoft Networks
  - Client for NetWare Networks
  - Novell Workstation Shell 3.x (NETX)
  - Novell Workstation Shell 4.x (VLM)
  - Banyan VINES DOS/Windows client

- Booting from a floppy disk using:
  - Client for Microsoft Networks
  - Client for NetWare Networks
  - Novell Workstation Shell 3.x (NETX)
  - Novell Workstation Shell 4.x (VLM)
  - Banyan VINES DOS/Windows client

- Booting from a remote boot server using:
  - Client for NetWare Networks
  - Novell Workstation Shell 3.x (NETX)
  - Novell Workstation Shell 4.x (VLM)

To use one of the Microsoft clients, your network card must have 
both an NDIS2 (16-bit real mode) *AND* an NDIS3 (32-bit protect 
mode) driver. If your network card is a PCI, EISA, or ISAPNP card, 
you must run Windows over a real-mode client.

To Install Windows 95 over Previous Builds
------------------------------------------
To install this final version of Windows 95 on network computers that 
are already running Windows 95, you have two choices:

- Do a clean install on each  computer;
  -or-
- Upgrade each computer using the following procedure:

  1. Shut down any clients running from the server.
  2. Windows 95 must be installed on the server into the same folder 
     that you were using for previous builds. Delete everything in the 
     shared Windows 95 folder, and then run Netsetup.exe to install this 
     build into that folder.
  3. Restart the client to a command prompt.
  4. If you are using the Microsoft Client for NetWare Networks and use 
     map rooted  drives, you must start either NETX or VLM to run Setup.
  5. Map drives to the machine folder and shared Windows 95 folder 
     as before. These must use the same drive letters as used in the 
     previous build, and map roots should be to the same folder level.
  6. Run Setup for the new build.


SUPPORT FOR THIRD-PARTY NETWORKS
================================

To install support for a third-party, real-mode network, you must be 
running the network when you run Windows 95 Setup. Windows 95 does not 
support installation of a real-mode network after Setup, unless you have 
a Windows 95-specific .inf file from your network vendor. For example, 
FTP includes a Windows 95 .inf in their 32-bit NFS client. Although 
Windows 95 supports other networks, network component files for networks 
other than Microsoft networks are not included with Windows 95. You must 
already have the files for the network you want to install. 

LANDESK 2.0
-----------
LANDESK version 2.0 uses a TSR named Usertsr.exe that might cause 
Windows 95 to stop responding when you use the Microsoft IPX/SPX-
compatible protocol (Nwlink.vxd) or file and printer sharing for 
Microsoft Networks (Vserver.vxd).

LANDESK version 2.01 fixes this problem, and the patch is available 
on Intel's BBS or from Intel product support. For the BBS and product 
support telephone numbers, consult the documentation that came with your 
copy of LANDESK.

SunSelect PC-NFS
----------------
Windows 95 supports versions 5.0 or greater of SunSelect PC-NFS. 
If SunSelect PC-NFS is installed using an NDIS 2 LAN driver or an 
ODI LAN driver, then SunSelect PC-NFS can be installed as an additional 
16-bit network client along with 32-bit protected-mode clients. If you 
are using a SunSelect PC-NFS LAN Driver, Windows 95 can support PC-NFS 
only as the primary network. Additional 32-bit network providers are not 
possible in this case.

Banyan VINES 
------------
If you see a message during startup that the VINES version is not the 
latest, edit the Vines.ini file in the Windows folder so it contains 
the following lines:

   [NEWREV]
   dontcopy=1
   vines.version=5.5x (x) USA      ; where x=your version
   windows.version=3.95

If you receive the message, "Vines NDIS Interface error: 1021. See 
NDISBAN.DOC for an error description," during startup, run the VINES 
utility PCCONFIG to change Banyan drivers to NDIS drivers. Also, make 
sure the section name matches the driver name in the Protocol.ini file.

DEC Pathworks
-------------
Windows 95 provides support for upgrading over existing DEC 
PATHWORKS V5.0, V5.0A and V5.1 configurations. This makes it possible 
to run your existing real-mode PATHWORKS components while migrating 
to Windows 95. However, it is strongly recommended that you upgrade 
to DEC's PATHWORKS for Windows 95, which contains protected-mode 
components.

Restrictions:
PATHWORKS must be started before running Windows 95 Setup to 
automatically detect and upgrade PATHWORKS components. If PATHWORKS 
is not started or is not automatically detected, you will see startup 
errors when you run STARTNET. To correct this, add the appropriate 
"PATHWORKS V5.0 and above" protocol, using the Network icon in Control 
Panel.

Once a system has been upgraded to Windows 95, you cannot change your
PATHWORKS configuration using PWSETUP. However, all existing template
configurations present when you upgrade are converted to work under
Windows 95.

PATHWORKS Native, DLC, X.25, and ISDN datalinks are converted to use
an NDIS driver, if available, during the upgrade. If the replacement
NDIS driver is not configured correctly or is not operating, startup
will display an error and prevent loading of other PATHWORKS components.

To correct this, double-click the Network icon in Control Panel, and 
verify that the adapter driver is configured correctly. If any changes 
are made to the adapter configuration, you must remove the "PATHWORKS 
V5.0 and above" protocol and add it again.

PATHWORKS NetWare client licenses (CCS or FPA) are not currently
supported with Windows 95. If you are using the Microsoft Client for
NetWare Networks to connect to PATHWORKS for OpenVMS (NetWare) or
PATHWORKS for OSF/1 (NetWare) servers, the server must have PATHWORKS 
FPS licenses.

Long filenames do not work correctly on PATHWORKS servers up to and
including version 5.0b. You will be able to create and delete LFN 
files and make and remove LFN folders, but the files and folders will 
not appear when you use the DIR command, or when you open an Explorer 
window to the PATHWORKS server. PATHWORKS server version 5.00 EC01 
corrects this problem and is available from DEC.

Artisoft LANtastic
------------------
The LANtastic server cannot be run when Windows 95 is setting up.

LANtastic also cannot be run in conjunction with networking support 
for other networks.


PRINTING TO A NETWORK PRINTER
=============================

You might have problems setting up a printer that is shared by a third-
party network server. The solution is to redirect LPT1 through an 
MS-DOS window to the third-party share, and then use the printer setup 
for LPT1.

For example, if a network printer is connected to LPT1, follow these 
steps: 

1. At the MS-DOS prompt, type:

   net use lpt1: \\servername\sharename

   (This command might be different on the network you are using. 
   Check the product documentation to find out how to redirect
   an LPT port.)  

2. Start Control Panel, double-click Printers, and then double-click 
   Add Printer. 


PROBLEMS PRINTING TO POSTSCRIPT PRINTERS
OVER A NETWARE NETWORK
=========================================

If you have problems when printing to a PostScript printer over a 
network, (error messages on the printer; no output is printed), it 
might be due to incorrectly configured Banner Pages. To solve this 
problem, you can do one of the following:

- Disable banner pages by removing the check mark from the Banner Pages 
  box on the Capture printer properties (open the Printers folder, click 
  the icon for the printer you are using, and then click Properties on 
  the File menu);
  -or-
- Ask your network administrator to correctly configure banner pages on 
  the Netware server for a PostScript printer.


ISSUES AND INSTALLATION OF
MS-DLC WITH WINDOWS 95
-=========================

Windows 95 contains MS-DLC and support for installing over an existing 
MS-DLC or IBM-DLC installation. Setup will detect DLC and make the 
appropriate changes to your configuration files for these. Refer to 
the Windows 95 Resource Kit, Chapter 10, for a complete description 
of DLC support.


MICROSOFT TCP/IP PROTOCOL
=========================

If Microsoft's TCP/IP is the only protocol you have loaded on your 
system, the IP Address will not be added during Setup. If you have 
a DHCP server, open Control Panel, double-click the Network icon, and 
then close it. This will update the IP Address. (If you don't know if 
you have a DHCP server, check with your network administrator, or check
if your IP address is already entered.)

If you don't have a DHCP server, start Control Panel, double-click 
the Network icon, double-click TCP/IP, click the IP Address tab, and 
then enter your IP Address.

If you are not updating from a previous Windows 95 installation (you 
are doing a "clean install"), to use DNS or LMHOSTS name resolution, 
make sure you have DNS enabled in the Network properties. To enable
DNS, double-click the Network icon in Control Panel, double-click 
TCP/IP, click the DNS configuration tab, and then click Enable DNS.


USER PROFILES OVER THE NETWORK
==============================

If you are using user profiles over a Windows NT or Novell NetWare 
network, and you include Start Menu/Programs, Network Neighborhood,
and/or desktop icons in your profile, the server must have long 
filename support to ensure that these parts of the user profile work 
over the network. 


NETWORK BACKUP AGENTS
=====================

Arcada Backup Exec Network Backup Agent
---------------------------------------
To use the Arcada Backup Exec network backup agent included in 
Windows 95, you must have Arcada Backup Exec version 5.x.


Cheyenne ARCserve Network Backup Agent
--------------------------------------
To use the Cheyenne ARCserve network backup agent included in 
Windows 95, you must have Cheyenne ARCserve version 5.01F. You might 
also use earlier versions if you obtain updated NLMs from Cheyenne 
Software.


REAL-MODE PROTOCOLS: WARNING ICONS ON YOUR NETWORK ADAPTER
==========================================================

If you install a network that does not use protected-mode protocols, 
such as Novell Netware 3.x, you might see a yellow warning icon next 
to your network adapter in Device Manager. You can ignore this warning; 
your network is fully functional. To remove the warning icon, use the 
program, Extract.exe on Setup disk 1 to extract the file Ndis.vxd from 
your Windows 95 disks. Then, copy Ndis.vxd into your Windows\System 
folder. When you reboot your system, the yellow warning icon will no 
longer appear.


USING AN IBM THINKPAD WITH A DOCK II
====================================
If you enable 32-bit PCMCIA support, and your network cards do not 
appear to work properly when inserted into the Dock II's PCMCIA slots; 
or, if you have an ISA network card in the Dock II that has a "Code 10" 
error in its properties in Device Manager, call the IBM Help Center. 
They will provide you with a file to correct this problem.


INTEL ETHEREXPRESS PRO /100B CARD NOT CORRECTLY DETECTED
========================================================

Windows 95 does not correctly detect an Intel EtherExpress Pro /100B 
card during Setup or hardware detection. After Setup, an entry for 
"PCI Ethernet controller" appears under Other Devices in Device Manager, 
which shows that the device is functioning properly; however, the card 
doesn't work.

To properly install the card, remove the PCI Ethernet controller from 
Device Manager, and then restart your computer. The card will then be 
detected; the Update Device Driver wizard will appear.  Insert the 
driver disk that came with the card, and then click Next. The wizard 
will search the disk and find drivers for the Intel 82557-based PCI 
Ethernet. This is correct. Click Finish and the card should work.


SETTING UP A WINS SERVER
========================

To set up a WINS server, carry out the following steps:

1. In Control Panel, double-click the Network icon.
2. Click TCP/IP, and then click Properties.
3. Click the WINS Configuration tab.
4. Make sure that both the Primary WINS Server and Secondary WINS 
   Server boxes are filled in.

   If you have only one WINS Server, you must enter the identical 
   information in both the Primary WINS Server and Secondary WINS 
   Server boxes.

   If you do not fill in both boxes, your WINS setting will be 
   changed to Disable WINS Resolution when you restart your computer. 


INTERLNK
========
The InterLnk networking product contained in MS-DOS 6.x does not 
function properly in MS-DOS mode if you are using FAT32.


USING COMSPEC VARIABLES POINTING TO NETWORK COMMAND.COM FILES
=============================================================

If you are on a network and are currently mapping your compspec to 
remote network file servers, you may get "incorrect DOS version" 
errors (and an explanation of the version shipping with Windows 95 
version 4.00.950 B being an updated ver 7.1 etc.). You need to map 
the comspec to the local copy or to a compatible version on the network.
