# Embedded LE options

The following LE options are embedded in the JES Job Monitor load module:

- ALL31(ON)
- HEAP(32K,32K,ANY,KEEP,8K,4K)
- POSIX(ON)
- STACK(128K,128K,ANYWHERE,KEEP)
- THREADHEAP(4K,4K,ANY,KEEP)
- THREADSTACK(OFF)
- STORAGE(NONE,NONE,NONE,0)

If required, these options can be changed by providing alternate values in the startup JCL. The sample JCL below shows an updated version of the startup JCL, `FEK.SFEKSAMP(FEJJJCL)`, where parameter `LEPRM` can be used to specify LE options.

    //*
    //* JES JOB MONITOR
    //*
    //JMON     PROC PRM=,                  * PRM='-TV' TO START TRACING
    //            LEPRM='RPTOPTS(ON)',
    //            HLQ=FEK,
    //            CFG=FEK.#CUST.PARMLIB(FEJJCNFG)
    //*
    //JMON     EXEC PGM=FEJJMON,REGION=0M,TIME=NOLIMIT,
    //            PARM=('&LEPRM,ENVAR("_CEE_ENVFILE=DD:ENVIRON")/&PRM')
    //STEPLIB  DD DISP=SHR,DSN=&HLQ..SFEKAUTH
    //ENVIRON  DD DISP=SHR,DSN=&CFG
    //SYSPRINT DD SYSOUT=*
    //SYSOUT   DD SYSOUT=*
    //         PEND
    //*

Note: Use caution when changing LE options, as inappropriate values can stop JES Job Monitor from working as designed.

Parent topic: JES Job Monitor