------------------------------------------------------
8/1/97
S3 Incorporated
------------------------------------------------------


Preparing to Install
--------------------
1. Uninstall any previous SonicVibes software:

Drivers:
a. Place the SonicVibes CD in your CD-ROM drive.
b. Select Run from the Windows 95 Start Menu and enter:

D:\UNINSTAL.EXE {assuming your CD-ROM is your D:drive}

DLS Manager:
a. Select Settings | Control Panel from the Start menu.
b. Highlight "S3 DLS Manager Uninstall" and click Add/Remove.

2. Delete any files remaining in the subdirectory where the DLS Manager
   had been installed.

3. Reboot your computer.

Installation
------------
1. Drivers:
a. Windows 95 will detect SonicVibes and display a screen.
b. Make sure that you select "Driver from disk provided by hardware
   manufacturer" and click OK.
c. When prompted for the driver disk, "Browse" to your SonicVibes CD.
   Click OK.

2. DLS Manager:
a. Select Run from the Start Menu and enter:
   D:\DLSMGR\SETUP.EXE {assuming your CD-ROM is your D:drive}
b. When prompted by Setup, indicate the folder where you wish the
   DLS Manager to be installed.

3. DOS Real-Mode Driver:
a. Select Run from the Start Menu and enter:
   D:\DOS\SETUP.EXE {assuming your CD-ROM is your D:drive}
b. When prompted by Setup, indicate the folder where you wish the
   DOS Real-Mode driver to be installed.

4. AudioStation 2 Application:
a. Select Run from the Start Menu and enter:
   D:\VOYETRA\SETUP.EXE {assuming your CD-ROM is your D:drive}
b. When prompted by Setup, indicate the folder where you wish the
   AudioStation 2 application to be installed.
   
Unresolved Issues
-----------------------------
S3 Audio Driver for Windows 95 
20108	When attempting to autodetect the SonicVibes sound card in
        Actua Soccer,  an error dialog saying "SonicVibes in use..."
        occurs in Windows.
20149	APM suspend/resume during DOS full screen GAME resets
        instruments to Piano.
20154	Looping sound occurs when context switching from DOS full
        screen Doom2 to Windows.
20163	If S3LEGACY.COM is not in autoexec.bat and the ROM option is
        selectable even though there is no ROM, the user gets silence
        when sound is expected.
        WORKAROUND: Add S3LEGACY.COM to autoexec.bat or select a
        1M RAM option.

S3 Audio Driver for DOS Real-Mode
20156	S3LEGACY.COM attempts to re-assign the resource to IRQ5 if the
        PnP BIOS is pre-assigned IRQ 2 to S3 PCI Audio card. This will
        cause a "stack overflow" and system lock up.
        WORKAROUND: Install PCI audio on a different slot.
20157	S3LEGACY.COM fails to assign the legacy spaces on Phoenix BIOS's
        which turn off "I/O Access Enabled Bit".
20158	Phoenix BIOS fails to call routing of IRQ.

 
