; GUEST.INF  -- This file install descriptions for Iomega adapters
; Copyright (c) 1995 Iomega Corporation

[Version]
signature="$CHICAGO$"
Class=SCSIAdapter
Provider=%Iomega%

[ClassInstall]
Addreg=SCSIReg

[SCSIReg]
HKR,,,,%SCSIClassName%

[Manufacturer]
%Iomega%=Iomega

;***************************************************************************
;Iomega-manufacturer device list
[Iomega]
%*isaPPA3.DeviceDesc%=*isaPPA3.drv,*isaPPA3
%*isaZOOM.DeviceDesc%=*isaZOOM.drv,*ISAZOOM
%PCI\VEN_9004&DEV_5078.DeviceDesc%= AIC78XX,PCI\VEN_9004&DEV_5078
%*isa1616.DeviceDesc%=*isa1616.drv,*isa1616
;Advansys device list
%ABPPCI.DriverDesc%=ABPPCI,PCI\VEN_10CD&DEV_1100
%ABPPCI.DriverDesc%=ABPPCI,PCI\VEN_10CD&DEV_1200
%ABPPCI.DriverDesc%=ABPPCI,PCI\VEN_10CD&DEV_1300
;Adaptec device list
%*ADP1502.DeviceDesc%= AIC6X60.drv,*ADP1502
%*ADP1520.DeviceDesc%= AIC6X60.drv,*ADP1520
%*ADP1520.DeviceDesc%= AIC6X60.drv,*ADP2015
%*ADP6360.DeviceDesc%= AIC6X60.drv,*ADP6360
%APA1460.DeviceDesc%=  AIC6X60.drv,PCMCIA\Adaptec__Inc.-APA-1460_SCSI_Host_Adapter-BE89
%APA1460.DeviceDesc%=  AIC6X60.drv,PCMCIA\Adaptec__Inc.-APA-1460_SCSI_Host_Adapter-B67E
;***************************************************************************
;Iomega Driver Installation Sections

[*isa1616.drv]
Copyfiles=@PC1616.MPD
AddReg=IOS,NCR406A.Reg
LogConfig = NormalOp

[NormalOp]
; Primary Configuration
ConfigPriority = HARDRECONFIG
IOConfig=330-33F(3ff::),230-23f(3ff::)
IRQConfig = 11,10,12,15

[*isaPPA3.drv]
Copyfiles=@PPA3.mpd
AddReg=IOS,Poll,PPA3.Reg

[*isaZOOM.drv]
CopyFiles=@SPARROW.MPD
AddReg=IOS,isaZOOM.Reg
DelFiles=ASPIDEV
LogConfig=*ADP6360.LogConfig,6x60.LogConfig

;adaptec driver installation section

[AIC78XX]
CopyFiles=@AIC78XX.MPD
AddReg=IOS,AIC78XX.Reg
DelFiles=ASPIDEV
UpdateInis=DoubleBuffer

[AIC6X60.drv]
CopyFiles=@SPARROW.MPD
AddReg=IOS,AHA152x.Reg
DelReg=APA1460Switches
DelFiles=ASPIDEV
LogConfig=*ADP6360.LogConfig,6x60.lc2
Reboot

[AIC6X60.PosDup]
*ADP6360

;Advansys driver installation section

[ABPPCI]
CopyFiles=@ASC.mpd
AddReg=IOS,ABPPCI.reg
DelFiles=ASPIDEV
UpdateInis=UpdateInisSection
UpdateCfgSys = UpdateConfigSys

[ASPIDEV]
VASPID.VXD

;******************************************
;Addreg Section

[NCR406A.Reg]
HKR,,DevLoader,,*IOS
HKR,,PortDriver,,PC1616.MPD

[PPA3.Reg]
HKR,,DevLoader,,*IOS
HKR,,PortDriver,,PPA3.MPD

;adaptec addreg section

[isaZOOM.Reg]
HKR,,DevLoader,,*IOS
HKR,,PortDriver,,SPARROW.MPD

[AHA152x.Reg]
HKR,,PortDriver,,SPARROW.MPD

[AIC78XX.Reg]
HKR,,PortDriver,,AIC78XX.MPD

;advansys addreg section

[ABPPCI.Reg]
HKR,,PortDriver,,ASC.MPD

[*ASC1000.Det]
AddReg=ForceMPCopy

[*ADP6360.Det]
AddReg=ForceMPCopy

[*ADP6360.LogConfig]
ConfigPriority=HARDRECONFIG
IOConfig=140-15F,340-35F
IRQConfig=11,12,9,10

[6x60.LogConfig]
ConfigPriority=HARDRECONFIG
IOConfig=140-15F,340-35F
IRQConfig=11,12,15,9,10

[6x60.LC2]
ConfigPriority=HARDRECONFIG
IOConfig=140-15F,340-35F
IRQConfig=9,10,11,12,15

[*ADP1520.LogConfig]
ConfigPriority = HARDRECONFIG
IOConfig           = 140-15F,340-35F
IRQConfig      = 9,10,11,12

;********************************
;IOS common section
[IOS]
HKR,,DevLoader,,*IOS
HKR,,DontLoadIfConflict,,"Y"

[IOSMCA]
HKR,,ConfigFlags,1,00,02,00,00

[Poll]   
HKR,,Polling,,1

[ForceMPCopy]
HKR,,NoSetupUI,,1

[DoubleBuffer]
%31%\msdos.sys,Options,,"DoubleBuffer=1"

[DestinationDirs]
ASPIDEV = 11                    ; delete from SYSTEM dir if exists
DefaultDestDir = 12             ; IOSubsys directory

[SourceDisksNames]
1=%instd1%,"",1

[SourceDisksFiles]
PPA3.MPD=1
SPARROW.MPD=1
AIC78XX.MPD=1
PC1616.MPD=1
ASC.MPD=1

[ControlFlags]
ExcludeFromSelect=*ABP5401

[UpdateInisSection]
%10%\IOS.INI, SafeList,, %AdvaspiStr%
%10%\IOS.INI, CDUnsafe,, %AdvancdStr%
%10%\SYSTEM.INI, 386Enh, "device=advw32.386", %Advw32Str%, 1

[UpdateConfigSys]
DevDelete = ADVANCD.SYS,1

;*******************************************************************
;User-Visible Strings

[Strings]
SCSIClassName="SCSI controllers"

Iomega="Iomega"
*ISAPPA3.DeviceDesc="Iomega Parallel Port Interface"
*ISAZOOM.DeviceDesc="Iomega Zip Zoom SCSI Host Adapter"
PCI\VEN_9004&DEV_5078.DeviceDesc="Iomega Jaz Jet SCSI Host Adapter"
*ISA1616.DeviceDesc="Iomega PC1616 16-bit SCSI Host Adapter"

; Adaptec visible strings

*ADP1502.DeviceDesc="Iomega Zip Zoom SCSI Host Adapter"
*ADP1520.DeviceDesc="Iomega Jaz Jet ISA SCSI Host Adapter"
*ADP2015.DeviceDesc="Iomega Jaz Jet ISA SCSI Host Adapter"
*ADP6360.DeviceDesc="Iomega Zip Zoom SCSI Host Adapter"
APA1460.DeviceDesc="Iomega Jaz & Zip Card PCMCIA SCSI Host Adapter"

; Advansys visible strings

ABPPCI.DriverDesc="Iomega Jaz Jet PCI SCSI Host Adapter"
instd1 = "Iomega Tools Install Diskette"
AdvaspiStr = "advaspi.sys	; Iomega ASPI Manager"
AdvancdStr = "advancd.sys	; Iomega CD-ROM Driver"
Advw32Str = ";By Iomega.INF: device=advw32.386"
