;***********************************************************************
;
; OEMSETUP.INF
;
;       Xircom CT-IIps Network Adapter Setup
;		Token Ring
;
; History:
;	Adapted by Richard E. Moore
;   Mar 3 1996  Rev 1.35   Updated for NT 4.0
;****************************************************************************************************

[Identification]
    OptionType = NetAdapter

[PlatformsSupported]
    ISA
    EISA
    MCA

[Options]
	CTNDNT

[OptionsTextENG]
    CTNDNT      = "Xircom CreditCard Token Ring"

[AllFileConstants]
GenericInfVersion  = " v1.35"
;  File names, etc. ----------------------------------------
UtilityInf      = "UTILITY.INF"
ParamInf        = "NCPARAM.INF"
subroutineinf   = "SUBROUTN.INF"
SoftwareType    = "driver"
Exit_Code       = 0
; EventLog Message File	 ----------------------------------------
NetEventDLL     = "%SystemRoot%\System32\netevent.dll"
IoLogMsgDLL     = "%SystemRoot%\System32\IoLogMsg.dll"
; Product Info ----------------------------------------
Manufacturer    = "Xircom"
; Flow control variables  ----------------------------------------
RUNDLLCODE		= 1
HOTPROGRAMPCMCIA = ""



[FileConstants-CTNDNT]
GenericAdapterName = "Xircom CreditCard Token Ring"
GenericDriverName  = "Xircom CreditCard Token Ring Driver"
GenericSysName     = "CTNDNT.SYS"
GenericName        = "CTNDNT"
; Product Info ----------------------------------------
ProductMajorVersion     = "2"
ProductMinorVersion     = "27"
ProductVersion  = $(ProductMajorVersion)"."$(ProductMinorVersion)
; Software  ----------------------------------------
ProductSoftwareName     = "CTNDNT"
ProductSoftwareDescription = "Xircom CreditCard Token Ring Driver"
ProductSoftwareImagePath = "\SystemRoot\System32\drivers\"$(GenericSysName)
NetRuleSoftwareType     = "ctndntSys ndisDriver ctndntDriver"
NetRuleSoftwareUse      = $(SoftwareType)
NetRuleSoftwareBindForm = """ctndntSys"" yes no container"
NetRuleSoftwareClass    = {"ctndntDriver basic"}
NetRuleSoftwareBindable = {"ctndntDriver ctndntAdapter non exclusive 100"}
; Hardware  ----------------------------------------
ProductHardwareName        = "CTNDNT"
ProductHardwareDescription = "Xircom CreditCard Token Ring"
NetRuleHardwareType        = "ctndnt ctndntAdapter"
NetRuleHardwareBindForm    = " yes yes container"
NetRuleHardwareClass       = {"ctndntAdapter basic"}
; Registry Key  ----------------------------------------
ProductKeyName  = $(!NTN_SoftwareBase)"\"$(Manufacturer)"\"$(ProductSoftwareName)"\CurrentVersion"
ParamKeyName    = $(!NTN_ServiceBase)"\"$(ProductHardwareName)"\Parameters"
; Tuple Information -----------------------------------
VERS1Manufacturer = "Xircom"
VERS1Product      = "CreditCard Token Ring"
VERS1Type		  = "CT-2"
PCMCIA			  = 1


[GeneralConstants]
;  Program flow control variables.
from      = ""
to        = ""
;  Return codes; Exit_Code is set to one of these
ExitCodeOk     = 0
ExitCodeCancel = 1
ExitCodeFatal  = 2
KeyNull         = ""
MAXIMUM_ALLOWED   = 33554432
RegistryErrorIndex = NO_ERROR
KeyProduct      = ""
KeyParameters   = ""
TRUE            = 1
FALSE           = 0
NoTitle            = 0
ExitState   = "Active"
OldVersionExisted = $(FALSE)
DriverPath      = $(!STF_NTPATH)\drivers




[date]
    ; Now is a list which contains { Sec from 1-1-1970, Year, Month, Day, Hour,
    ; Minute, Second }
    Now = {} ? $(!LIBHANDLE) GetSystemDate


;---------------------------------------------------------------------------
; 1. Identify
;
; DESCRIPTION:   To verify that this INF deals with the same type of options
;                as we are choosing currently.
;
; INPUT:         None
;
; OUTPUT:        $($R0): STATUS: STATUS_SUCCESSFUL
;                $($R1): Option Type (COMPUTER ...)
;                $($R2): Diskette description
;---------------------------------------------------------------------------

[Identify]
    ;
    ;
    read-syms Identification

    set Status     = STATUS_SUCCESSFUL
    set Identifier = $(OptionType)
    set Media      = #("Source Media Descriptions", 1, 1)

    Return $(Status) $(Identifier) $(Media)

;------------------------------------------------------------------------
; 2. ReturnOptions:
;
; DESCRIPTION:   To return the option list supported by this INF and the
;                localised text list representing the options.
;
;
; INPUT:         $($0):  Language used. ( ENG | FRN | ... )
;
; OUTPUT:        $($R0): STATUS: STATUS_SUCCESSFUL |
;                                STATUS_NOLANGUAGE
;                                STATUS_FAILED
;                                STATUS_NOTSUPPORTED
;
;                $($R1): Option List
;                $($R2): Option Text List
;------------------------------------------------------------------------

[ReturnOptions]
    ;
    ;
    set Status        = STATUS_FAILED
    set OptionList     = {}
    set OptionTextList = {}

    ;
    ; Check if the language requested is supported
    ;
    set LanguageList = ^(LanguagesSupported, 1)
    Ifcontains(i) $($0) in $(LanguageList)
        ;
        ; Check if the platforms requested is supported
        ;
        ifstr(i) $($1) == ""
                        goto returnoptions
        endif

        set PlatformList = ^(PlatformsSupported, 1)
        Ifcontains(i) $($1) in $(PlatformList)
                        goto returnoptions
        else
                        set Status = STATUS_NOTSUPPORTED
                        goto finish_ReturnOptions
        endif
    else
                set Status = STATUS_NOLANGUAGE
                goto finish_ReturnOptions
    endif

    ;
    ; form a list of all the options and another of the text representing
    ;

returnoptions = +
    set OptionList     = ^(Options, 1)
    set OptionTextList = ^(OptionsText$($0), 1)
    set Status         = STATUS_SUCCESSFUL

finish_ReturnOptions = +
    Return $(Status) $(OptionList) $(OptionTextList)

;------------------------------------------------------------------------
;
; InstallOption:
;
;      This section is shelled to by main installation processing
;      or by NCPASHEL.INF during reconfig, removal, update, etc.
;
;
; FUNCTION:  To copy files representing Options
;            To configure the installed option
;            To update the registry for the installed option
;
; INPUT:     $($0):  Language to use
;            $($1):  OptionID to install
;            $($2):  SourceDirectory
;            $($3):  AddCopy  (YES | NO)
;            $($4):  DoCopy   (YES | NO)
;            $($5):  DoConfig (YES | NO)
;
; OUTPUT:    $($R0): STATUS: STATUS_SUCCESSFUL |
;                            STATUS_NOLANGUAGE |
;                            STATUS_USERCANCEL |
;                            STATUS_FAILED
;
;------------------------------------------------------------------------
[InstallOption]
    ;
    ; Set default values for
    ;
    set Status   = STATUS_FAILED
    ;
    ; extract parameters
    ;
    set Option   = $($1)
    set SrcDir   = $($2)
    set AddCopy  = $($3)
    set DoCopy   = $($4)
    set DoConfig = $($5)

    Set !DebugOutputControl = 1

    ;
    ; Check if the language requested is supported
    ;
    set LanguageList = ^(LanguagesSupported, 1)
    Ifcontains(i) $($0) NOT-IN $(LanguageList)
        Return STATUS_NOLANGUAGE
    endif

    set-subst LF = "\n"

    read-syms GeneralConstants
	read-syms AllFileConstants
    read-syms FileConstants"-"$(Option)
    read-syms DialogConstants$(!STF_LANGUAGE)"-"$(Option)
    ifstr(i) $(!NTN_Origination) == "NCPA"
        set Continue = $(OK)
    endif

    read-syms AllFileConstants$(!STF_LANGUAGE)
    read-syms FileConstants$(!STF_LANGUAGE)"-"$(Option)

    detect date

    set-title  $(FunctionTitle)

    set to   = Begin
    set from = Begin
;
;  Assume all is well.
;
    set CommonStatus = STATUS_SUCCESSFUL

    EndWait

;
;   Set up the operation-mode-based variables and gaily welcome
;   the user.  If the "install mode" variable is improperly set,
;   assume this is a new installation.
;

Begin = +
    Set ActivateDetection = FALSE

    Ifstr(i) $(!NTN_InstallMode) == deinstall
        set StartLabel = removeadapter
    else-Ifstr(i) $(!NTN_InstallMode) == Update
        set StartLabel = UpgradeSoftware
    else-Ifstr(i) $(!NTN_InstallMode) == bind
        set StartLabel = bindingadapter
    else-Ifstr(i) $(!NTN_InstallMode) == configure
;        set ActivateDetection = TRUE
        set StartLabel = configureadapter
        ;
        ;   You cannot config the software component
        ;
        Ifstr(i) $(ProductKeyName) == $(!NTN_RegBase)
            ;Debug-Output "Cannot configure the software."
            Shell $(UtilityInf),RegistryErrorString,CANNOT_CONFIGURE_SOFTWARE
            ifint $($ShellCode) != $(!SHELL_CODE_OK)
                Debug-Output "ShellCode error: cannot get an error string."
                goto ShellCodeError
            endif
            set Error = $($R0)
            set from = end
            set to = end
            goto nonfatalinfo
        endif
    else
;        set ActivateDetection = TRUE
        set StartLabel = installadapter
        set OEM_ABANDON_OPTIONS = {}
        set OEM_ABANDON_SOFTWARE = FALSE
        set OEM_ABANDON_ON = TRUE
    endif


    ;  set the [Default values]

    set IRQValue 					= *($(IRQList), 3)	  				; IRQ Level      = 10
    set IOBaseAddrValue 			= *($(IOBaseAddrList), 16)	 		; IOBase Address = 0x300
    set MemoryAddrValue 			= *($(MemoryAddrList), 49)	 		; Memory Address =	0xD0000
    set LineSpeedValue  			= *($(LineSpeedList), 0)	 		;

    Set from = $(fatal)
    Set to = $(fatal)
    Goto $(StartLabel)

;-----------------------------------------------
; Installation Section
;-----------------------------------------------

installadapter = +
;
;   First, check whether the same version of the software exists
;
    OpenRegKey $(!REG_H_LOCAL) "" $(ProductKeyName) $(MAXIMUM_ALLOWED) KeyProduct

    Ifstr $(KeyProduct) != $(KeyNull)
        ;
        ; Same version already existed in the local machine
        ; Popup the dialog and ask the user whether he wants to continue
        ;
        CloseRegKey $(KeyProduct)

        ifstr(i) !(NTN_RegBase) == $(ProductKeyName)
           ;
           ; Cannot Install the same software again
           ;
           Shell $(UtilityInf), VerExistedDlg, $(ProductSoftwareTitle),+
               $(ProductVersion)
           ifint $($ShellCode) != $(!SHELL_CODE_OK)
               Debug-Output "ShellCode error: cannot get an error string."
               goto ShellCodeError
           endif

           goto end
        else
           ;
           ; Add a new adapter card?
           ;
           Shell $(UtilityInf), CardExistedDlg

           ifint $($ShellCode) != $(!SHELL_CODE_OK)
               Debug-Output "ShellCode error: cannot get an error string."
               goto ShellCodeError
           endif

           ifstr(i) $($R1) != "OK"
               goto end
           endif
           set OldVersionExisted = $(TRUE)
        endif
    endif

;
;  dll load addition
;
    Shell $(UtilityInf), DoAskSource, $(!STF_CWDDIR), $(SrcDir) NO

    Ifint $($ShellCode) != $(!SHELL_CODE_OK)
        Goto ShellCodeError
    Else-Ifstr(i) $($R0) == STATUS_FAILED
        Shell $(UtilityInf) RegistryErrorString "ASK_SOURCE_FAIL"
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            goto ShellCodeError
        endif
        set Error = $($R0)
        Goto fatal
    Else-Ifstr(i) $($R0) == STATUS_USERCANCEL
        Goto successful
    Endif

    Set SrcDir = $($R1)

    install "Install-Dll"

    goto adaptersetup

;-----------------------------------------------
; Configuration Section
;-----------------------------------------------
;
;   Get the current values of all the parameters
;
configureadapter = +
    Ifstr $(KeyProduct) == $(KeyNull)
        OpenRegKey $(!REG_H_LOCAL) "" $(!NTN_RegBase) $(MAXIMUM_ALLOWED) KeyProduct
        Ifstr $(KeyProduct) == $(KeyNull)
            set RegistryErrorIndex = CANNOT_FIND_COMPONENT_SERVICE
            Debug-Output "Cannot find component product key"
            goto fatalregistry
        Endif
    Endif

    ;
    ; Get the other parameters;  they're attached to the service parameters key
    ;
    Debug-Output "INF: Shelling to FindService"
    Shell $(UtilityInf) FindService, $(KeyProduct)
    Ifint $($ShellCode) != $(!SHELL_CODE_OK)
        Debug-Output "INF: FindService shell failure"
        Goto ShellCodeError
    Endif
    Ifstr(i) $($R0) != NO_ERROR
        Debug-Output "INF: FindService Shell error: "$($R0)
        Goto fatalregistry
    endif

    Set KeyParameters = $($R2)

    ;
    ;  We don't need the services key, so close it.
    ;
    CloseRegKey $($R1)

    Ifstr $(KeyParameters) == $(KeyNull)
        set RegistryErrorIndex = CANNOT_FIND_COMPONENT_SERVICE
        Debug-Output "Cannot find component service"
        goto fatalregistry
    endif

    set OldVersionExisted = $(TRUE)

    set ValueName = ""
    set ValueData = ""
    set ValueStr  = ""
    set ValueList = {}


    ;
    ; Get the old values from the Registry	[Get Values]
    ; *********************************************************
    EnumRegValue $(KeyParameters) ValueList
    ForListDo $(ValueList)
		set ValueItem = $($)
		set ValueName = *($(ValueItem),1)
		set ValueData = *($(ValueItem),4)
		ifstr(i) $(ValueName) == "IoBaseAddress"
		    set IOBaseAddrIndex = $(ValueData)
	    else-ifstr(i) $(ValueName) == "InterruptNumber"
		    set IRQValueIndex = $(ValueData)
	    else-ifstr(i) $(ValueName) == "PCCARDAttributeMemoryAddress"
		    set MemoryAddrIndex = $(ValueData)
	    else-ifstr(i) $(ValueName) == "LineSpeed"
		    set LineSpeedIndex = $(ValueData)
		endif
    EndForListDo

    set IRQValue = *($(IRQList), ~($(IRQValues),$(IRQValueIndex)))
    ifstr(i) $(IRQValue) == ""
		set IRQValue = *($(IRQList), 2)
    endif

    set MemoryAddrValue = *($(MemoryAddrList), ~($(MemoryAddrValues),$(MemoryAddrIndex)))
    ifstr(i) $(MemoryAddrValue) == ""
		set MemoryAddrValue = *($(MemoryAddrValues), 2)
    endif

    set IOBaseAddrValue = *($(IOBaseAddrList), ~($(IOBaseAddrValues),$(IOBaseAddrIndex)))
    ifstr(i) $(IOBaseAddrValue) == ""
		set IOBaseAddrValue = *($(IOBaseAddrList), 1)
    endif

    set LineSpeedValue = *($(LineSpeedList), ~($(LineSpeedValues),$(LineSpeedIndex)))
    ifstr(i) $(LineSpeedValue) == ""
		set LineSpeedValue = *($(LineSpeedList), 1)
    endif

	 

    ;  Save the settings as they were read from the Registry.

;    Shell $(ParamInf) Param_SaveValues
;    Set CurrParamSettings = $($R0)
;
;   Put up the adapter configuration dialog if necessary.
;
;   Note that $(CurrParamSettings) has the old known parameter values.
;
adaptersetup = +


    ;Shell "" DebugConfiguration "before displaying dialog"

    Set from = adapteroptions


adapteroptions = +

    LoadLibrary "disk 1" $(DialogDllName) hLib
    read-syms FileDependentDlg$(!STF_LANGUAGE)"-"$(Option)
	set ENABLER = 0

	ifint $(RUNDLLCODE) == 1
		ifint $(PCMCIA) == 1
		    LibraryProcedure ENABLER, $(hLib), EnablerRunning 		; check for enabler type
		    ifint $(ENABLER) == 1
				set Static1Label = "Configuring driver for Microsoft Enabler"
		    else-ifint $(ENABLER) == 2
				set Static1Label = "Configuring driver for third party Card & Socket Services"
		    else
				set Static1Label = "Configuring driver for Xircom Enabler"
			endif
		endif
	endif

    ui start "InputDlg"  $(hLib)

    set ExitButton      = $(ButtonPressed)
    ;Debug-Output " ButtonPressed "$(ButtonPressed)
    ;Debug-Output " DLGEVENT "$(DLGEVENT)
	FreeLibrary $(hLib)

	ifstr(i) $(DLGEVENT) == "CONTINUE"
		set IOBaseAddrIndex  = $(Combo1Out)
        set MemoryAddrIndex  = $(Combo2Out)
		set IRQValueIndex    = $(Combo3Out)
		set LineSpeedIndex   = $(Combo4Out)
        set ExitButton       = $(ButtonPressed)
	else-ifstr(i) $(DLGEVENT) == "EXIT"
		set CommonStatus = STATUS_USERCANCEL
		ui pop 1
		goto end
    else
		set CommonStatus = STATUS_USERCANCEL
		ui pop 1
		Debug-Output "Action: unknown. Bye."
		goto end
    endif


;
;   If installing, go create the necessary keys;
;   if configuring, they're already open.
;
skipoptions =+

    ifint $(OldVersionExisted) == $(TRUE)
        ifstr(i) $(!NTN_InstallMode) == configure
            goto writeparameters
        endif
    endif
    StartWait
    ;
    ; Add Software Component
    ;
    ifint $(OldVersionExisted) == $(FALSE)

        ifstr(i) $(!NTN_InstallMode) == "install"
           Ifstr(i) $(DoCopy) == "YES"

              Shell $(UtilityInf), DoAskSource, $(!STF_CWDDIR), $(SrcDir) YES

              Ifint $($ShellCode) != $(!SHELL_CODE_OK)
                  Goto ShellCodeError
              Else-Ifstr(i) $($R0) == STATUS_FAILED
                  Shell $(UtilityInf) RegistryErrorString "ASK_SOURCE_FAIL"
                  ifint $($ShellCode) != $(!SHELL_CODE_OK)
                      goto ShellCodeError
                  endif
                  set Error = $($R0)
                  Goto fatal
              Else-Ifstr(i) $($R0) == STATUS_USERCANCEL
                  Goto successful
              Endif

              Set SrcDir = $($R1)

           Endif

           install "Install-Option"

           ifstr(i) $(STF_INSTALL_OUTCOME) != STF_SUCCESS
              Shell $(UtilityInf) RegistryErrorString "UNABLE_COPY_FILE"
              ifint $($ShellCode) != $(!SHELL_CODE_OK)
                  goto ShellCodeError
              endif
              set Error = $($R0)
              goto fatal
           endif
        endif



        Shell $(UtilityInf), AddSoftwareComponent, $(Manufacturer), +
            $(ProductSoftwareName), +
            $(ProductSoftwareName), +
            $(ProductSoftwareTitle), $(STF_CONTEXTINFNAME), +
            $(ProductSoftwareImagePath), "kernel", "NDIS", {}, "",+
            $(NetEventDLL)

        Set OEM_ABANDON_SOFTWARE = TRUE

        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            Debug-Output "ShellCode error"
            goto ShellCodeError
        endif
        ;
        ;   At this point:
        ;     $R1 contains the product version key handle;
        ;     $R2 contains the NetRules subkey handle;
        ;     $R3 contains the new Services key handle; and
        ;     $R4 contains the Parameters key
        ;     $R5 contains the Linkage Key
        ;
        set RegistryErrorIndex = $($R0)
        set KeyProduct      = $($R1)
        Set SoftNetRulesKey = $($R2)
        CloseRegKey $($R3)
        CloseRegKey $($R4)
        CloseRegKey $($R5)

        Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
            EndWait
            Debug-Output "Registry error: add software components"
            CloseRegKey $(KeyProduct)
            CloseRegKey $(SoftNetRulesKey)
            goto fatalregistry
        endif

        set NewValueList = {{SoftwareType,$(NoTitle),$(!REG_VT_SZ),$(SoftwareType)},+
                           {MajorVersion,$(NoTitle),$(!REG_VT_DWORD),$(ProductMajorVersion)},+
                           {MinorVersion,$(NoTitle),$(!REG_VT_DWORD),$(ProductMinorVersion)},+
                           {Title,$(NoTitle),$(!REG_VT_SZ),$(ProductSoftwareTitle)},+
                           {Description,$(NoTitle),$(!REG_VT_SZ),$(ProductSoftwareDescription)},+
                           {ServiceName,$(NoTitle),$(!REG_VT_SZ),$(ProductSoftwareName)},+
                           {InstallDate,$(NoTitle),$(!REG_VT_DWORD),*($(Now),1)}}

        Shell  $(UtilityInf), AddValueList, $(KeyProduct), $(NewValueList)
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            Debug-Output "ShellCode error."
            goto ShellCodeError
        endif

        set RegistryErrorIndex = $($R0)

        Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
            EndWait
            Debug-Output "Registry error: add value list."
            CloseRegKey $(KeyProduct)
            CloseRegKey $(SoftNetRulesKey)
            goto fatalregistry
        endif

        set NewValueList = {{type,$(NoTitle),$(!REG_VT_SZ),$(NetRuleSoftwareType)},+
                            {use,$(NoTitle),$(!REG_VT_SZ),$(NetRuleSoftwareUse)}, +
                            {bindform,$(NoTitle),$(!REG_VT_SZ),$(NetRuleSoftwareBindForm)}, +
                            {class,$(NoTitle),$(!REG_VT_MULTI_SZ),$(NetRuleSoftwareClass)}, +
                            {bindable,$(NoTitle),$(!REG_VT_MULTI_SZ),$(NetRuleSoftwareBindable)}, +
                            {InfOption,$(NoTitle),$(!REG_VT_SZ),$(Option)}}

        Shell  $(UtilityInf), AddValueList, $(SoftNetRulesKey), $(NewValueList)
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            Debug-Output "ShellCode error."
            goto ShellCodeError
        endif

        set RegistryErrorIndex = $($R0)

        CloseRegKey $(KeyProduct)
        CloseRegKey $(SoftNetRulesKey)

        Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
            EndWait
            Debug-Output "Resgitry error: add value list."
            goto fatalregistry
        endif
    endif
;
;   Create the HARDWARE\Netcard region and its corresponding service
;
    Shell $(UtilityInf), AddHardwareComponent, $(ProductHardwareName),$(STF_CONTEXTINFNAME),$(ProductKeyName)

    ifint $($R4) != -1
        Set OEM_ABANDON_OPTIONS = >($(OEM_ABANDON_OPTIONS), $(!NTN_SoftwareBase)"\Microsoft\Windows NT\CurrentVersion\NetworkCards\"$($R4))
    endif

    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        Debug-Output "Cannot add hardware component"
        goto ShellCodeError
    endif

    set RegistryErrorIndex = $($R0)

    Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
        EndWait
        Debug-Output "Registry error: add hardware component"
        CloseRegKey $($R1)
        CloseRegKey $($R2)
        CloseRegKey $($R3)
        goto fatalregistry
    endif

;
;   At this point:
;     $R1  Registry key variable for HARDWARE\Netcard\(n)
;     $R2  Registry key variable for HARDWARE\Netcard\(n)\\NetRules
;     $R3  Registry key handle for <service>\Parameters key
;     $R4  Adapter number assigned to adapter
;     $R5  Service name generated by combining svc name with adapter number
;
    set KeyParameters = $($R3)
    set KeyAdapterRules = $($R2)
    set AdapterNumber = $($R4)

    set NewValueList = {{Manufacturer,$(NoTitle),$(!REG_VT_SZ),$(Manufacturer)},+
                       {Title,$(NoTitle),$(!REG_VT_SZ),"["$($R4)"] "$(ProductHardwareTitle)},+
                       {Description,$(NoTitle),$(!REG_VT_SZ),$(ProductHardwareDescription)},+
                       {ProductName,$(NoTitle),$(!REG_VT_SZ),$(ProductHardwareName)},+
                       {ServiceName,$(NoTitle),$(!REG_VT_SZ),$($R5)},+
                       {InstallDate,$(NoTitle),$(!REG_VT_DWORD),*($(Now),1)}}

    Shell  $(UtilityInf), AddValueList, $($R1), $(NewValueList)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        Debug-Output "ShellCode error"
        goto ShellCodeError
    endif

    CloseRegKey $($R1)

    set TempProdName = """"$(ProductHardwareName)$(AdapterNumber)""""
    set TempBindForm = $(TempProdName)$(NetRuleHardwareBindForm)

    set NewValueList = {{type,$(NoTitle),$(!REG_VT_SZ),$(NetRuleHardwareType)},+
                        {bindform,$(NoTitle),$(!REG_VT_SZ),$(TempBindForm)}, +
                        {class,$(NoTitle),$(!REG_VT_MULTI_SZ),$(NetRuleHardwareClass)}, +
                        {InfOption,$(NoTitle),$(!REG_VT_SZ),$(Option)}}

    Shell  $(UtilityInf), AddValueList, $(KeyAdapterRules), $(NewValueList)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        Debug-Output "ShellCode error."
        goto ShellCodeError
    endif

    set RegistryErrorIndex = $($R0)

    Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
        EndWait
        Debug-Output "Resgitry error: add value list."
        CloseRegKey $(KeyParameters)
        CloseRegKey $(KeyAdapterRules)
        goto fatalregistry
    endif

    CloseRegKey $(KeyAdapterRules)

    goto writeparameters
;
;   REQUIRED:   $(KeyParameters) contains service Parameters key handle
;
writeparameters = +
    Shell $(UtilityInf), GetBusTypeNum
    set BusTypeNum = $($R1)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        Debug-Output "ShellCode error."
        goto ShellCodeError
    endif
;
;   Add the rest of the parameters to the Services area
;
    set MemoryAddrValue  = *($(MemoryAddrValues),  ~($(MemoryAddrList), $(MemoryAddrIndex)))
    set-add CommonMemoryAddrValue  = $(MemoryAddrValue), 4096
    set IRQValue         = *($(IRQValues),         ~($(IRQList),        $(IRQValueIndex)))
    set IOBaseAddrValue  = *($(IOBaseAddrValues),  ~($(IOBaseAddrList), $(IOBaseAddrIndex)))
    set LineSpeed	     = *($(LineSpeedValues),   ~($(LineSpeedList),  $(LineSpeedIndex)))
    set IOLengthValue	 = 31
    set NewValueList     = {{IoBaseAddress,           $(NoTitle),$(!REG_VT_DWORD),$(IOBaseAddrValue)},+
       	                    {IoLength,        		  $(NoTitle),$(!REG_VT_DWORD), $(IOLengthValue)},+
       	                    {PCCARDAttributeMemoryAddress, $(NoTitle),$(!REG_VT_DWORD),$(MemoryAddrValue)},+
       	                    {PCCARDAttributeMemorySize,    $(NoTitle),$(!REG_VT_DWORD),4096},+
       	                    {PCCARDAttributeMemoryOffset,  $(NoTitle),$(!REG_VT_DWORD),0},+
       	                    {MemoryMappedBaseAddress, $(NoTitle),$(!REG_VT_DWORD),$(CommonMemoryAddrValue)},+
       	                    {MemoryMappedSize,        $(NoTitle),$(!REG_VT_DWORD),4096},+			 ;4k
       	                    {PCCARDMemoryWindowOffset, $(NoTitle),$(!REG_VT_DWORD),131072},+		 ;0x20000
       	                    {InterruptNumber,         $(NoTitle),$(!REG_VT_DWORD),$(IRQValue)},+
                            {BusType,                 $(NoTitle),$(!REG_VT_DWORD),$(BusTypeNum)},+
                            {BusNumber,               $(NoTitle),$(!REG_VT_DWORD),0},+
							{ResourceManager,         $(NoTitle),$(!REG_VT_DWORD),$(ENABLER)},+
							{MediaType,               $(NoTitle),$(!REG_VT_DWORD),2},+
							{LineSpeed,               $(NoTitle),$(!REG_VT_DWORD),$(LineSpeed)},+
                            {PCMCIA,                  $(NoTitle),$(!REG_VT_DWORD),1}}


    Shell  $(UtilityInf), AddValueList, $(KeyParameters), $(NewValueList)
    CloseRegKey $(KeyParameters)

	; --------------------------------------------------------------------------------
	; Reprogram the PCMCIA slot with the new parameters
	; Should only be done during first time installation of NT, and if Xircom card was found
	; For now, we do it always...
	; --------------------------------------------------------------------------------
	; Call out to the PCMCIA driver only if we're loading a PCMCIA device
	ifint $(RUNDLLCODE) == 1
		ifint $(PCMCIA) == 1
			ifint $(ENABLER) == 1
				ifint $(HOTPROGRAMPCMCIA) == 1
					ifint $(SLOTFOUND) == 1			; and a Xircom card was found in a slot
						LoadLibrary "disk 1" $(DialogDllName) hLib
						Debug-Output "Enabling network resources"
						ifstr(i) $(Option) == CM2NDIS3
							LibraryProcedure STATUS, $(hLib), SetupSlot $(SLOT) 0 $(IRQValue) $(IOBaseAddrValue) $(IOLengthValue) $(MemoryAddrValue) 4096 0
						else
							LibraryProcedure STATUS, $(hLib), SetupSlot $(SLOT) $(IRQValue) 0 $(IOBaseAddrValue) $(IOLengthValue) $(MemoryAddrValue) 4096 0
						endif
						Debug-Output "SetupSlot: "$(STATUS)
						FreeLibrary $(hLib)
					endif
				endif
			endif
		endif
	endif

	; --------------------------------------------------------------------------------
	; Write the parameters to the PCMCIA database section, iff running MS Enabler
	; Add/replace only the parts for the CT2
	; --------------------------------------------------------------------------------
	set PCMCIADatabaseKeyName = $(!NTN_ServiceBase)"\Pcmcia\DataBase"
	set PCMCIADatabaseXircomKeyName = $(PCMCIADatabaseKeyName)"\Xircom"
    OpenRegKey $(!REG_H_LOCAL) "" $(PCMCIADatabaseKeyName) $(MAXIMUM_ALLOWED) PCMCIADatabaseKey

	ifstr $(PCMCIADatabaseKey) == $(NULL)
		;Debug-Output "Pcmcia\DataBase not present"
	else ; PCMCIA.sys is installed and registry has database section in it.
		; Try to open Xircom section.  Delete it if found
    	OpenRegKey $(!REG_H_LOCAL) "" $(PCMCIADatabaseKeyName)"\Xircom" $(MAXIMUM_ALLOWED) PCMCIADatabaseXircomKey
		ifstr $(PCMCIADatabaseXircomKey) == $(NULL) ; open failed, so create Xircom subkey
			CreateRegKey $(PCMCIADatabaseKey) {"Xircom", 0, 0} "" $(MAXIMUM_ALLOWED) "" PCMCIADatabaseXircomKey
		endif

		; Open "CreditCard Token Ring"  aka $(VERS1Product) ----------------------------------------------------------------------
    	OpenRegKey $(!REG_H_LOCAL) "" $(PCMCIADatabaseXircomKeyName)"\"$(VERS1Product) $(MAXIMUM_ALLOWED) PCMCIADatabaseXircomCT2Key
		ifstr $(PCMCIADatabaseXircomCT2Key) == $(NULL)
			CreateRegKey $(PCMCIADatabaseXircomKey) {$(VERS1Product), 0, 0} "" $(MAXIMUM_ALLOWED) 0 PCMCIADatabaseXircomCT2Key
		endif

		; Do the TokenRing --------------------------------------------------------------------------------------
		SetRegValue $(PCMCIADatabaseXircomCT2Key) {Driver, 0, $(!REG_VT_SZ),"ctndnt"}
		SetRegValue $(PCMCIADatabaseXircomCT2Key) {AttributeMemorySize, 0, $(!REG_VT_DWORD),4096}
		SetRegValue $(PCMCIADatabaseXircomCT2Key) {DeviceType, 0, $(!REG_VT_SZ),"NET"}
		CloseRegKey $(PCMCIADatabaseXircomCT2Key)
	    CloseRegKey $(PCMCIADatabaseXircomKey)
    	CloseRegKey $(PCMCIADatabaseKey)
	endif


    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        Debug-Output "ShellCode error."
        goto ShellCodeError
    endif

    set RegistryErrorIndex = $($R0)

    Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
        Debug-Output "Registry error: Add value list"
        goto fatalregistry
    endif

    EndWait

    goto successful

;-----------------------------------------------
; Binding section
;-----------------------------------------------
bindingadapter =+
    set Error = "Binding: Sorry, not yet implemented."
    goto fatal

;-----------------------------------------------
; Removeadapter section
;-----------------------------------------------

removeadapter = +
    Ifstr(i) $(ProductKeyName) == $(!NTN_RegBase)
        ; Remove Software Component
        Shell $(UtilityInf), RemoveSoftwareComponent, $(Manufacturer), +
            $(ProductSoftwareName)
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            Debug-Output "ShellCode error"
            goto ShellCodeError
        endif

        set RegistryErrorIndex = $($R0)

        Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
            goto fatalregistry
        endif
    else
        Shell $(UtilityInf), RemoveHardwareComponent, $(Manufacturer), +
            $(ProductSoftwareName), $(!NTN_RegBase)
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            Debug-Output "ShellCode error"
            goto ShellCodeError
        endif

        set RegistryErrorIndex = $($R0)

        Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
            goto fatalregistry
        endif


    endif

    goto end

;-----------------------------------------------
; Upgrade Software section
;-----------------------------------------------

UpgradeSoftware = +
    ;
    ; First determine whether we want to do upgrade or update for software
    ; or hardware component. Then we will determine whether the Mode is
    ; update or upgrade.
    ;
    ; If the same version of the product existed in the registry, we do
    ; update. Otherwise, we will do a upgrade
    ;
    ifstr(i) $(ProductKeyName) == $(!NTN_RegBase)
        ; Upgrade software component
        ;
        ; see whether the same version exist or not
        ;
        OpenRegKey $(!REG_H_LOCAL) "" $(ProductKeyName) $(MAXIMUM_ALLOWED) KeyProduct

        Ifstr $(KeyProduct) != $(KeyNull)
            GetRegValue $(KeyProduct),"MajorVersion", VersionInfo
            set Version = *($(VersionInfo), 4)

            ;
            ; Update the binaries
            ;
            Shell $(UtilityInf), GetInfFileNameFromRegistry, $(KeyProduct)

            ifint $($ShellCode) != $(!SHELL_CODE_OK)
                Debug-Output "ShellCode error"
                goto ShellCodeError
            endif

            set !UG_Filename = $($R0)

            ifstr(i) $(!UG_Filename) != ""
                install "Install-Update"
                ifstr(i) $(STF_INSTALL_OUTCOME) != STF_SUCCESS
                    goto fatal
                endif
            endif

            ; Upgrade the version number
            ;
            SetRegValue $(KeyProduct) {MajorVersion,$(NoTitle),$(!REG_VT_SZ),$(ProductMajorVersion)}
            SetRegValue $(KeyProduct) {MinorVersion,$(NoTitle),$(!REG_VT_SZ),$(ProductMinorVersion)}

            ;
            ; do nothing for update
            ;
            ifint $(Version) != $(ProductVersion)
               ;
               ; If the major version number is not the same,
               ; it is major upgrade. So let Upgrade the product
               ;
               ;
               ; make other upgrade change if necessary
               ;
            endif
            CloseRegKey $(KeyProduct)
        else
            ;
            ; Cannot Open software key, goto ERROR
            ;
            goto fatalregistry
        endif
    else
        ;
        ; upgrade/update hardware component
        ; There is no different between upgrade and update for hardware
        ; component
        ;
        ; 1. Get the Service Name
        ; 2. Change the NetRule section if necessary
        ;
        OpenRegKey $(!REG_H_LOCAL) "" $(!NTN_RegBase) +
              $(MAXIMUM_ALLOWED) NetworkCardKey
        Ifstr(i) $(NetworkCardKey) != $(KeyNull)
            ;
            ; Get Service name
            ;
            GetRegValue $(NetworkCardKey),"ServiceName", ServiceNameInfo
            set ServiceName = *($(ServiceNameInfo), 4)

            ;
            ; Change the NetRule if necessary
            ;
            OpenRegKey $(NetworkCardKey) "" "NetRules" +
                $(MAXIMUM_ALLOWED) NetRuleKey
            Ifstr(i) $(NetRuleKey) != $(KeyNull)
                ;
                ; Make the change....
                ;
            else
                ;
                ; Error, cannot open net rules key
                ;
                goto fatalregistry
            endif

            CloseRegKey $(NetRules)
            CloseRegKey $(NetworkCardKey)
        else
            ;
            ; Error, cannot open network card key
            ;
            goto fatalregistry
        endif
        ;
        ; 3. Change the service section of the hardware. i.e.,
        ;    ParameterName change, value change, etc.
        ;
        OpenRegKey $(!REG_H_LOCAL) "" +
              $(!NTN_ServiceBase)"\"$(ServiceName) +
              $(MAXIMUM_ALLOWED) ServiceKey

        Ifstr(i) $(ServiceKey) != $(KeyNull)
            ;
            ; Get the ServiceKey to change the Start value
            ; or Type value. Or open Parameters key to
            ; change the hardware parameters if necessary.
            ;
            CloseRegKey $(ServiceKey)
        else
            ;
            ; Error, cannot open network card key
            ;
            goto fatalregistry
        endif
    endif

    goto end
    ;
    ; End of Upgrade Software
    ;

;
;  Escape hatches
;
successful = +
    goto end

abandon = +
    ForListDo $(OEM_ABANDON_OPTIONS)
        Shell $(UtilityInf), RemoveHardwareComponent, $(Manufacturer), +
            $(ProductSoftwareName), $($)
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            Debug-Output "ShellCode error"
            goto ShellCodeError
        endif

        set RegistryErrorIndex = $($R0)

        Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
            goto fatalregistry
        endif
    EndForListDo

    Ifstr(i) $(OEM_ABANDON_SOFTWARE) == TRUE
        ; Remove Software Component
        Shell $(UtilityInf), RemoveSoftwareComponent, $(Manufacturer), +
            $(ProductSoftwareName), FALSE
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            Debug-Output "ShellCode error"
            goto ShellCodeError
        endif

        set RegistryErrorIndex = $($R0)

        Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
            goto fatalregistry
        endif
    endif

    goto end

;
; warning display
;
warning = +
    Shell $(subroutineinf) SetupMessage, $(!STF_LANGUAGE), "WARNING", $(Error)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        goto ShellCodeError
    endif
    ifstr(i) $($R1) == "OK"
        goto $(to)
    else-ifstr(i) $($R1) == "CANCEL"
        goto $(from)
    else
        goto "end"
    endif
;
; non fatal error display
;
nonfatalinfo = +
    Set Severity = STATUS
    Set CommonStatus = STATUS_USERCANCEL
    goto nonfatalmsg
nonfatal = +
    Set Severity = NONFATAL
    goto nonfatalmsg
nonfatalmsg = +
    ifstr(i) $(Error) == ""
        Set Severity = NONFATAL
        Shell $(UtilityInf) RegistryErrorString "SETUP_FAIL"
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            goto ShellCodeError
        endif
        set Error = $($R0)
    endif
    Shell $(subroutineinf) SetupMessage, $(!STF_LANGUAGE), $(Severity), $(Error)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        goto ShellCodeError
    endif
    ifstr(i) $($R1) == "OK"
        goto $(from)
    else
        goto "end"
    endif

;
;  Registry is broken
;
fatalregistry = +
    Shell $(UtilityInf) RegistryErrorString $(RegistryErrorIndex)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        goto ShellCodeError
    endif
    set Error = $($R0)
    goto fatal
;
;  Netcard detection failure
;
fataldetect = +
    Shell $(UtilityInf),RegistryErrorString,CANNOT_DETECT
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        Debug-Output "ShellCode error: cannot get an error string."
        goto ShellCodeError
    endif
    set Error = $($R0)
    Goto fatal
;
; fatal error display
;
fatal = +
    ifstr(i) $(Error) == ""
        Shell $(UtilityInf) RegistryErrorString "SETUP_FAIL"
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            goto ShellCodeError
        endif
        set Error = $($R0)
    endif
    Shell $(subroutineinf) SetupMessage, $(!STF_LANGUAGE), "FATAL", $(Error)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
        goto ShellCodeError
    endif

    goto setfailed

;
;  Shelling error
;
ShellCodeError = +
    set DlgType      = "MessageBox"
    set STF_MB_TITLE = $(ShellCodeErrorTitle)
    set STF_MB_TEXT  = $(ShellCodeErrorText)
    set STF_MB_TYPE  = 1
    set STF_MB_ICON  = 3
    set STF_MB_DEF   = 1
    ui start "Error Message"
    goto setfailed

setfailed = +
    set CommonStatus = STATUS_FAILED
    ;
    ; if OEM_ABANDON_ON == TRUE, then remove the registry entries
    ;
    ifstr(i) $(OEM_ABANDON_ON) == TRUE
        set OEM_ABANDON_ON = FALSE
        goto abandon
    endif
    goto end

end = +
    goto term

term = +

    Return $(CommonStatus)

[DebugConfiguration]

    Set InfName = "OEMSETNT.INF"
    ;Debug-Output $(InfName)" **CONFIGURATION STATE: "$($0)
    ;Debug-Output $(InfName)" IRQ_Level is "$(!p:IRQ_Level)
    ;Debug-Output $(InfName)" IOBaseAddrValue is "$(!p:IOBaseAddrValue)
    ;Debug-Output $(InfName)" TransceiverValue is "$(!p:TransceiverValue)
    ;Debug-Output $(InfName)" MemoryAddr is "$(!p:MemoryAddr)
    ;Debug-Output $(InfName)" MappedValue is "$(!p:MappedValue)

    return


;***************************************************************
;  INSTALL SECTIONS
;***************************************************************
[Install-Option]
    set STF_VITAL = ""

    ifstr(i) $(AddCopy) == "YES"

        AddSectionFilesToCopyList Files-$(Option) $(SrcDir) $(!STF_WINDOWSSYSPATH)\drivers

    endif

    ifstr(i) $(DoCopy) == "YES"

       ;
       ; Copy files in the copy list
       ;
       set !STF_NCPA_FLUSH_COPYLIST = TRUE
       CopyFilesInCopyList

    endif

    Exit

[Install-Update]
   set STF_VITAL        = ""
   set STF_OVERWRITE    = "VERIFYSOURCEOLDER"
   ;set STF_VERSION     = "YES"

   AddSectionFilesToCopyList Files-$(Option) $(SrcDir) $(!STF_WINDOWSSYSPATH)\drivers
   AddSectionFilesToCopyList Files-Inf $(SrcDir) $(!STF_WINDOWSSYSPATH)

   set !STF_NCPA_FLUSH_COPYLIST = TRUE
   CopyFilesInCopyList

   exit


[Install-Dll]
   set STF_VITAL 	= ""
   AddSectionFilesToCopyList Files-Dll $(SrcDir) $(!STF_WINDOWSSYSPATH)
   set !STF_NCPA_FLUSH_COPYLIST = TRUE
   CopyFilesInCopyList
   exit





[Source Media Descriptions]
    1  = "Xircom Setup Disk for NT"


[ProductType]
STF_PRODUCT  = Winnt
STF_PLATFORM = I386


[Files-Inf]
1, OEMSETNT.INF, SIZE=43500,	RENAME=$(!UG_Filename)

[Files-Dll]
1, CTNDNT.DLL,  SIZE=23000

[Files-CTNDNT]
1, CTNDNT.SYS, SIZE=43008


[LanguagesSupported]
    ENG

[AllFileConstantsENG]
ProCaption   = "Windows NT Setup"
ProCancel    = "Cancel"
ProCancelMsg = "Windows NT Networking is not correctly installed.  "+
               "Are you sure you want to cancel copying files?"
ProCancelCap = "Network Setup Message"
ProText1     = "Copying:"
ProText2     = "To:"
DialogDllName     = "CTNDNT.DLL"

   

; START TOKEN RING ---------------------------------------------------------------------------------------
[FileConstantsENG-CTNDNT]
FunctionTitle   = $(GenericAdapterName)" Setup"$(GenericInfVersion)
ProductSoftwareTitle        = $(GenericDriverName)
ProductHardwareTitle        = $(GenericAdapterName)
IRQList           = ^(IRQChoices, 1)
IRQValues         = ^(IRQChoices, 2)
IOBaseAddrList    = ^(IOBaseAddrChoices, 1)
IOBaseAddrValues  = ^(IOBaseAddrChoices, 2)
MemoryAddrList    = ^(MemoryAddrChoices,1)
MemoryAddrValues  = ^(MemoryAddrChoices,2)
LineSpeedList     = ^(LineSpeedChoices,1)
LineSpeedValues   = ^(LineSpeedChoices,2)

[DialogConstantsENG-CTNDNT]
Help        = "&Help"
Exit        = "Cancel"
OK          = "OK"
HelpContext = ""
Continue    = "Continue"
Cancel      = "Cancel"
;CardInfo    = "Card Info"

[FileDependentDlgENG-CTNDNT]
DlgType = "RadioCombination"
DlgTemplate = "CT2"
Caption = $(FunctionTitle)
HelpContext = $(!IDH_DB_OEMNADE2_INS)
CBOptionsGreyed = {}
NotifyFields = {NO, NO, NO, NO}
Combo1Label = "I/&O Port:"
Combo2Label = "&Memory Address:"
Combo3Label = "&Interrupt:"
Combo4Label = "&Link Speed:"
;---------------------------
Combo1List = $(IOBaseAddrList)
Combo1Out  = $(IOBaseAddrValue)
Combo2List = $(MemoryAddrList)
Combo2Out  = $(MemoryAddrValue)
Combo3List = $(IRQList)
Combo3Out  = $(IRQValue)
Combo4List = $(LineSpeedList)
Combo4Out  = $(LineSpeedValue)
;---------------------------
ComboListItemsIn  = {Combo1List,Combo2List,Combo3List,Combo4List}
ComboListItemsOut = {Combo1Out, Combo2Out, Combo3Out, Combo4Out}
EditTextIn = {"","","","",""}
EditTextLim = {"","","","",""}

; END TOKEN RING ---------------------------------------------------------------------------------------


[MemoryAddrChoices]
MA_1  = "0xA0000", 655360
MA_2  = "0xA1000", 659456
MA_3  = "0xA2000", 663552
MA_4  = "0xA3000", 667648
MA_5  = "0xA4000", 671744
MA_6  = "0xA5000", 675840
MA_7  = "0xA6000", 679936
MA_8  = "0xA7000", 684032
MA_9  = "0xA8000", 688128
MA_10 = "0xA9000", 692224
MA_11 = "0xAA000", 696320
MA_12 = "0xAB000", 700416
MA_13 = "0xAC000", 704512
MA_14 = "0xAD000", 708608
MA_15 = "0xAE000", 712704
MA_16 = "0xAF000", 716800
MA_17 = "0xB0000", 720896
MA_18 = "0xB1000", 724992
MA_19 = "0xB2000", 729088
MA_20 = "0xB3000", 733184
MA_21 = "0xB4000", 737280
MA_22 = "0xB5000", 741376
MA_23 = "0xB6000", 745472
MA_24 = "0xB7000", 749568
MA_25 = "0xB8000", 753664
MA_26 = "0xB9000", 757760
MA_27 = "0xBA000", 761856
MA_28 = "0xBB000", 765952
MA_29 = "0xBC000", 770048
MA_30 = "0xBD000", 774144
MA_31 = "0xBE000", 778240
MA_32 = "0xBF000", 782336
MA_33 = "0xC0000", 786432
MA_34 = "0xC1000", 790528
MA_35 = "0xC2000", 794624
MA_36 = "0xC3000", 798720
MA_37 = "0xC4000", 802816
MA_38 = "0xC5000", 806912
MA_39 = "0xC6000", 811008
MA_40 = "0xC7000", 815104
MA_41 = "0xC8000", 819200
MA_42 = "0xC9000", 823296
MA_43 = "0xCA000", 827392
MA_44 = "0xCB000", 831488
MA_45 = "0xCC000", 835584
MA_46 = "0xCD000", 839680
MA_47 = "0xCE000", 843776
MA_48 = "0xCF000", 847872
MA_49 = "0xD0000", 851968
MA_50 = "0xD1000", 856064
MA_51 = "0xD2000", 860160
MA_52 = "0xD3000", 864256
MA_53 = "0xD4000", 868352
MA_54 = "0xD5000", 872448
MA_55 = "0xD6000", 876544
MA_56 = "0xD7000", 880640
MA_57 = "0xD8000", 884736
MA_58 = "0xD9000", 888832
MA_59 = "0xDA000", 892928
MA_60 = "0xDB000", 897024
MA_61 = "0xDC000", 901120
MA_62 = "0xDD000", 905216
MA_63 = "0xDE000", 909312
MA_64 = "0xDF000", 913408
MA_65 = "0xE0000", 917504
MA_66 = "0xE1000", 921600
MA_67 = "0xE2000", 925696
MA_68 = "0xE3000", 929792
MA_69 = "0xE4000", 933888
MA_70 = "0xE5000", 937984
MA_71 = "0xE6000", 942080
MA_72 = "0xE7000", 946176
MA_73 = "0xE8000", 950272
MA_74 = "0xE9000", 954368
MA_75 = "0xEA000", 958464
MA_76 = "0xEB000", 962560
MA_77 = "0xEC000", 966656
MA_78 = "0xED000", 970752
MA_79 = "0xEE000", 974848
MA_80 = "0xEF000", 978944
MA_81 = "0xF0000", 983040
MA_82 = "0xF1000", 987136
MA_83 = "0xF2000", 991232
MA_84 = "0xF3000", 995328
MA_85 = "0xF4000", 999424
MA_86 = "0xF5000", 1003520
MA_87 = "0xF6000", 1007616
MA_88 = "0xF7000", 1011712
MA_89 = "0xF8000", 1015808
MA_90 = "0xF9000", 1019904
MA_91 = "0xFA000", 1024000
MA_92 = "0xFB000", 1028096
MA_93 = "0xFC000", 1032192
MA_94 = "0xFD000", 1036288
MA_95 = "0xFE000", 1040384

[IRQChoices]
;Interrupts available on the PCIC: { 3,4,5,7,8,10,11,12,14,15 }
;Interrupts available on the TCIC: { 3,4,5,6,7,10,14 }
;14 = fixed disk
;12 = keyboard
;6  = floppy disk
;union(PCIC, TCIC) - {14} = 3,4,5,7,10
IRQ_1 = "3",3
IRQ_2 = "4",4
IRQ_3 = "5",5
IRQ_4 = "7",7
IRQ_5 = "10",10
IRQ_6 = "11",11
IRQ_7 = "15",15


[LineSpeedChoices]
LS0_0 = "EEPROM",238
LS1_1 = "4 Mbps",4
LS2_2 = "16 Mbps",16
;LS2_3 = "Auto",10

[IOBaseAddrChoices]
; 0x3E0 is where PCIC is located
; 0x240 is where TCIC is located
; therefore user cannot select these for locating the ethernet adapter
IOBase_1  = "0x200",512
IOBase_2  = "0x210",528
IOBase_3  = "0x220",544
IOBase_4  = "0x230",560
;IOBase_5  = "0x240",576
IOBase_6  = "0x250",592
IOBase_7  = "0x260",608
IOBase_8  = "0x270",624
IOBase_9  = "0x280",640
IOBase_10 = "0x290",656
IOBase_11 = "0x2A0",672
IOBase_12 = "0x2B0",698
IOBase_13 = "0x2C0",714
IOBase_14 = "0x2D0",730
IOBase_15 = "0x2E0",746
IOBase_16 = "0x2F0",752
IOBase_17 = "0x300",768
IOBase_18 = "0x310",784
IOBase_19 = "0x320",800
IOBase_20 = "0x330",816
IOBase_21 = "0x340",832
IOBase_22 = "0x350",848
IOBase_23 = "0x360",864
IOBase_24 = "0x370",880
IOBase_25 = "0x380",896
IOBase_26 = "0x390",912
IOBase_27 = "0x3A0",928
IOBase_28 = "0x3B0",944
IOBase_29 = "0x3C0",960
IOBase_30 = "0x3D0",976


