[Identification]
    OptionType = NetAdapter
[PlatformsSupported]
    ISA
    EISA
    PCI
[Options]
    AMDPCI
[FileConstants]
GenericInfVersion  = " v2.45"
GenericSysName     = "amdpcn.sys"
GenericName        = "AMDPCN"
UtilityInf      = "UTILITY.INF"
ParamInf        = "NCPARAM.INF"
subroutineinf   = "SUBROUTN.INF"
SoftwareType    = "driver"
Exit_Code       = 0
NetEventDLL     = "%SystemRoot%\System32\netevent.dll"
IoLogMsgDLL     = "%SystemRoot%\System32\IoLogMsg.dll"
Manufacturer    = "Microsoft"
ProductMajorVersion     = "4"
ProductMinorVersion     = "0"
ProductVersion  = $(ProductMajorVersion)"."$(ProductMinorVersion)
ProductSoftwareName     = "AMDPCN"
ProductSoftwareImagePath = "\SystemRoot\System32\drivers\"$(GenericSysName)
NetRuleSoftwareType     = "pcntn3Sys ndisDriver pcntn3Driver"
NetRuleSoftwareUse      = $(SoftwareType)
NetRuleSoftwareBindForm = """pcntn3Sys"" yes no container"
NetRuleSoftwareClass    = {"pcntn3Driver basic"}
NetRuleSoftwareBindable = {"pcntn3Driver pcntn3Adapter non exclusive 100"}
ProductHardwareName        = "AMDPCN"
NetRuleHardwareType        = "pcntn3 pcntn3Adapter"
NetRuleHardwareBindForm    = " yes yes container"
NetRuleHardwareClass       = {"pcntn3Adapter basic"}
ProductKeyName  = $(!NTN_SoftwareBase)"\"$(Manufacturer)"\"$(ProductSoftwareName)"\CurrentVersion"
ParamKeyName    = $(!NTN_ServiceBase)"\"$(ProductHardwareName)"\Parameters"
[GeneralConstants]
from      = ""
to        = ""
ExitCodeOk     = 0
ExitCodeCancel = 1
ExitCodeFatal  = 2
KeyNull         = ""
MAXIMUM_ALLOWED   = 33554432
RegistryErrorIndex = NO_ERROR
KeyProduct      = ""
KeyParameters   = ""
TRUE            = 1
FALSE           = 0
NoTitle         = 0
ExitState   = "Active"
OldVersionExisted = $(FALSE)
DriverPath      = $(!STF_NTPATH)\drivers
[date]
    Now = {} ? $(!LIBHANDLE) GetSystemDate
[Identify]
    read-syms Identification
    set Status     = STATUS_SUCCESSFUL
    set Identifier = $(OptionType)
    set Media      = #("Source Media Descriptions", 1, 1)
    Return $(Status) $(Identifier) $(Media)
[ReturnOptions]
    set Status        = STATUS_FAILED
    set OptionList     = {}
    set OptionTextList = {}
    set LanguageList = ^(LanguagesSupported, 1)
    Ifcontains(i) $($0) in $(LanguageList)
	ifstr(i) $($1) == ""
			goto returnoptions
	endif
	set PlatformList = ^(PlatformsSupported, 1)
	Ifcontains(i) $($1) in $(PlatformList)
			goto returnoptions
	else
			set Status = STATUS_NOTSUPPORTED
			goto finish_ReturnOptions
	endif
    else
		set Status = STATUS_NOLANGUAGE
		goto finish_ReturnOptions
    endif
returnoptions = +
    set OptionList     = ^(Options, 1)
    set OptionTextList = ^(OptionsText$($0), 1)
    set Status         = STATUS_SUCCESSFUL
finish_ReturnOptions = +
    Return $(Status) $(OptionList) $(OptionTextList)
[InstallOption]
    set Status   = STATUS_FAILED
    set Option   = $($1)
    set SrcDir   = $($2)
    set AddCopy  = $($3)
    set DoCopy   = $($4)
    set DoConfig = $($5)
    set LanguageList = ^(LanguagesSupported, 1)
    Ifcontains(i) $($0) NOT-IN $(LanguageList)
	Return STATUS_NOLANGUAGE
    endif
    set-subst LF = "\n"
    read-syms GeneralConstants
    read-syms FileConstants
    read-syms FileConstants$(!STF_LANGUAGE)
    read-syms DialogConstants$(!STF_LANGUAGE)
    ifstr(i) $(!NTN_Origination) == "NCPA"
	set Continue = $(OK)
    endif
    detect date
    set-title  $(FunctionTitle)
    set to   = Begin
    set from = Begin
    set CommonStatus = STATUS_SUCCESSFUL
    EndWait
Begin = +
    Set ActivateDetection = FALSE
    Ifstr(i) $(!NTN_InstallMode) == deinstall
	set StartLabel = removeadapter
    else-Ifstr(i) $(!NTN_InstallMode) == Update
	set StartLabel = UpgradeSoftware
    else-Ifstr(i) $(!NTN_InstallMode) == bind
	set StartLabel = bindingadapter
    else-Ifstr(i) $(!NTN_InstallMode) == configure
	set StartLabel = configureadapter
	Ifstr(i) $(ProductKeyName) == $(!NTN_RegBase)
	    Debug-Output "Cannot configure the PCNet family driver software."
	    Shell $(UtilityInf),RegistryErrorString,CANNOT_CONFIGURE_SOFTWARE
	    ifint $($ShellCode) != $(!SHELL_CODE_OK)
		Debug-Output "ShellCode error: cannot get an error string."
		goto ShellCodeError
	    endif
	    set Error = $($R0)
	    set from = end
	    set to = end
	    goto nonfatalinfo
	endif
    else
	set StartLabel = installadapter
	set OEM_ABANDON_OPTIONS = {}
	set OEM_ABANDON_SOFTWARE = FALSE
	set OEM_ABANDON_ON = TRUE
    endif
    set IRQValue = *($(IRQList), 9)
    set IOBaseAddrValue = *($(IOBaseAddrList), 17)
    set DMAChannelValue = *($(DMAChannelList), 5)
    set RadioIn  = {4}
    set BusScanValue = "ALL"
    set LED0Value = *($(LEDList), 1)
    set LED1Value = *($(LEDList), 1)
    set LED2Value = *($(LEDList), 1)
    set LED3Value = *($(LEDList), 1)
    set TPValue = 1
    set FullDuplexValue = *($(FullDuplexList), 4)
    set BusTimerValue = *($(BusTimerList), 10)
    Set from = $(fatal)
    Set to = $(fatal)
    Goto $(StartLabel)
installadapter = +
	set IsISA = 0
	set Vendor = 4130
	set CardID = 8192
	Shell $(UtilityInf), GetPCIInformation, $(Vendor) $(CardID)
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    goto ShellCodeError
	endif
	set AdapterList = $($R0)
        set NewAdapterList = {}
	set NumNew = 0
	ForListDo $(AdapterList)
	    set BusNum = *($($),1)
	    set SlotNum = *($($),2)
	    Shell $(UtilityInf), IsNetCardAlreadyInstalled, $(BusNum), +
		$(SlotNum), $(GenericPCIAdapterName), $(ProductHardwareName)
	    ifstr(i) $($R1) != "YES"
		    set-add NumNew = $(NumNew),1
		    ifstr(i) $(NewAdapterList) == {}
	            set NewAdapterList = {$($)}
            else
		        set NewAdapterList = >($(NewAdapterList),$($))
            endif
	    endif
	EndForListDo
	set AdapterList = $(NewAdapterList)
	ifint $(NumNew) == 0
	    set AdapterList = {{0,0,0}}
	    set IsISA = 1
	endif
	debug-output $(AdapterList)
    OpenRegKey $(!REG_H_LOCAL) "" $(ProductKeyName) $(MAXIMUM_ALLOWED) KeyProduct
    Ifstr $(KeyProduct) != $(KeyNull)
	CloseRegKey $(KeyProduct)
	ifstr(i) !(NTN_RegBase) == $(ProductKeyName)
	   Shell $(UtilityInf), VerExistedDlg, $(ProductSoftwareTitle),+
	       $(ProductVersion)
	   ifint $($ShellCode) != $(!SHELL_CODE_OK)
	       Debug-Output "ShellCode error: cannot get an error string."
	       goto ShellCodeError
	   endif
	   goto end
	else
	   Shell $(UtilityInf), CardExistedDlg
	   ifint $($ShellCode) != $(!SHELL_CODE_OK)
	       Debug-Output "ShellCode error: cannot get an error string."
	       goto ShellCodeError
	   endif
	   ifstr(i) $($R1) != "OK"
	       goto end
	   endif
	   set OldVersionExisted = $(TRUE)
	endif
    endif
    ifint $(OldVersionExisted) == $(FALSE)
	ifstr(i) $(!NTN_InstallMode) == "install"
	   Ifstr(i) $(DoCopy) == "YES"
		Shell $(UtilityInf), DoAskSource, $(!STF_CWDDIR), $(SrcDir) NO
		Ifint $($ShellCode) != $(!SHELL_CODE_OK)
		    Goto ShellCodeError
		Else-Ifstr(i) $($R0) == STATUS_FAILED
		    Shell $(UtilityInf) RegistryErrorString "ASK_SOURCE_FAIL"
		    ifint $($ShellCode) != $(!SHELL_CODE_OK)
			goto ShellCodeError
		    endif
		    set Error = $($R0)
		    Goto fatal
		Else-Ifstr(i) $($R0) == STATUS_USERCANCEL
		    Goto successful
		Endif
		Set SrcDir = $($R1)
	    endif
	    install "Install-Helpfile"
	endif
    endif
    SetHelpFile "pcnet.hlp" 1 11
    Shell $(UtilityInf), DoAskSource, $(!STF_CWDDIR), $(SrcDir) YES
    Ifint $($ShellCode) != $(!SHELL_CODE_OK)
	Goto ShellCodeError
    Else-Ifstr(i) $($R0) == STATUS_FAILED
	Shell $(UtilityInf) RegistryErrorString "ASK_SOURCE_FAIL"
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    goto ShellCodeError
	endif
	set Error = $($R0)
	Goto fatal
    Else-Ifstr(i) $($R0) == STATUS_USERCANCEL
	Goto successful
    Endif
    Set SrcDir = $($R1)
    install "Install-Dll"
    goto adaptersetup
configureadapter = +
    SetHelpFile "pcnet.hlp" 1 11
    Ifstr $(KeyProduct) == $(KeyNull)
	OpenRegKey $(!REG_H_LOCAL) "" $(!NTN_RegBase) $(MAXIMUM_ALLOWED) KeyProduct
	Ifstr $(KeyProduct) == $(KeyNull)
	    set RegistryErrorIndex = CANNOT_FIND_COMPONENT_SERVICE
	    Debug-Output "Cannot find component product key"
	    goto fatalregistry
	Endif
    Endif
    Debug-Output "INF: Shelling to FindService"
    Shell $(UtilityInf) FindService, $(KeyProduct)
    Ifint $($ShellCode) != $(!SHELL_CODE_OK)
	Debug-Output "INF: FindService shell failure"
	Goto ShellCodeError
    Endif
    Ifstr(i) $($R0) != NO_ERROR
	Debug-Output "INF: FindService Shell error: "$($R0)
	Goto fatalregistry
    endif
    Set KeyParameters = $($R2)
    CloseRegKey $($R1)
    Ifstr $(KeyParameters) == $(KeyNull)
	set RegistryErrorIndex = CANNOT_FIND_COMPONENT_SERVICE
	Debug-Output "Cannot find component service"
	goto fatalregistry
    endif
    set OldVersionExisted = $(TRUE)
    set ValueName = ""
    set ValueData = ""
    set ValueStr  = ""
    set ValueList = {}
    EnumRegValue $(KeyParameters) ValueList
    ForListDo $(ValueList)
	set ValueItem = $($)
	set ValueName = *($(ValueItem),1)
	set ValueData = *($(ValueItem),4)
	ifstr(i) $(ValueName) == "BUS_TO_SCAN"
	    set BusScanValue = $(ValueData)
	else-ifstr(i) $(ValueName) == "TP"
	    set TPValue = $(ValueData)
	else-ifstr(i) $(ValueName) == "LED0"
	    set LED0Value = $(ValueData)
	else-ifstr(i) $(ValueName) == "LED1"
	    set LED1Value = $(ValueData)
	else-ifstr(i) $(ValueName) == "LED2"
	    set LED2Value = $(ValueData)
	else-ifstr(i) $(ValueName) == "LED3"
	    set LED3Value = $(ValueData)
	else-ifstr(i) $(ValueName) == "IOBaseAddress"
	    set IOBaseAddrValue = $(ValueData)
	else-ifstr(i) $(ValueName) == "InterruptNumber"
	    set IRQValue = $(ValueData)
	else-ifstr(i) $(ValueName) == "DMAChannel"
	    set DMAChannelValue = $(ValueData)
	else-ifstr(i) $(ValueName) == "FDUP"
	    set FullDuplexValue = $(ValueData)
	else-ifstr(i) $(ValueName) == "BUSTIMER"
	    set BusTimerValue = $(ValueData)
	else-ifstr(i) $(ValueName) == "BusType"
	    set BusInterfaceType = $(ValueData)
        ifint $(BusInterfaceType) == 5
            set IsISA = 0
        else
            set IsISA = 1
        endif
	else-ifstr(i) $(ValueName) == "BusNum"
	    set BusNumber = $(ValueData)
	endif
    EndForListDo
    Ifint $(TPValue) == 0
	Set CheckItemsIn = {"OFF"}
    Else
	Set CheckItemsIn = {"ON"}
    Endif
    Ifstr $(BusScanValue) == "PNP"
	Set RadioIn = {1}
    Else-Ifstr $(BusScanValue) == "VESA"
	Set RadioIn = {2}
    Else-Ifstr $(BusScanValue) == "ISA"
	Set RadioIn = {3}
    Else-Ifstr $(BusScanValue) == "ALL"
	Set RadioIn = {4}
    Else-Ifstr $(BusScanValue) == ""
	Set RadioIn = {4}
    Endif
    Debug-Output $(InfName)" TP is "$(TPValue)
ifint $(IsISA) == 1
    set IRQValue = *($(IRQList), ~($(IRQValues),$(IRQValue)))
    ifstr(i) $(IRQValue) == ""
	set IRQValue = *($(IRQList), 2)
    endif
    Debug-Output $(InfName)" IRQ_Level is "$(IRQValue)
    set DMAChannelValue = *($(DMAChannelList), ~($(DMAChannelValues),$(DMAChannelValue)))
    ifstr(i) $(DMAChannelValue) == ""
	set DMAChannelValue = *($(DMAChannelList), 2)
    endif
    Debug-Output $(InfName)" DMA is "$(DMAChannelValue)
    set IOBaseAddrValue = *($(IOBaseAddrList), ~($(IOBaseAddrValues),$(IOBaseAddrValue)))
    ifstr(i) $(IOBaseAddrValue) == ""
	set IOBaseAddrValue = *($(IOBaseAddrList), 1)
    endif
    Debug-Output $(InfName)" I/o base is "$(IOBaseAddrValue)
endif
    set LED0Value = *($(LEDList), ~($(LEDValues),$(LED0Value)))
    ifstr(i) $(LED0Value) == ""
	set LED0Value = *($(LEDList), 1)
    endif
    Debug-Output $(InfName)" LED0 is "$(LED0Value)
    set LED1Value = *($(LEDList), ~($(LEDValues),$(LED1Value)))
    ifstr(i) $(LED1Value) == ""
	set LED1Value = *($(LEDList), 1)
    endif
    Debug-Output $(InfName)" LED1 is "$(LED1Value)
    set LED2Value = *($(LEDList), ~($(LEDValues),$(LED2Value)))
    ifstr(i) $(LED2Value) == ""
	set LED2Value = *($(LEDList), 1)
    endif
    Debug-Output $(InfName)" LED2 is "$(LED0Value)
    set LED3Value = *($(LEDList), ~($(LEDValues),$(LED3Value)))
    ifstr(i) $(LED3Value) == ""
	set LED3Value = *($(LEDList), 1)
    endif
    Debug-Output $(InfName)" LED3 is "$(LED3Value)
    set FullDuplexValue = *($(FullDuplexList), ~($(FullDuplexValues),$(FullDuplexValue)))
    ifstr(i) $(FullDuplexValue) == ""
	set FullDuplexValue = *($(FullDuplexList), 1)
    endif
    Debug-Output $(InfName)" Full Duplex is "$(FullDuplexValue)
    set BusTimerValue = *($(BusTimerList), ~($(BusTimerValues),$(BusTimerValue)))
    ifstr(i) $(BusTimerValue) == ""
	set BusTimerValue = *($(BusTimerList), 1)
    endif
    Debug-Output $(InfName)" Bus Timer is "$(BusTimerValue)
adaptersetup = +
    Set from = adapteroptions
adapteroptions = +
    LoadLibrary "x" $(!STF_CWDDIR)\$(DialogDllName) hLib
ifint $(IsISA) == 0
    read-syms FileDependentDlgPCI$(!STF_LANGUAGE)
    Debug-Output $(InfName)" TP is "$(TPValue)
    Debug-Output $(InfName)" LED0 is "$(LED0Value)
    Debug-Output $(InfName)" LED1 is "$(LED1Value)
    Debug-Output $(InfName)" LED2 is "$(LED2Value)
    Debug-Output $(InfName)" LED3 is "$(LED3Value)
    Debug-Output $(InfName)" Full Duplex is "$(FullDuplexValue)
    Debug-Output $(InfName)" Bus Timer is "$(BusTimerValue)
    ui start "Inputdlg" $(hLib)
else
debug-output "read the isa dialog"
    read-syms FileDependentDlg$(!STF_LANGUAGE)
    Debug-Output $(InfName)" Bus is "$(BusScanValue)
    Debug-Output $(InfName)" TP is "$(TPValue)
    Debug-Output $(InfName)" LED0 is "$(LED0Value)
    Debug-Output $(InfName)" LED1 is "$(LED1Value)
    Debug-Output $(InfName)" LED2 is "$(LED2Value)
    Debug-Output $(InfName)" LED3 is "$(LED3Value)
    Debug-Output $(InfName)" DMA is "$(DMAChannelValue)
    Debug-Output $(InfName)" I/o base is "$(IOBaseAddrValue)
    Debug-Output $(InfName)" Full Duplex is "$(FullDuplexValue)
    Debug-Output $(InfName)" Bus Timer is "$(BusTimerValue)
    ui start "InputDlg"  $(hLib)
endif
    set ExitButton      = $(ButtonPressed)
    Debug-Output " ButtonPressed "$(ButtonPressed)
debug-output $(DLGEVENT)
    FreeLibrary $(hLib)
    ifstr(i) $(DLGEVENT) == "CONTINUE"
ifint $(IsISA) == 1
		set IOBaseAddrValue = $(Combo1Out)
		set IRQValueValue = $(Combo2Out)
		set DMAChannelValue = $(Combo3Out)
		set FullDuplexValue = $(Combo4Out)
		set BusTimerValue = $(Combo5Out)
		set ExitButton = $(ButtonPressed)
		set BusIndex = *($(RadioOut),1)
else
		set FullDuplexValue = $(Combo1Out)
		set BusTimerValue = $(Combo2Out)
		set ExitButton = $(ButtonPressed)
		set BusIndex = *($(RadioOut),1)
endif
		Ifint $(BusIndex) == 1
		    Set BusScanValue = "PNP"
		else-Ifint $(BusIndex) == 2
		    Set BusScanValue = "VESA"
		else-Ifint $(BusIndex) == 3
		    Set BusScanValue = "ISA"
		else-Ifint $(BusIndex) ==  4
		    Set BusScanValue = "ALL"
		Endif
	Set Chk = *($(CheckItemsOut), 1)
	Ifstr(i) $(Chk) == "ON"
	    Set TPValue = 1
	Else
	    Set TPValue = 0
	Endif
		ui pop 1
    else-ifstr(i) $(DLGEVENT) == "EXIT"
		set CommonStatus = STATUS_USERCANCEL
		Debug-Output "Action: exit. Bye."
		ui pop 1
		goto end
    else
		ui pop 1
		Debug-Output "Action: unknown. Bye."
		goto end
    endif
    Debug-Output " Combo list out "$(ComboListItemsOut)
skipoptions =+
    ifint $(OldVersionExisted) == $(TRUE)
	ifstr(i) $(!NTN_InstallMode) == configure
    Shell $(UtilityInf), GetBusTypeNum
    set BusTypeNum = $($R1)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	Debug-Output "ShellCode error."
	goto ShellCodeError
    endif
debug-output "before write registry"
    set DMAChannelValue = *($(DMAChannelValues), ~($(DMAChannelList),$(DMAChannelValue)))
    set IRQValue = *($(IRQValues), ~($(IRQList),$(IRQValueValue)))
    set IOBaseAddrValue = *($(IOBaseAddrValues), ~($(IOBaseAddrList),$(IOBaseAddrValue)))
    set LED0Value = *($(LEDValues), ~($(LEDList),$(LED0Value)))
    set LED1Value = *($(LEDValues), ~($(LEDList),$(LED1Value)))
    set LED2Value = *($(LEDValues), ~($(LEDList),$(LED2Value)))
    set LED3Value = *($(LEDValues), ~($(LEDList),$(LED3Value)))
    set FullDuplexValue = *($(FullDuplexValues), ~($(FullDuplexList),$(FullDuplexValue)))
    set BusTimerValue = *($(BusTimerValues), ~($(BusTimerList),$(BusTimerValue)))
    ifint $(IsISA) == 0
    set NewValueList = {{FDUP,  $(NoTitle),$(!REG_VT_DWORD),$(FullDuplexValue)},+
			{BUSTIMER,  $(NoTitle),$(!REG_VT_DWORD),$(BusTimerValue)},+
			{TP,    $(NoTitle),$(!REG_VT_DWORD),$(TPValue)}}
    Shell  $(UtilityInf), AddValueList, $(KeyParameters), $(NewValueList)
    else
    set NewValueList = {{BUS_TO_SCAN,$(NoTitle),$(!REG_VT_SZ),$(BusScanValue)},+
			{FDUP,  $(NoTitle),$(!REG_VT_DWORD),$(FullDuplexValue)},+
			{BUSTIMER,  $(NoTitle),$(!REG_VT_DWORD),$(BusTimerValue)},+
			{TP,    $(NoTitle),$(!REG_VT_DWORD),$(TPValue)},+
			{IOBaseAddress,  $(NoTitle),$(!REG_VT_DWORD),$(IOBaseAddrValue)},+
			{InterruptNumber,  $(NoTitle),$(!REG_VT_DWORD),$(IRQValue)},+
			{DMAChannel, $(NoTitle),$(!REG_VT_DWORD),$(DMAChannelValue)}}
    Shell  $(UtilityInf), AddValueList, $(KeyParameters), $(NewValueList)
    endif
    CloseRegKey $(KeyParameters)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	Debug-Output "ShellCode error."
	goto ShellCodeError
    endif
    set RegistryErrorIndex = $($R0)
    Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	Debug-Output "Registry error: Add value list"
	goto fatalregistry
    endif
    EndWait
    goto successful
	endif
    endif
    StartWait
    ifint $(OldVersionExisted) == $(FALSE)
	ifstr(i) $(!NTN_InstallMode) == "install"
	   Ifstr(i) $(DoCopy) == "YES"
	      Shell $(UtilityInf), DoAskSource, $(!STF_CWDDIR), $(SrcDir) YES
	      Ifint $($ShellCode) != $(!SHELL_CODE_OK)
		  Goto ShellCodeError
	      Else-Ifstr(i) $($R0) == STATUS_FAILED
		  Shell $(UtilityInf) RegistryErrorString "ASK_SOURCE_FAIL"
		  ifint $($ShellCode) != $(!SHELL_CODE_OK)
		      goto ShellCodeError
		  endif
		  set Error = $($R0)
		  Goto fatal
	      Else-Ifstr(i) $($R0) == STATUS_USERCANCEL
		  Goto successful
	      Endif
	      Set SrcDir = $($R1)
	   Endif
	   install "Install-Option"
	   ifstr(i) $(STF_INSTALL_OUTCOME) != STF_SUCCESS
	      Shell $(UtilityInf) RegistryErrorString "UNABLE_COPY_FILE"
	      ifint $($ShellCode) != $(!SHELL_CODE_OK)
		  goto ShellCodeError
	      endif
	      set Error = $($R0)
	      goto fatal
	   endif
	endif
	Shell $(UtilityInf), AddSoftwareComponent, $(Manufacturer), +
	    $(ProductSoftwareName), +
	    $(ProductSoftwareName), +
	    $(ProductSoftwareTitle), $(STF_CONTEXTINFNAME), +
	    $(ProductSoftwareImagePath), "kernel", "NDIS", {}, "",+
	    $(NetEventDLL)
	Set OEM_ABANDON_SOFTWARE = TRUE
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    Debug-Output "ShellCode error"
	    goto ShellCodeError
	endif
	set RegistryErrorIndex = $($R0)
	set KeyProduct      = $($R1)
	Set SoftNetRulesKey = $($R2)
	CloseRegKey $($R3)
	CloseRegKey $($R4)
	CloseRegKey $($R5)
	Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	    EndWait
	    Debug-Output "Registry error: add software components"
	    CloseRegKey $(KeyProduct)
	    CloseRegKey $(SoftNetRulesKey)
	    goto fatalregistry
	endif
	set NewValueList = {{SoftwareType,$(NoTitle),$(!REG_VT_SZ),$(SoftwareType)},+
			   {MajorVersion,$(NoTitle),$(!REG_VT_DWORD),$(ProductMajorVersion)},+
			   {MinorVersion,$(NoTitle),$(!REG_VT_DWORD),$(ProductMinorVersion)},+
			   {Title,$(NoTitle),$(!REG_VT_SZ),$(ProductSoftwareTitle)},+
			   {Description,$(NoTitle),$(!REG_VT_SZ),$(ProductSoftwareDescription)},+
			   {ServiceName,$(NoTitle),$(!REG_VT_SZ),$(ProductSoftwareName)},+
			   {InstallDate,$(NoTitle),$(!REG_VT_DWORD),*($(Now),1)}}
	Shell  $(UtilityInf), AddValueList, $(KeyProduct), $(NewValueList)
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    Debug-Output "ShellCode error."
	    goto ShellCodeError
	endif
	set RegistryErrorIndex = $($R0)
	Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	    EndWait
	    Debug-Output "Registry error: add value list."
	    CloseRegKey $(KeyProduct)
	    CloseRegKey $(SoftNetRulesKey)
	    goto fatalregistry
	endif
	set NewValueList = {{type,$(NoTitle),$(!REG_VT_SZ),$(NetRuleSoftwareType)},+
			    {use,$(NoTitle),$(!REG_VT_SZ),$(NetRuleSoftwareUse)}, +
			    {bindform,$(NoTitle),$(!REG_VT_SZ),$(NetRuleSoftwareBindForm)}, +
			    {class,$(NoTitle),$(!REG_VT_MULTI_SZ),$(NetRuleSoftwareClass)}, +
			    {bindable,$(NoTitle),$(!REG_VT_MULTI_SZ),$(NetRuleSoftwareBindable)}, +
			    {InfOption,$(NoTitle),$(!REG_VT_SZ),$(Option)}}
	Shell  $(UtilityInf), AddValueList, $(SoftNetRulesKey), $(NewValueList)
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    Debug-Output "ShellCode error."
	    goto ShellCodeError
	endif
	set RegistryErrorIndex = $($R0)
	CloseRegKey $(KeyProduct)
	CloseRegKey $(SoftNetRulesKey)
	Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	    EndWait
	    Debug-Output "Resgitry error: add value list."
	    goto fatalregistry
	endif
    endif
    debug-output $(AdapterList)
    ForListDo $(AdapterList)
	    set BusNumber = *($($),1)
	    set DeviceNum = *($($),2)
	    set FunctionNum = *($($),3)
        Shell $(UtilityInf), AddHardwareComponent, $(ProductHardwareName),$(STF_CONTEXTINFNAME),$(ProductKeyName)
        ifint $($R4) != -1
	        Set OEM_ABANDON_OPTIONS = >($(OEM_ABANDON_OPTIONS), $(!NTN_SoftwareBase)"\Microsoft\Windows NT\CurrentVersion\NetworkCards\"$($R4))
        endif
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
	        Debug-Output "Cannot add hardware component"
	        goto ShellCodeError
        endif
        set RegistryErrorIndex = $($R0)
        Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	        EndWait
	        Debug-Output "Registry error: add hardware component"
	        CloseRegKey $($R1)
	        CloseRegKey $($R2)
	        CloseRegKey $($R3)
	        goto fatalregistry
        endif
        set KeyParameters = $($R3)
        set KeyAdapterRules = $($R2)
        set AdapterNumber = $($R4)
        ifint $(IsISA) == 1
            set HardwareDescription = $(GenericAdapterName)
            set HardwareTitle = $(GenericAdapterName)
        else
            set HardwareDescription = $(GenericPCIAdapterName)
            set HardwareTitle = $(GenericPCIAdapterName)
        endif
        set NewValueList = {{Manufacturer,$(NoTitle),$(!REG_VT_SZ),$(Manufacturer)},+
		           {Title,$(NoTitle),$(!REG_VT_SZ),"["$($R4)"] "$(HardwareTitle)},+
		           {Description,$(NoTitle),$(!REG_VT_SZ),$(HardwareDescription)},+
		           {ProductName,$(NoTitle),$(!REG_VT_SZ),$(ProductHardwareName)},+
		           {ServiceName,$(NoTitle),$(!REG_VT_SZ),$($R5)},+
		           {InstallDate,$(NoTitle),$(!REG_VT_DWORD),*($(Now),1)}}
        Shell  $(UtilityInf), AddValueList, $($R1), $(NewValueList)
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
	        Debug-Output "ShellCode error"
	        goto ShellCodeError
        endif
        CloseRegKey $($R1)
        set TempProdName = """"$(ProductHardwareName)$(AdapterNumber)""""
        set TempBindForm = $(TempProdName)$(NetRuleHardwareBindForm)
        set NewValueList = {{type,$(NoTitle),$(!REG_VT_SZ),$(NetRuleHardwareType)},+
			    {bindform,$(NoTitle),$(!REG_VT_SZ),$(TempBindForm)}, +
			    {class,$(NoTitle),$(!REG_VT_MULTI_SZ),$(NetRuleHardwareClass)}, +
			    {InfOption,$(NoTitle),$(!REG_VT_SZ),$(Option)}}
        Shell  $(UtilityInf), AddValueList, $(KeyAdapterRules), $(NewValueList)
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
	        Debug-Output "ShellCode error."
	        goto ShellCodeError
        endif
        set RegistryErrorIndex = $($R0)
        Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	        EndWait
	        Debug-Output "Resgitry error: add value list."
	        CloseRegKey $(KeyParameters)
	        CloseRegKey $(KeyAdapterRules)
	        goto fatalregistry
        endif
        CloseRegKey $(KeyAdapterRules)
        goto writeparameters
writeparameters = +
        Shell $(UtilityInf), GetBusTypeNum
        set BusTypeNum = $($R1)
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
	        Debug-Output "ShellCode error."
	        goto ShellCodeError
        endif
        debug-output "before write registry"
        set DMAChannelValue = *($(DMAChannelValues), ~($(DMAChannelList),$(DMAChannelValue)))
        set IRQValue = *($(IRQValues), ~($(IRQList),$(IRQValueValue)))
        set IOBaseAddrValue = *($(IOBaseAddrValues), ~($(IOBaseAddrList),$(IOBaseAddrValue)))
        set LED0Value = *($(LEDValues), ~($(LEDList),$(LED0Value)))
        set LED1Value = *($(LEDValues), ~($(LEDList),$(LED1Value)))
        set LED2Value = *($(LEDValues), ~($(LEDList),$(LED2Value)))
        set LED3Value = *($(LEDValues), ~($(LEDList),$(LED3Value)))
        set FullDuplexValue = *($(FullDuplexValues), ~($(FullDuplexList),$(FullDuplexValue)))
        set BusTimerValue = *($(BusTimerValues), ~($(BusTimerList),$(BusTimerValue)))
        ifint $(IsISA) == 0
            set NewValueList = {{BusType,$(NoTitle),$(!REG_VT_DWORD),5},+
			    {MediaType,$(NoTitle),$(!REG_VT_DWORD),1},+
			    {LED0,  $(NoTitle),$(!REG_VT_DWORD),$(LED0Value)},+
			    {LED1,  $(NoTitle),$(!REG_VT_DWORD),$(LED1Value)},+
			    {LED2,  $(NoTitle),$(!REG_VT_DWORD),$(LED2Value)},+
			    {LED3,  $(NoTitle),$(!REG_VT_DWORD),$(LED3Value)},+
			    {FDUP,  $(NoTitle),$(!REG_VT_DWORD),$(FullDuplexValue)},+
			    {BUSTIMER,  $(NoTitle),$(!REG_VT_DWORD),$(BusTimerValue)},+
			    {TP,    $(NoTitle),$(!REG_VT_DWORD),$(TPValue)},+
                            {AdapterCFID,$(NoTitle),$(!REG_VT_DWORD),536875042},+
			    {SlotNumber, $(NoTitle),$(!REG_VT_DWORD),$(DeviceNum)},+
			    {BusNumber,  $(NoTitle),$(!REG_VT_DWORD),$(BusNumber)}}
            Shell  $(UtilityInf), AddValueList, $(KeyParameters), $(NewValueList)
        else
            set NewValueList = {{BUS_TO_SCAN,$(NoTitle),$(!REG_VT_SZ),$(BusScanValue)},+
			    {BusType,$(NoTitle),$(!REG_VT_DWORD),1},+
			    {MediaType,$(NoTitle),$(!REG_VT_DWORD),1},+
			    {LED0,  $(NoTitle),$(!REG_VT_DWORD),$(LED0Value)},+
			    {LED1,  $(NoTitle),$(!REG_VT_DWORD),$(LED1Value)},+
			    {LED2,  $(NoTitle),$(!REG_VT_DWORD),$(LED2Value)},+
			    {LED3,  $(NoTitle),$(!REG_VT_DWORD),$(LED3Value)},+
			    {FDUP,  $(NoTitle),$(!REG_VT_DWORD),$(FullDuplexValue)},+
			    {BUSTIMER,  $(NoTitle),$(!REG_VT_DWORD),$(BusTimerValue)},+
			    {TP,    $(NoTitle),$(!REG_VT_DWORD),$(TPValue)},+
			    {IOBaseAddress,  $(NoTitle),$(!REG_VT_DWORD),$(IOBaseAddrValue)},+
			    {InterruptNumber,  $(NoTitle),$(!REG_VT_DWORD),$(IRQValue)},+
			    {DMAChannel, $(NoTitle),$(!REG_VT_DWORD),$(DMAChannelValue)},+
			    {BusNumber,  $(NoTitle),$(!REG_VT_DWORD),$(BusNumber)}}
            Shell  $(UtilityInf), AddValueList, $(KeyParameters), $(NewValueList)
        endif
        CloseRegKey $(KeyParameters)
        ifint $($ShellCode) != $(!SHELL_CODE_OK)
	        Debug-Output "ShellCode error."
	        goto ShellCodeError
        endif
        set RegistryErrorIndex = $($R0)
        Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	        Debug-Output "Registry error: Add value list"
	        goto fatalregistry
    endif
    EndForListDo
    EndWait
    goto successful
bindingadapter =+
    set Error = "Binding: Sorry, not yet implemented."
    goto fatal
removeadapter = +
    Ifstr(i) $(ProductKeyName) == $(!NTN_RegBase)
	Shell $(UtilityInf), RemoveSoftwareComponent, $(Manufacturer), +
	    $(ProductSoftwareName)
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    Debug-Output "ShellCode error"
	    goto ShellCodeError
	endif
	set RegistryErrorIndex = $($R0)
	Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	    goto fatalregistry
	endif
    else
	Shell $(UtilityInf), RemoveHardwareComponent, $(Manufacturer), +
	    $(ProductSoftwareName), $(!NTN_RegBase)
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    Debug-Output "ShellCode error"
	    goto ShellCodeError
	endif
	set RegistryErrorIndex = $($R0)
	Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	    goto fatalregistry
	endif
    endif
    goto end
UpgradeSoftware = +
    LoadLibrary "x" $(!STF_CWDDIR)\ncpa.cpl NCPA_HANDLE
    OpenRegKey $(!REG_H_LOCAL) "" "Software\Microsoft\PCNTN3" $(MAXIMUM_ALLOWED) KeyProduct
    Ifstr $(KeyProduct) != $(KeyNull)
        DeleteRegTree $(KeyProduct) ""
        LibraryProcedure NCPA_RESULT $(NCPA_HANDLE), CPlSetup $(!STF_HWND), DELETESVC, "PCNTN3"
        set NetworkCardKeyName = $(!NTN_SoftwareBase)"\Microsoft\Windows NT\CurrentVersion\NetworkCards"
            OpenRegKey $(!REG_H_LOCAL) "" $(NetworkCardKeyName) $(MAXIMUM_ALLOWED) IE_KeyNetcards
        ifstr(i) $(IE_KeyNetcards) != ""    
            EnumRegKey $(IE_KeyNetcards) IE_KeyNameList
            ForListDo $(IE_KeyNameList)
                OpenRegKey $(IE_KeyNetcards) "" *($($),1) +
                    $(MAXIMUM_ALLOWED) NetworkCardKey
                Ifstr(i) $(NetworkCardKey) != $(KeyNull)
                    GetRegValue $(NetworkCardKey),"ProductName", ProductNameInfo
                    set ProductName = *($(ProductNameInfo), 4)
                    Debug-Output "   ProductName = "$(ProductName)
                    ifstr(i) $(ProductName) != "PCNTN3"
                        goto nextnetcard
                    endif
                    GetRegValue $(NetworkCardKey),"ServiceName", ServiceNameInfo
                    set ServiceName = *($(ServiceNameInfo), 4)
                    Debug-Output "   ServiceName = "$(ServiceName)
                    OpenRegKey $(!REG_H_LOCAL) "" "System\CurrentControlSet\Services\"$(ServiceName) +
                          $(MAXIMUM_ALLOWED) ServiceKey
                DeleteRegTree $(ServiceKey) ""
                DeleteRegTree $(NetworkCardKey) ""
                endif
    nextnetcard = +
            EndForListDo
        endif	
        OpenRegKey $(!REG_H_LOCAL) "" "Software\Microsoft\AMDPCI" $(MAXIMUM_ALLOWED) KeyProduct2
        ifstr $(KeyProduct2) == $(KeyNull)
            LibraryProcedure NCPA_RESULT $(NCPA_HANDLE), CPlSetup $(!STF_HWND), STARTSVC, NetDetect
            set !NTN_InstallMode = Install
            Shell "" InstallOption $(!STF_LANGUAGE) "AMDPCI" $(SrcDir) "YES" "YES" "NO"
            set !NTN_InstallMode = Update
        else
        endif
    else
    endif
    FreeLibrary $(NCPA_HANDLE)
    goto end
successful = +
    goto end
abandon = +
    ForListDo $(OEM_ABANDON_OPTIONS)
	Shell $(UtilityInf), RemoveHardwareComponent, $(Manufacturer), +
	    $(ProductSoftwareName), $($)
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    Debug-Output "ShellCode error"
	    goto ShellCodeError
	endif
	set RegistryErrorIndex = $($R0)
	Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	    goto fatalregistry
	endif
    EndForListDo
    Ifstr(i) $(OEM_ABANDON_SOFTWARE) == TRUE
	Shell $(UtilityInf), RemoveSoftwareComponent, $(Manufacturer), +
	    $(ProductSoftwareName), FALSE
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    Debug-Output "ShellCode error"
	    goto ShellCodeError
	endif
	set RegistryErrorIndex = $($R0)
	Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	    goto fatalregistry
	endif
    endif
    goto end
warning = +
    Shell $(subroutineinf) SetupMessage, $(!STF_LANGUAGE), "WARNING", $(Error)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	goto ShellCodeError
    endif
    ifstr(i) $($R1) == "OK"
	goto $(to)
    else-ifstr(i) $($R1) == "CANCEL"
	goto $(from)
    else
	goto "end"
    endif
nonfatalinfo = +
    Set Severity = STATUS
    Set CommonStatus = STATUS_USERCANCEL
    goto nonfatalmsg
nonfatal = +
    Set Severity = NONFATAL
    goto nonfatalmsg
nonfatalmsg = +
    ifstr(i) $(Error) == ""
	Set Severity = NONFATAL
	Shell $(UtilityInf) RegistryErrorString "SETUP_FAIL"
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    goto ShellCodeError
	endif
	set Error = $($R0)
    endif
    Shell $(subroutineinf) SetupMessage, $(!STF_LANGUAGE), $(Severity), $(Error)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	goto ShellCodeError
    endif
    ifstr(i) $($R1) == "OK"
	goto $(from)
    else
	goto "end"
    endif
fatalregistry = +
    Shell $(UtilityInf) RegistryErrorString $(RegistryErrorIndex)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	goto ShellCodeError
    endif
    set Error = $($R0)
    goto fatal
fataldetect = +
    Shell $(UtilityInf),RegistryErrorString,CANNOT_DETECT
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	Debug-Output "ShellCode error: cannot get an error string."
	goto ShellCodeError
    endif
    set Error = $($R0)
    Goto fatal
fatal = +
    ifstr(i) $(Error) == ""
	Shell $(UtilityInf) RegistryErrorString "SETUP_FAIL"
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    goto ShellCodeError
	endif
	set Error = $($R0)
    endif
    Shell $(subroutineinf) SetupMessage, $(!STF_LANGUAGE), "FATAL", $(Error)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	goto ShellCodeError
    endif
    goto setfailed
ShellCodeError = +
    set DlgType      = "MessageBox"
    set STF_MB_TITLE = $(ShellCodeErrorTitle)
    set STF_MB_TEXT  = $(ShellCodeErrorText)
    set STF_MB_TYPE  = 1
    set STF_MB_ICON  = 3
    set STF_MB_DEF   = 1
    ui start "Error Message"
    goto setfailed
setfailed = +
    set CommonStatus = STATUS_FAILED
    ifstr(i) $(OEM_ABANDON_ON) == TRUE
	set OEM_ABANDON_ON = FALSE
	goto abandon
    endif
    goto end
end = +
    goto term
term = +
    Return $(CommonStatus)
[DebugConfiguration]
    Set InfName = "OEMNADAM.INF"
    Debug-Output $(InfName)" **CONFIGURATION STATE: "$($0)
    Debug-Output $(InfName)" IRQ_Level is "$(!p:IRQ_Level)
    Debug-Output $(InfName)" IOBaseAddrValue is "$(!p:IOBaseAddrValue)
    return
[Install-Option]
    set STF_VITAL = ""
    ifstr(i) $(AddCopy) == "YES"
	AddSectionFilesToCopyList Files-$(Option) $(SrcDir) $(!STF_WINDOWSSYSPATH)\drivers
    endif
    ifstr(i) $(DoCopy) == "YES"
       set !STF_NCPA_FLUSH_COPYLIST = TRUE
       CopyFilesInCopyList
    endif
    Exit
[Install-Update]
   set STF_VITAL        = ""
   set STF_OVERWRITE    = "VERIFYSOURCEOLDER"
   AddSectionFilesToCopyList Files-$(Option) $(SrcDir) $(!STF_WINDOWSSYSPATH)\drivers
   AddSectionFilesToCopyList Files-Dll $(SrcDir) $(!STF_WINDOWSSYSPATH)
   AddSectionFilesToCopyList Files-hlp $(SrcDir) $(!STF_WINDOWSSYSPATH)
   exit
[Install-Helpfile]
   Debug-Output "At Install-Helpfile"
   set STF_VITAL        = ""
   set STF_OVERWRITE    = "VERIFYSOURCEOLDER"
   ifstr(i) $(AddCopy) == "YES"
       AddSectionFilesToCopyList Files-hlp $(SrcDir) $(!STF_WINDOWSSYSPATH)
   endif
   ifstr(i) $(DoCopy) == "YES"
      set !STF_NCPA_FLUSH_COPYLIST = TRUE
      CopyFilesInCopyList
   endif
   exit
[Install-Dll]
   set STF_VITAL        = ""
   ifstr(i) $(AddCopy) == "YES"
       AddSectionFilesToCopyList Files-Dll $(SrcDir) $(!STF_WINDOWSSYSPATH)
   endif
   ifstr(i) $(DoCopy) == "YES"
       set !STF_NCPA_FLUSH_COPYLIST = TRUE
       CopyFilesInCopyList
   endif
   exit
[Source Media Descriptions]
    1 = "Windows NT Server CD-ROM", TAGFILE = cdrom.s
[Signature]
    FileType = MICROSOFT_FILE
[GetSignature]
    read-syms Signature
    return $(FileType)
[ProductType]
STF_PRODUCT  = LanmanNT
STF_PLATFORM = I386
[Files-Inf]
2,	oemsetup.inf,	 SIZE=1000,	RENAME=$(!UG_Filename)
[Files-AMDPCI]
1,AMDPCN.SYS , SIZE=999
[Files-Dll]
1,AMDDLG.DLL , SIZE=999
[Files-hlp]
1,PCNET.HLP , SIZE=999
[LanguagesSupported]
    ENG
[OptionsTextENG]
    AMDPCI     = "AMD PCNET Family Ethernet Adapter"
[FileConstantsENG]
ProCaption   = "Windows NT Setup"
ProCancel    = "Cancel"
ProCancelMsg = "Windows NT Networking is not correctly installed.  "+
               "Are you sure you want to cancel copying files?"
ProCancelCap = "Network Setup Message"
ProText1     = "Copying:"
ProText2     = "To:"
GenericAdapterName = "AMD PCNET ISA/VESA Ethernet Adapter"
GenericPCIAdapterName = "AMD PCNET PCI Ethernet Adapter"
GenericDriverName  = "AMD PCNET Family Ethernet Adapter Driver"
ProductSoftwareDescription = $(GenericDriverName)
ProductHardwareDescription = $(GenericAdapterName)
ProductHardwarePCNTN3Description="AMD PCnet Family Driver"
ProductSoftwareTitle =       $(GenericDriverName)
ProductHardwarePCNTN3Title = $(GenericAdapterName)
DialogDllName   = "amddlg.dll"
IRQList  = ^(IRQChoices, 1)
IRQValues = ^(IRQChoices, 2)
IOBaseAddrList = ^(IOBaseAddrChoices, 1)
IOBaseAddrValues = ^(IOBaseAddrChoices, 2)
DMAChannelList = ^(DMAChannelChoices,1)
DMAChannelValues = ^(DMAChannelChoices,2)
LEDList = ^(LEDChoices,1)
LEDValues = ^(LEDChoices,2)
FullDuplexList = ^(FullDuplexChoices,1)
FullDuplexValues = ^(FullDuplexChoices,2)
BusTimerList = ^(BusTimerChoices,1)
BusTimerValues = ^(BusTimerChoices,2)
[DialogConstantsENG]
FunctionTitle   = $(GenericAdapterName)$(GenericInfVersion)
Help        = "&Help"
Exit        = "Cancel"
OK          = "&OK"
HelpContext = ""
Continue    = "Continue"
Cancel      = "&Cancel"
[MemoryMappedChoicesENG]
Map_1 = 1, "ON"
Map_2 = 0, "OFF"
[FileDependentDlgENG]
DlgText = "Please select values for the following fields:"
Combo1Label = "I/O Port:"
Combo2Label = "IRQ Number:"
Combo3Label = "DMA Number:"
Combo4Label = "Full Duplex:"
Combo5Label = "Bus Timer:"
BigButton   = "More options >>"
CheckBox1 = "10Base-&T port"
Group1 = "&Bus to scan"
Radio1 = "PNP"
Radio2 = "VESA"
Radio3 = "ISA"
Radio4 = "ALL"
DlgType = "RadioCombination"
DlgTemplate = "PCNTN3"
Caption = $(FunctionTitle)
CBOptionsGreyed = {}
NotifyFields = {NO, NO}
HelpContext = 1
Combo1List = $(IOBaseAddrList)
Combo1Out  = $(IOBaseAddrValue)
Combo2List = $(IRQList)
Combo2Out  = $(IRQValue)
Combo3List = $(DMAChannelList)
Combo3Out  = $(DMAChannelValue)
Combo4List = $(FullDuplexList)
Combo4Out  = $(FullDuplexValue)
Combo5List = $(BusTimerList)
Combo5Out  = $(BusTimerValue)
ComboListItemsIn  = {Combo1List,Combo2List,Combo3List,Combo4List,Combo5List}
ComboListItemsOut = {Combo1Out,Combo2Out,Combo3Out,Combo4Out,Combo5Out}
EditTextIn = ""
EditTextLim = ""
[IRQChoices]
IRQ_1 = "3",3
IRQ_2 = "4",4
IRQ_3 = "5",5
IRQ_4 = "9",9
IRQ_5 = "10",10
IRQ_6 = "11",11
IRQ_7 = "12",12
IRQ_8 = "15",15
IRQ_9 = "Auto_Scan",0
[IOBaseAddrChoices]
IOBase_1  = "0x200",512
IOBase_2  = "0x220",544
IOBase_3  = "0x240",576
IOBase_4  = "0x260",608
IOBase_5  = "0x280",640
IOBase_6  = "0x2a0",672
IOBase_7  = "0x2c0",714
IOBase_8  = "0x2e0",746
IOBase_9  = "0x300",768
IOBase_10 = "0x320",800
IOBase_11 = "0x340",832
IOBase_12 = "0x360",864
IOBase_13 = "0x380",896
IOBase_14 = "0x3a0",928
IOBase_15 = "0x3c0",960
IOBase_16 = "0x3e0",992
IOBase_17 = "Auto_Scan",0
[DMAChannelChoices]
DMAChannel_1 = "3",3
DMAChannel_2 = "5",5
DMAChannel_3 = "6",6
DMAChannel_4 = "7",7
DMAChannel_5 = "Auto_Scan",0
[LEDChoices]
LED_1 = "Default",65536
LED_2 = "0x0",0
LED_3 = "0x2",2
LED_4 = "0x4",4
LED_5 = "0x8",8
LED_6 = "0x10",16
LED_7 = "0x20",32
LED_8 = "0x30",48
LED_9 = "0x34",52
LED_10 = "0x40",64
LED_11 = "0xc0",192
LED_12 = "0x4088",16520
LED_13 = "0xb0",176
LED_14 = "0x21",129
[FullDuplexChoices]
FULLDUPLEX_1 = "OFF",1
FULLDUPLEX_2 = "AUI",2
FULLDUPLEX_3 = "UTP",3
FULLDUPLEX_4 = "Default",0
[BusTimerChoices]
BUSTIMER_1 = "5",5
BUSTIMER_2 = "6",6
BUSTIMER_3 = "7",7
BUSTIMER_4 = "8",8
BUSTIMER_5 = "9",9
BUSTIMER_6 = "10",10
BUSTIMER_7 = "11",11
BUSTIMER_8 = "12",12
BUSTIMER_9 = "13",13
BUSTIMER_10 = "Default",0
[FileDependentDlgPCIENG]
FunctionTitle   = $(GenericPCIAdapterName)$(GenericInfVersion)
DlgText = "Please select values for the following fields:"
Combo1Label = "Full Duplex:"
Combo2Label = "Bus Timer:"
BigButton   = "More options >>"
CheckBox1 = "10Base-&T port"
Radio1 = "PNP"
Radio2 = "VESA"
Radio3 = "ISA"
Radio4 = "ALL"
DlgType = "RadioCombination"
DlgTemplate = "PCNTN3PCI"
Caption = $(FunctionTitle)
CBOptionsGreyed = {}
NotifyFields = {NO, NO}
HelpContext = 1
Combo1List = $(FullDuplexList)
Combo1Out  = $(FullDuplexValue)
Combo2List = $(BusTimerList)
Combo2Out  = $(BusTimerValue)
Combo3List = $(LEDList)
Combo3Out  = $(LED0Value)
Combo4List = $(LEDList)
Combo4Out  = $(LED1Value)
Combo5List = $(LEDList)
Combo5Out  = $(LED2Value)
Combo6List = $(LEDList)
Combo6Out  = $(LED3Value)
ComboListItemsIn  = {Combo1List,Combo2List}
ComboListItemsOut = {Combo1Out,Combo2Out}
EditTextIn = ""
EditTextLim = ""
[LEDChoices]
LED_1 = "Default",65536
LED_2 = "0x0",0
LED_3 = "0x2",2
LED_4 = "0x4",4
LED_5 = "0x8",8
LED_6 = "0x10",16
LED_7 = "0x20",32
LED_8 = "0x30",48
LED_9 = "0x34",52
LED_10 = "0x40",64
LED_11 = "0xc0",192
LED_12 = "0x4088",16520
LED_13 = "0xb0",176
LED_14 = "0x21",129
[FullDuplexChoices]
FULLDUPLEX_1 = "OFF",1
FULLDUPLEX_2 = "AUI",2
FULLDUPLEX_3 = "UTP",3
FULLDUPLEX_4 = "Default",0
[BusTimerChoices]
BUSTIMER_1 = "5",5
BUSTIMER_2 = "6",6
BUSTIMER_3 = "7",7
BUSTIMER_4 = "8",8
BUSTIMER_5 = "9",9
BUSTIMER_6 = "10",10
BUSTIMER_7 = "11",11
BUSTIMER_8 = "12",12
BUSTIMER_9 = "13",13
BUSTIMER_10 = "Default",0
