*PPD-Adobe: "4.0"
*% Adobe Systems PostScript(R) Printer Description File
*% Copyright 1987-1992 Adobe Systems Incorporated. 
*% All Rights Reserved. 
*% Permission is granted for redistribution of this file as
*% long as this copyright notice is intact and the contents
*% of the file is not altered in any way from its original form.
*% End of Copyright statement
*FormatVersion: "4.0"
*FileVersion: "3.0"
*PCFileName: "VT600P1.PPD"
*LanguageVersion: English

*Product: "(Varityper VT-600)"
*PSVersion: "(48.0) 5"
*ModelName: "Varityper VT-600P"
*NickName: "Varityper VT-600P"

*% General Information and Defaults ===============
*ColorDevice: False
*DefaultColorSpace: Gray
*FreeVM: "1259626"
*LanguageLevel: "1"
*Extensions: FileSystem CMYK
*VariablePaperSize: False
*FileSystem: True
*?FileSystem: "save
  statusdict /diskstatus get exec
  exch pop 0 eq {(False)}{(True)}ifelse = flush restore
"
*End

*Throughput: "10"
*Password: "0"
*ExitServer: "
  count 0 eq {  % is the password on the stack?
    true 
  }{
    dup % potential password
    statusdict /checkpassword get exec not
  } ifelse 
  {  %  if no password or not valid 
    (WARNING : Cannot perform the exitserver command.) = 
    (Password supplied is not valid.) = 
    (Please contact the author of this software.) = flush
    quit
  } if 
  serverdict /exitserver get exec
"
*End

*Reset: "
  count 0 eq {  % is the password on the stack?
    true 
  }{
    dup % potential password
    statusdict /checkpassword get exec not
  } ifelse 
  {  %  if no password or not valid 
    (WARNING : Cannot reset printer.) = 
    (Password supplied is not valid.) = 
    (Please contact the author of this software.) = flush
    quit
  } if 
  serverdict /exitserver get exec
  systemdict /quit get exec
  (WARNING : Printer Reset Failed.) = flush
"
*End

*DefaultResolution: 600dpi
*?Resolution: "
save
  initgraphics
  0 0 moveto currentpoint matrix defaultmatrix transform
  0 72 lineto currentpoint matrix defaultmatrix transform
  3 -1 roll sub dup mul
  3 1 roll exch sub dup mul
  add sqrt round cvi
  (          ) cvs print  (dpi) = flush
restore
"
*End

*% Halftone Information ===============
*ScreenFreq: "75.0"
*ScreenAngle: "45.0"
*DefaultScreenProc: Dot
*ScreenProc Dot: "
{abs exch abs 2 copy add 1 gt {1 sub dup mul exch 1 sub dup mul add 1 
sub }{dup mul exch dup mul add 1 exch sub }ifelse }
"
*End
*ScreenProc Line: "{ pop }"
*ScreenProc Ellipse: "{ dup 5 mul 8 div mul exch dup mul exch add sqrt 1 exch sub }"

*DefaultTransfer: Null
*Transfer Null: "{ }"
*Transfer Null.Inverse: "{ 1 exch sub }"

*% Paper Handling ===================

*% Use these entries to set paper size most of the time, unless there is
*% specific reason to use PageRegion.
*OpenUI *PageSize: PickOne
*OrderDependency: 30 AnySetup *PageSize
*DefaultPageSize: Letter
*PageSize Letter: "letter"
*PageSize Legal: "legal"
*PageSize A4: "a4"
*PageSize B4: "b4"
*PageSize ISOB4: "729.72 1031.46 1 statusdict /setpage get exec"
*CloseUI: *PageSize

*% These entries will set up the frame buffer. Usually used with manual feed.
*OpenUI *PageRegion: PickOne
*OrderDependency: 40 AnySetup *PageRegion
*DefaultPageRegion: Letter
*PageRegion Letter: "letter"
*PageRegion Legal: "legal"
*PageRegion A4: "a4"
*PageRegion B4: "b4"
*PageRegion ISOB4: "729.72 1031.46 1 statusdict /setpage get exec"
*CloseUI: *PageRegion

*% The following entries provide information about specific paper keywords.
*DefaultImageableArea: Letter
*ImageableArea Letter: "18 18 593 772 "
*ImageableArea Legal: "18 19 593 990 "
*ImageableArea A4: "17 19 577 822 "
*ImageableArea B4: "48 48 680 983 "
*ImageableArea ISOB4: "48 48 680 983 "
*?ImageableArea: "
  save
   /cvp { (                ) cvs print ( ) print } bind def
   /upperright {10000 mul floor 10000 div} bind def
   /lowerleft {10000 mul ceiling 10000 div} bind def
   newpath clippath pathbbox
   4 -2 roll exch 2 {lowerleft cvp} repeat
   exch 2 {upperright cvp} repeat flush
 restore"
*End

*% These provide the physical dimensions of the paper (by keyword)
*DefaultPaperDimension: Letter
*PaperDimension Letter: "612 792"
*PaperDimension Legal: "612 1008"
*PaperDimension A4: "595 842"
*PaperDimension B4: "729 1032"
*PaperDimension ISOB4: "729.72 1031.46"

*DefaultOutputBin: Upper
*OpenUI *InputSlot: PickOne
*OrderDependency: 20 AnySetup *InputSlot
*DefaultInputSlot: Cassette
*InputSlot Cassette: ""
*CloseUI: *InputSlot

*DefaultOutputOrder: Normal

*% Font Information =====================

*DefaultFont: Courier
*Font Courier: Standard "(001.004)" Standard ROM
*Font Courier-Bold: Standard "(001.004)" Standard ROM
*Font Courier-BoldOblique: Standard "(001.004)" Standard ROM
*Font Courier-Oblique: Standard "(001.004)" Standard ROM
*Font Symbol: Special "(001.001)" Special ROM
*Font Varitimes#Bold: Standard "(001.000)" Standard ROM
*Font Varitimes#BoldItalic: Standard "(001.000)" Standard ROM
*Font Varitimes#Italic: Standard "(001.000)" Standard ROM
*Font Varitimes#Roman: Standard "(001.000)" Standard ROM
*?FontQuery: "
save
{
  count 1 gt {
  exch dup 128 string cvs (/) print print (:) print
  dup FontDirectory exch known {pop (Yes)}
  {
    (fonts/                              )
      dup 3 -1 roll 128 string cvs dup length /len exch def
      6 exch putinterval
      0 len 6 add getinterval mark exch
      { } 128 string filenameforall counttomark 0 gt {
      cleartomark (Yes)}{cleartomark (No)}ifelse
      }ifelse =
      }{ exit } ifelse
  } bind loop
  (*) = flush
restore
"
*End

*?FontList: "
save
  FontDirectory { pop == } bind forall flush
  /filenameforall where {
    pop (fonts/*) {
    dup length 6 sub 6 exch getinterval cvn ==
    } bind
    128 string filenameforall flush
  } if
  (*) = flush
restore
"
*End

*% Printer Messages (verbatim from printer):
*Message: "%%[ exitserver: permanent state may be changed ]%%"
*Message: "%%[ Flushing: rest of job (to end-of-file) will be ignored ]%%"
*Message: "\FontName\ not found, using Courier"

*% Status (format: %%[ status: <one of these> ]%% )
*Status: "idle"
*Status: "busy"
*Status: "waiting"
*Status: "printing"
*Status: "warming up"
*Status: "initializing"
*Status: "PrinterError: PE not responding"
*Status: "PrinterError: paper jam"
*Status: "PrinterError: PE sync error"
*Status: "PrinterError: PE scan motor error"
*Status: "PrinterError: PE laser power error"
*Status: "PrinterError: PE drum motor error"
*Status: "PrinterError: PE fuser error"
*Status: "PrinterError: PE laser adjustment error"
*Status: "PrinterError: PE needs attention"
*Status: "PrinterError: out of paper"
*Status: "PrinterError: no paper tray"
*Status: "PrinterError: heater not ready"
*Status: "PrinterError: door open"

*% Input Sources (format: %%[ status: <stat>; source: <one of these> ]%% )
*Source: "serial9"
*Source: "serial25"
*Source: "AppleTalk"
*Source: "Centronics"

*% Printer Error (format: %%[ PrinterError: <one of these> ]%%)
*PrinterError: "PE not responding"
*PrinterError: "paper jam"
*PrinterError: "PE sync error"
*PrinterError: "PE scan motor error"
*PrinterError: "PE laser power error"
*PrinterError: "PE drum motor error"
*PrinterError: "PE fuser error"
*PrinterError: "PE laser adjustment error"
*PrinterError: "PE needs attention"
*PrinterError: "out of paper"
*PrinterError: "no paper tray"
*PrinterError: "heater not ready"
*PrinterError: "door open"

*%DeviceAdjustMatrix: "[1 0 0 1 0 0]"

*% Color Separation Information =====================
*% Accuratescreen angles/freqs added to bottom of file

*DefaultColorSep: ProcessCyan.85lpi.600dpi/85 lpi / 600 dpi

*InkName: ProcessBlack/Process Black
*InkName: CustomColor/Custom Color
*InkName: ProcessCyan/Process Cyan
*InkName: ProcessMagenta/Process Magenta
*InkName: ProcessYellow/Process Yellow

*% For 85 lpi / 600 dpi (5,5,2,6,6,2,20/3,0) ===============================

*ColorSepScreenAngle ProcessBlack.85lpi.600dpi/85 lpi / 600 dpi: "45.0"
*ColorSepScreenAngle CustomColor.85lpi.600dpi/85 lpi / 600 dpi: "45.0"
*ColorSepScreenAngle ProcessCyan.85lpi.600dpi/85 lpi / 600 dpi: "71.5651"
*ColorSepScreenAngle ProcessMagenta.85lpi.600dpi/85 lpi / 600 dpi: "18.4349"
*ColorSepScreenAngle ProcessYellow.85lpi.600dpi/85 lpi / 600 dpi: "0.0"

*ColorSepScreenFreq ProcessBlack.85lpi.600dpi/85 lpi / 600 dpi: "84.8528"
*ColorSepScreenFreq CustomColor.85lpi.600dpi/85 lpi / 600 dpi: "84.8528"
*ColorSepScreenFreq ProcessCyan.85lpi.600dpi/85 lpi / 600 dpi: "94.8683"
*ColorSepScreenFreq ProcessMagenta.85lpi.600dpi/85 lpi / 600 dpi: "94.8683"
*ColorSepScreenFreq ProcessYellow.85lpi.600dpi/85 lpi / 600 dpi: "30.0"

*ColorSepScreenProc ProcessYellow.85lpi.600dpi/85 lpi / 600 dpi: "
{1 add 2 div 3 mul dup floor sub 2 mul 1 sub exch 
1 add 2 div 3 mul dup floor sub 2 mul 1 sub exch 
abs exch abs 2 copy add 1 gt {1 sub dup mul exch 1 sub dup mul add 1 
sub }{dup mul exch dup mul add 1 exch sub }ifelse }"
*End

*% For 71 lpi / 600 dpi =====================================================

*ColorSepScreenAngle ProcessBlack.71lpi.600dpi/71 lpi / 600 dpi: "45.0"
*ColorSepScreenAngle CustomColor.71lpi.600dpi/71 lpi / 600 dpi: "45.0"
*ColorSepScreenAngle ProcessCyan.71lpi.600dpi/71 lpi / 600 dpi: "71.5651"
*ColorSepScreenAngle ProcessMagenta.71lpi.600dpi/71 lpi / 600 dpi: "18.4349"
*ColorSepScreenAngle ProcessYellow.71lpi.600dpi/71 lpi / 600 dpi: "0.0"

*ColorSepScreenFreq ProcessBlack.71lpi.600dpi/71 lpi / 600 dpi: "70.7107"
*ColorSepScreenFreq CustomColor.71lpi.600dpi/71 lpi / 600 dpi: "70.7107"
*ColorSepScreenFreq ProcessCyan.71lpi.600dpi/71 lpi / 600 dpi: "63.2456"
*ColorSepScreenFreq ProcessMagenta.71lpi.600dpi/71 lpi / 600 dpi: "63.2456"
*ColorSepScreenFreq ProcessYellow.71lpi.600dpi/71 lpi / 600 dpi: "66.6667"

*% For "Varityper VT-600P" version 48.0
*% Produced by "BuildPPD.ps" version 3.0 edit 58
*% Converted to meet 4.0 specification
*% Last Edit Date: May 27 1992
*% The byte count of this file should be exactly 009985 or 010294
*% depending on the filesystem it resides in.
*% end of PPD file for Varityper VT-600P
