WINDOWS 95 PEN SERVICES
=======================

Release notes for Windows 95 Pen Services

1) Installation of the Pen Services has been removed from the
base Windows 95 setup procedure.  The setup procedure below
assumes you have already installed Windows 95.  If your pen
hardware does not appear in the list below, please contact the
manufacturer for a Windows 95 pen driver before proceeding.
The pen driver installed by the procedure below only supports
the pen hardware listed below.

To install this beta of Windows 95 Pen Services:

a. From the Start menu select Settings, then Control Panel,
then Add/Remove Programs.
b. From the Add/Remove Programs Properties sheet, select the
Windows Setup tab, and click the Have Disk button.  Click the
Browse button and use the file browser to locate the PENWIN.INF
file.  It will be found in the \PEN direcotry of your installation
CD.  Select PENWIN.INF and click OK.  Then in the Install From
Disk dialog, click OK.
c. In the Have Disk dialog optional components list box, check
the box next to "Pen Services for Windows 95" and then click 
Install.
d. When the Add/Remove Programs Properties sheet is
redisplayed, click OK. When you are prompted to restart your
computer, click Yes.
e. After Windows 95 restarts, the Pen Driver Configuration
dialog will appear. The four digitizers supported by the sample
pen driver you have just installed are displayed:
     - Wacom Technologies Digitizer Model SD-510C
     - Wacom Technologies Digitizer Model HD-648A
     - Wacom Technologies Digitizer Model UD-0608-R
     - Compaq Concerto
Select the digitizer you are using from the list and, if
necessary, select a COM port and whether or not your stylus is
pressure-sensitive. Then click OK.
f. When you are prompted to exit and restart your computer,
use the Start menu to restart Windows 95 instead of turning
off the machine or using Ctl-Alt-Del.  This will allow Windows
95 to finish loading properly.  Do not try to use the pen in
this intermediate stage since the pen driver will not yet be
configured.

2) Some video driver and video resolution combinations have
not been tested for compatibility with the Pen Services inking
scheme.  Please report any inking problems found.
