[Version]
LayoutFile=Layout.inf
Signature="$CHICAGO$"
Class=PCMCIA
Provider=%MS%

;
;   Information for installing the PCMCIA class
;
[ClassInstall]
AddReg=ClassAddReg

[ClassAddReg]
HKR,,,,%ClassName%
HKR,,Installer,,PCCard.Cpl
HKR,,Icon,,0


;
;   List of manufacturers and devices
;
[Manufacturer]
%GenDrvs%=Generic
%IntelMfg%=Intel
%DatabookMfg%=TMI160

[Generic]
%GenPCIC%=PCIC,*PNP0E00

[Intel]
%IntelProto%=PCIC

[TMI160]
%*DBK0402.DeviceDesc%=DB86082,*DBK0402

[DB86082]
CopyFiles=CSCopyfiles, @dbkvssd.386
AddReg=CSReg, TMI160Reg

[TMI160Reg]
HKR,,Driver,,"DbkVssD.386"

;
;   Intel compatible PCIC controller
;
[PCIC]
CopyFiles=CSCopyfiles, @socketsv.386
AddReg=CSReg, PCICReg
LogConfig=*PNP0E00.LogConfig

[PCICReg]
HKR,,Driver,,"SocketSv.386"
HKR,,Properties,,"PCCard.Cpl, PCICProperties"

[*PNP0E00.LogConfig]
ConfigPriority=HARDWIRED
IOConfig=3e0-3e1(3ff::),3e2-3e3(3ff::)
;;;;IRQConfig=3,4,5,7,9,10,11,12,14,15
IRQConfig=5,7,9,10,11,12,14,15


;
;   Card services information
;
[CSCopyfiles]
PCCard.386

[CSReg]
HKR,,DevLoader,,"PCCARD.386"

;
;   Information about where the files are
;
[DestinationDirs]
DefaultDestDir=11               ; LDID_SYS

[Strings]
ClassName="PCMCIA Socket"
MS="Microsoft"
GenDrvs="(Generic Drivers)"
GenPCIC="Intel PCIC or compatible controller"
IntelMfg="Intel"
IntelProto="Intel development prototype board"
DatabookMfg="Databook"
;
;   Strings with "*PNPxxxx" are descriptions used by hardware detection
;   for PCMCIA controllers
;
*PNP0E00.DeviceDesc="Intel PCIC Compatible PCMCIA Controller"
*DBK0402.DeviceDesc="Databook's Plug and Play PCMCIA Controller"
