; SCSI.INF  -- This file contains descriptions of all the SCSI
;              Host adapters supported in Chicago
;
;*** Created 9/30/93  (Creation Date)
;  FD7000EX      Future Domain EISA 7000EX              Added
;  Future Domain 16 bit Host Adapters                   Added
;  Future Domain 8 bit Host Adapters                    Added
;*** Updated 9/30/93
; UltraStor 14F ISA SCSI Host Adapter                   Added
; UltraStor 34F/34FA VESA SCSI Host Adapter             Added
; UltraStor 14FB ISA SCSI Host Adapter                  Added
; UltraStor 34FB VESA SCSI Host Adapter                 Added
; UltraStor 24F/24FA EISA SCSI Host Adapter             Added
; UltraStor 124F EISA SCSI Disk Array Controller        Added
;*** Updated 10/01/93
; Acculogic (NCR) EISA SCSI Controller                  Added
;*** Updated 10/4/93
; DPT EISA and ISA boards                               Added
; Adaptec boards                                        Added

[Version]
signature="$CHICAGO$"
Class=SCSIAdapter
Provider=%Msft%
LayoutFile=LAYOUT.INF

; Class Install
[ClassInstall]
Addreg=SCSIReg

[SCSIReg]
HKR,,,,%SCSIClassName%


; Table of Contents
[Manufacturer]
%FDC%=FUTURED
%ULTRASTOR%=ULTRASTOR
%ACCULOGIC%=ACCULOGIC
%DPT%=DPT
%ADP%=ADAPTEC
%BLCName%=BLCDevices
%IOMega%=IOMega


[DPT]
%DPTEISA%=DPT_eisa,*DPTA401,*DPTA410,*DPTA411,*DPTA501,*DPTA502
%DPTISA%=DPT_isa,*DPTA701

[ACCULOGIC]
%NCRSDMS%=Accu_SCSI,*ACU0101

[FUTURED]
%FDCEISA%=FDEISA,*WDC2001
%FD16ISA%=FD16Bit,*FDC0000
%FD16EISA%=FD16Bit,*FDC0000
%FD16MCA%=FD16Bit,*FDC0000
%FD8SHORT%=FD8Bit,*FDC0950
%FD8LONG%=FD8Bit,*FDC0950

[ULTRASTOR]
%ULTRA14F%=Ultra_140,*USC0140,*USC0141,*USC0142,*USC0143
%ULTRA24F%=Ultra_240,*USC0240
%ULTRA124F%=Ultra_1240,*USC1240

[ADAPTEC]
%*ADP7770.DeviceDesc%=  AIC777X,*ADP7770,*ADP7771
%*ADP2840.DeviceDesc%= AHA284X,*ADP2840
%*ADP1740.DeviceDesc%= AHA174X,*ADP1740
%*ADP1540.DeviceDesc%= AHA154X,*ADP1540
%*ADP1520.DeviceDesc%= AIC6X60,*ADP1520
%*ADP1522.DeviceDesc%= AIC6X60,*ADP1522
%*ADP6360.DeviceDesc%= AIC6X60,*ADP6360

[BLCdevices]
%*BUS0042.DeviceDesc%=AllBLC,*BUS0042

[IOMega]
%*isaB701.DeviceDesc%=*isaB701.drv,*isaB701     ;IOMEGA Card

[*isaB701.drv]          ;Iomega installation
Copyfiles=@PC2X.mpd
AddReg=IOS,PC2XReg

[*isaB701.det]          ; Iomega installation
addreg=ForceMPCopy

[pc2xReg]
HKR,,PortDriver,,pc2x.mpd

[*isaB701.LogConfig]
ConfigPriority=HARDWIRED
IOConfig=4@340-370%fff0(3ff::)
IRQConfig=5,7
DMAConfig=1,3

;******************************** BusLogic Driver Installation Sections
;
[AllBLC]
CopyFiles=@buslogic.mpd
AddReg=IOS,BLCRegLines

[BLCRegLines]
HKR,,PortDriver,,buslogic.mpd


;********************************Adaptec Driver Installation Sections
;

[AIC777X]
CopyFiles=@ARROW.MPD
AddReg=IOS,AIC777.Reg
DelFiles=ASPIDEV

[AIC777.REG]
HKR,,PortDriver,,ARROW.MPD

[AHA284X]
CopyFiles=@ARROW.MPD
AddReg=IOS,AHA284X.Reg
DelFiles=ASPIDEV

[AHA284X.REG]
HKR,,PortDriver,,ARROW.MPD

[AHA174X]
CopyFiles=@AHA174x.MPD
AddReg=IOS,AHA174x.Reg
DelFiles=ASPIDEV

[AHA174x.REG]
HKR,,PortDriver,,AHA174X.MPD

[AHA154X]
CopyFiles=@AHA154x.MPD
AddReg=IOS,AHA154x.Reg
DelFiles=ASPIDEV

[AHA154x.REG]
HKR,,PortDriver,,AHA154X.MPD

[AIC6X60]
CopyFiles=@SPARROW.MPD
AddReg=IOS,AHA152x.Reg
DelFiles=ASPIDEV

[AHA152x.Reg]
HKR,,PortDriver,,SPARROW.MPD

[ASPIDEV]
VASPID.386
;********************************DPT Driver Installation Sections
;
[DPT_isa]
CopyFiles=@DPTSCSI.MPD
AddReg=IOS,DPT_reg

[DPT_eisa]
CopyFiles=@DPTSCSI.MPD
AddReg=IOS,DPT_reg

[DPT_reg]
HKR,,PortDriver,,DPTSCSI.MPD

;********************************Future Domain Driver Installation Sections
;
; EISA SCSI Host Adapter FD7000EX
[FDEISA]
CopyFiles=@WD7000EX.MPD
AddReg=IOS,ADDREG_32_BIT

[ADDREG_32_BIT]
HKR,,PortDriver,,WD7000EX.MPD

; FDC 16 Bit SCSI Host Adapters
;       ISA -- TMC1660/1670/1680 
;       MCA -- MCS-600/700
;       EISA -- TMC-1790/1795
[FD16Bit]
CopyFiles=@FD16_700.MPD
AddReg=IOS,ADDREG_16_BIT

[ADDREG_16_BIT]
HKR,,PortDriver,,FD16_700.MPD

; FDC 8 Bit Cards including:
;       TMC 860,860M,885,885M,850,850M,850MEX,850MER
[FD8Bit]
CopyFiles=@FD8XX.MPD
AddReg=IOS,ADDREG_8_BIT

[ADDREG_8_BIT]
HKR,,PortDriver,,FD8XX.MPD

;********************************ULTRA 14xx,24xx,34xx,124xx Drivers
[Ultra_140]
CopyFiles=@ULTRA14F.MPD
AddReg=IOS,ULTRA14F_REG

[Ultra_240]
CopyFiles=@ULTRA24F.MPD
AddReg=IOS,ULTRA24F_REG

[Ultra_1240]
CopyFiles=@ULTRA124.MPD
AddReg=IOS,ULTRA124_REG

[ULTRA14F_REG]
HKR,,PortDriver,,ULTRA14F.MPD

[ULTRA24F_REG]
HKR,,PortDriver,,ULTRA24F.MPD

[ULTRA124_REG]
HKR,,PortDriver,,ULTRA124.MPD

;********************NCR Chipset/Acculogic EISApport SCSI board Drivers
[Accu_SCSI]
CopyFiles=@NCRSDMS.MPD
AddReg=IOS,ACCULOG_REG

[ACCULOG_REG]
HKR,,PortDriver,,NCRSDMS.MPD


; Hardware Sections

;********************************BusLogic Hardware Sections
;
[*BUS0042.Det]
AddReg=ForceMPCopy

[*BUS0042.LogConfig]
ConfigPriority=HARDWIRED
IOConfig=130-133(3FF::),230-233(3FF::),330-333(3FF::),134-137(3FF::),234-237(3FF::),334-337(3FF::)
IRQConfig=9,10,11,12,14,15
DMAConfig=0,5,6,7

;**********************************Future Domain Hardware Sections
; 
[*WDC2001.Det]
AddReg=ForceMPCopy

[*WDC2001.LogConfig]
ConfigPriority=REBOOT
MemConfig=4000@C0000-DC000%FFFFF000
IRQConfig=10,12,14,15

[*FDC0000.Det]
AddReg=ForceMPCopy

[*FDC0000.LogConfig]
ConfigPriority=HARDRECONFIG
MemConfig=2000@C8000-DE000%FFFFE000
IRQConfig=3,5,10,11,12,14,15

[*FDC0950.Det]
AddReg=ForceMPCopy

[*FDC0950.LogConfig]
ConfigPriority=HARDRECONFIG
MemConfig=C8000-C9FFF,CA000-CBFFF,CE000-CFFFF,DE000-DFFFF
IRQConfig=3,5,10,11,12,14,15

;********************************ULTRA 14xx,24xx,34xx,124xx hardware sections
[*USC0140.Det]
AddReg=ForceMPCopy

[*USC0140.LogConfig]
ConfigPriority=HARDRECONFIG
MemConfig=4000@c4000-dc000%FFFFC000
IOConfig=130-13F(3FF::),230-23F(3FF::),330-33F(3FF::),210-21F(3FF::),310-31F(3FF::),140-14F(3FF::),240-24F(3FF::),340-34F(3FF::)
IOConfig=1f0-1f7(3FF::),170-177(3FF::)
IOConfig=3f6-3f7(3FF::),376-377(3FF::)
IRQConfig=10,11,14,15
DMAConfig=5,6,7

[*USC0141.Det]
Addreg=ForceMPCopy

[*USC0141.LogConfig]
ConfigPriority=HARDRECONFIG
MemConfig=4000@c4000-dc000%FFFFC000
IOConfig=130-13F(3FF::),230-23F(3FF::),330-33F(3FF::),210-21F(3FF::),310-31F(3FF::),140-14F(3FF::),240-24F(3FF::),340-34F(3FF::)
IOConfig=1f0-1f7(3FF::),170-177(3FF::)
IOConfig=3f6-3f7(3FF::),376-377(3FF::)
IRQConfig=10,11,14,15

[*USC0142.Det]
AddReg=ForceMPCopy

[*USC0142.LogConfig]
ConfigPriority=NORMAL
MemConfig=4000@c4000-dc000%FFFFC000
IOConfig=130-13F(3FF::),230-23F(3FF::),330-33F(3FF::),210-21F(3FF::),310-31F(3FF::),140-14F(3FF::),240-24F(3FF::),340-34F(3FF::)
IOConfig=1f0-1f7(3FF::),170-177(3FF::)
IOConfig=3f6-3f7(3FF::),376-377(3FF::)
IRQConfig=10,11,14,15
DMAConfig=0,5,6,7

[*USC0143.Det]
AddReg=ForceMPCopy

[*USC0143.LogConfig]
ConfigPriority=NORMAL
MemConfig=4000@c4000-dc000%FFFFC000
IOConfig=130-13F(3FF::),230-23F(3FF::),330-33F(3FF::),210-21F(3FF::),310-31F(3FF::),140-14F(3FF::),240-24F(3FF::),340-34F(3FF::)
IOConfig=1f0-1f7(3FF::),170-177(3FF::)
IOConfig=3f6-3f7(3FF::),376-377(3FF::)
IRQConfig=10,11,14,15

[*USC0240.Det]
AddReg=ForceMPCopy

[*USC0240.LogConfig]
ConfigPriority=NORMAL
MemConfig=4000@c4000-dc000%FFFFC000
IOConfig=1f0-1f7(3FF::),170-177(3FF::)
IOConfig=3f6-3f7(3FF::),376-377(3FF::)
IRQConfig=10,11,14,15

[*USC1240.Det]
AddReg=ForceMPCopy

[*USC1240.LogConfig]
ConfigPriority=NORMAL
MemConfig=4000@c4000-dc000%FFFFC000
IOConfig=1f0-1f7(3FF::),170-177(3FF::)
IOConfig=3f6-3f7(3FF::),376-377(3FF::)
IRQConfig=10,11,14,15

;********************************Acculogic(NCR) EISApport SCSI adapter
[*ACU0101.Det]
AddReg=ForceMPCopy

[*ACU0101.LogConfig]
ConfigPriority=NORMAL
MemConfig=8000@C8000-D8000%FFFF8000
IRQConfig=10,11,12,14,15

;********************************DPT SCSI adapters
[*DPTA701.Det]
AddReg=ForceMPCopy

[*DPTA701.LogConfig]
ConfigPriority=HARDWIRED
IOConfig=1f0-1f8(3FF::),170-178(3FF::),230-238(3FF::),330-338(3FF::)
IRQConfig=12,14,15
DMAConfig=0,5,6,7

[*DPTA401.Det]
AddReg=ForceMPCopy

[*DPTA401.LogConfig]
ConfigPriority=NORMAL
IRQConfig=11,14,15

[*DPTA410.Det]
AddReg=ForceMPCopy

[*DPTA410.LogConfig]
ConfigPriority=NORMAL
IRQConfig=11,14,15

[*DPTA411.Det]
AddReg=ForceMPCopy

[*DPTA411.LogConfig]
ConfigPriority=NORMAL
IRQConfig=11,14,15

[*DPTA501.Det]
AddReg=ForceMPCopy

[*DPTA501.LogConfig]
ConfigPriority=NORMAL
IRQConfig=11,14,15

[*DPTA502.Det]
AddReg=ForceMPCopy

[*DPTA502.LogConfig]
ConfigPriority=NORMAL
IRQConfig=11,14,15

;********************************Adaptec SCSI adapters
[*ADP7770.Det]
AddReg=ForceMPCopy

[*ADP7770.LogConfig]
ConfigPriority = REBOOT
IRQConfig      = 9,10,11,12

[*ADP7771.Det]
AddReg=ForceMPCopy

[*ADP7771.LogConfig]
ConfigPriority = REBOOT
IRQConfig      = 9,10,11,12

[*ADP2840.Det]
AddReg=ForceMPCopy

[*ADP2840.LogConfig]
ConfigPriority = REBOOT
IOConfig       = 256@1C00-EC00%FC00(FFFF::)
; VL Bus IO address space, 14 base ports at 256 ports each
; 1C00-1CFF, 2C00-2CFF,..,EC00-ECFF
IRQConfig      = 9,10,11,12

[*ADP1740.Det]
AddReg=ForceMPCopy

[*ADP1740.LogConfig]
ConfigPriority = HARDRECONFIG
IRQConfig      = S:9,10,11,12,14,15

[*ADP1540.Det]
AddReg=ForceMPCopy

[*ADP1540.LogConfig]
ConfigPriority = HARDRECONFIG
IOConfig       = 130-133(3FF::),230-233(3FF::),330-333(3FF::),134-137(3FF::),234-237(3FF::),334-337(3FF::)
IRQConfig      = 9,10,11,12,14,15
DMAConfig      = W:5,6,7

[*ADP1520.Det]
AddReg=ForceMPCopy

[*ADP1520.LogConfig]
ConfigPriority = HARDRECONFIG
IOConfig           = 140-15F,340-35F
IRQConfig      = 9,10,11,12

[*ADP6360.Det]
AddReg=ForceMPCopy

[*ADP6360.LogConfig]
ConfigPriority=HARDRECONFIG
IOConfig=140-15F,340-35F
IRQConfig=9,10,11,12

;********************************IOS common section
[IOS]
HKR,,DevLoader,,IOS.386

[ForceMPCopy]
HKR,,NoSetupUI,,1

[DestinationDirs]
ASPIDEV = 11                    ; delete from SYSTEM dir if exists
DefaultDestDir = 12             ; IOSubsys directory

[Strings]
FDC="Future Domain Corporation"
FDCEISA="Future Domain TMC-7000EX SCSI Host Adapter"
Msft="Microsoft"
FD16ISA="Future Domain TMC-1650/1660/1670/1680 SCSI Host Adapter"
FD16EISA="Future Domain TMC-1790/1795 SCSI Host Adapter"
FD16MCA="Future Domain MCS-600/700 SCSI Host Adapter"
FD8SHORT="Future Domain TMC-850/M/MER/MEX SCSI Host Adapter"
FD8LONG="Future Domain TMC-860/860M/885/885M SCSI Host Adapter"
SCSIClassName="SCSI Controllers"
ULTRASTOR="UltraStor Corporation"
ULTRA14F="UltraStor 14F/14FB/34F/34FA/34FB Driver"
ULTRA24F="UltraStor 24F/24FA Driver"
ULTRA124F="UltraStor 124F Driver"
*USC0140.DeviceDesc="UltraStor 14F ISA SCSI Host Adapter"
*USC0141.DeviceDesc="UltraStor 34F/34FA VESA SCSI Host Adapter"
*USC0142.DeviceDesc="UltraStor 14FB ISA SCSI Host Adapter"
*USC0143.DeviceDesc="UltraStor 34FB VESA SCSI Host Adapter"
*USC0240.DeviceDesc="UltraStor 24F/24FA EISA SCSI Host Adapter"
*USC1240.DeviceDesc="UltraStor 124F EISA SCSI Disk Array Controller"
*WDC2001.DeviceDesc="Future Domain 7000EX EISA SCSI Host Adapter"
*FDC0000.DeviceDesc="Future Domain TMC-18XX SIC-based SCSI Host Adapter"
*FDC0950.DeviceDesc="Future Domain TMC-950 SIC-based SCSI Host Adapter"
ACCULOGIC="NCR/Acculogic"
NCRSDMS="NCR SDMS (TM) Miniport Driver"
*ACU0101.DeviceDesc="Acculogic EISApport SCSI Host Adapter"
DPT="DPT Corporation"
DPTISA="DPT 20x1 ISA SCSI Host Adapters"
DPTEISA="DPT 2xx2 EISA SCSI Host Adapters"
*DPTA401.DeviceDesc="DPT PM2012B EISA SCSI Host Adapters"
*DPTA410.DeviceDesc="DPT PM2x22A EISA SCSI Host Adapters"
*DPTA411.DeviceDesc="DPT Spectre chipset SCSI Adapters"
*DPTA501.DeviceDesc="DPT PM2012B1/9x EISA SCSI Host Adapters"
*DPTA502.DeviceDesc="DPT PM2012B2/9x EISA SCSI Host Adapters"
*DPTA701.DeviceDesc="DPT PM2011B1/9x ISA SCSI Host Adapters"
ADP="Adaptec"
*ADP7770.DeviceDesc="Adaptec AHA-274X/AIC-777X EISA SCSI Controller"
*ADP7771.DeviceDesc="Adaptec AHA-274X/AIC-777X EISA SCSI Controller"
*ADP2840.DeviceDesc="Adaptec AHA-284X VESA SCSI Host Adapter"
*ADP1740.DeviceDesc="Adaptec AHA-174X EISA Host Adapter"
*ADP1540.DeviceDesc="Adaptec AHA-154X/AHA-164X SCSI Host Adapter"
*ADP1520.DeviceDesc="Adaptec AHA-152X SCSI Host Adapter"
*ADP1522.DeviceDesc="Adaptec Plug and Play SCSI Host Adapter"
*ADP6360.DeviceDesc="Adaptec AIC-6X60 ISA Single-Chip SCSI Controller"
BLCName="BusLogic"
*BUS0042.DeviceDesc="All Buslogic SCSI Host Adapters"
IOMega="IOMega"
*isaB701.DeviceDesc="Iomega PC2x 8-bit SCSI Host Adapters"
