     
                        Installing Standard IrDA
     
Standard IrDA communicates at speeds up to 115200 bps.  It requires IRQ 3 
or IRQ 4 but no DMA channel.

System Installation Requirements:

HP OmniBook with Windows 95 version 4.00.950 C (or B) installed.  
The Windows 95 version can be verified by looking at the system properties 
(Start/Settings/Control Panel/System/).

Infrared Support for Windows 95 Version 2.0 drivers.  These drivers are
located on the hard disk in C:\OMNIBOOK\DRIVERS\WIN95\IRDA.  These drivers
are also located on the HP OmniBook Recovery CD in the 
\OMNIBOOK\DRIVERS\WIN95\IRDA directory.

To install IrDA support, you need to complete the following three steps:
	* Remove existing Fast Infrared support for Windows 95.
	* Setup IR Port.
	* Install IR Support for Windows 95

To remove existing IrDA support:
--------------------------------     
1.  Remove the IR Monitor
        - In the Control Panel, run Add/Remove Programs.
        - If present, highlight "Fast Infrared Support for Windows 95". 
        - Click the "Add/Remove" button to remove it.  
        - Restart the computer when prompted to do so.
       
To Setup IR port:
------------------
1.  Start Setup Utility
        - Restart the computer.
        - Press F2 during the reboot to enter Setup Utility. 
2.  In BIOS SETUP, Enable IR Port
	- Select "Advance" submenu.
        - Under "I/O Device Configuration" find the "Serial Port B:" 
        - Set the Serial Port B to "Auto".
     	- Set Mode to "IrDA".
3.  Exit SETUP, saving the changes.  ("Exit", "Save Changes and Exit", Yes)

To install IR Support for Windows 95:
-------------------------------------              
1.  Check the serial driver
        - In the Control Panel, run "System". 
        - Click the "Device Manager" tab.
        - Double-click "Ports (COM & LPT)".
        - Verify that the "Fast Infrared Commucation Port" is present.
     
5.  Install the IR Monitor
-----------------------------------------
        - In the Control Panel, run Add/Remove Programs.
        - Click the "Install" button on the "Install/Uninstall" tab. 
        - Click "Next".
        - Type "c:\omnibook\drivers\win95\irda\setup".  (If you are installing
	  from the recovery CD, use the drive letter for the CD drive.)
        - Click "Next" to run the "Add Infrared Device Wizard".
        - Click "Next" to choose "Built-in Infrared port on laptop...". 
        - Select "Fast Infrared Communication Port" and click "Next".
        - Click "Next" to use the default ports (COM4 and LPT3).
        - Click "Finish" to exit the "Add Infrared Device Wizard".
     	- Restart Windows 
	- In the Control Panel, double click on the infrared icon to enable IR communications.
